,Model##OTHER##,Shielding Type##OTHER##,Fixture Height##OTHER##,Lumen Output Comment##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Color Temperature Note##OTHER##,Circuit##OTHER##,Voltage Comment##OTHER##,Driver Comment##OTHER##,Mounting##Other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,C Cable Integer##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Photometric Web File##OTHER##,Driver##Other##
"ASM1SRL8""100LF27K1CUNVxJ24_","ASM1SRL8""100LF27K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF27K1CUNVxJ48_","ASM1SRL8""100LF27K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF27K1CUNVxJ96_","ASM1SRL8""100LF27K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF27K1CUNVxJ120_","ASM1SRL8""100LF27K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF27K1CUNVxDTG","ASM1SRL8""100LF27K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF27K1CUNVxDTS","ASM1SRL8""100LF27K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF27K1CUNVxJ24_","ASM1SRL8""200LF27K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF27K1CUNVxJ48_","ASM1SRL8""200LF27K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF27K1CUNVxJ96_","ASM1SRL8""200LF27K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF27K1CUNVxJ120_","ASM1SRL8""200LF27K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF27K1CUNVxDTG","ASM1SRL8""200LF27K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF27K1CUNVxDTS","ASM1SRL8""200LF27K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF27K1CUNVxJ24_","ASM1SRL8""300LF27K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF27K1CUNVxJ48_","ASM1SRL8""300LF27K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF27K1CUNVxJ96_","ASM1SRL8""300LF27K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF27K1CUNVxJ120_","ASM1SRL8""300LF27K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF27K1CUNVxDTG","ASM1SRL8""300LF27K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF27K1CUNVxDTS","ASM1SRL8""300LF27K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF27K1CUNVxJ24_","ASM1SRL8""400LF27K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF27K1CUNVxJ48_","ASM1SRL8""400LF27K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF27K1CUNVxJ96_","ASM1SRL8""400LF27K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF27K1CUNVxJ120_","ASM1SRL8""400LF27K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF27K1CUNVxDTG","ASM1SRL8""400LF27K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF27K1CUNVxDTS","ASM1SRL8""400LF27K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF27K1CUNVxJ24_","ASM1SRL8""500LF27K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF27K1CUNVxJ48_","ASM1SRL8""500LF27K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF27K1CUNVxJ96_","ASM1SRL8""500LF27K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF27K1CUNVxJ120_","ASM1SRL8""500LF27K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF27K1CUNVxDTG","ASM1SRL8""500LF27K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF27K1CUNVxDTS","ASM1SRL8""500LF27K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF27K1CUNVxJ24_","ASM1SRL12""100LF27K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF27K1CUNVxJ48_","ASM1SRL12""100LF27K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF27K1CUNVxJ96_","ASM1SRL12""100LF27K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF27K1CUNVxJ120_","ASM1SRL12""100LF27K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF27K1CUNVxDTG","ASM1SRL12""100LF27K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF27K1CUNVxDTS","ASM1SRL12""100LF27K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF27K1CUNVxJ24_","ASM1SRL12""200LF27K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF27K1CUNVxJ48_","ASM1SRL12""200LF27K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF27K1CUNVxJ96_","ASM1SRL12""200LF27K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF27K1CUNVxJ120_","ASM1SRL12""200LF27K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF27K1CUNVxDTG","ASM1SRL12""200LF27K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF27K1CUNVxDTS","ASM1SRL12""200LF27K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF27K1CUNVxJ24_","ASM1SRL12""300LF27K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF27K1CUNVxJ48_","ASM1SRL12""300LF27K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF27K1CUNVxJ96_","ASM1SRL12""300LF27K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF27K1CUNVxJ120_","ASM1SRL12""300LF27K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF27K1CUNVxDTG","ASM1SRL12""300LF27K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF27K1CUNVxDTS","ASM1SRL12""300LF27K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF27K1CUNVxJ24_","ASM1SRL12""400LF27K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF27K1CUNVxJ48_","ASM1SRL12""400LF27K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF27K1CUNVxJ96_","ASM1SRL12""400LF27K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF27K1CUNVxJ120_","ASM1SRL12""400LF27K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF27K1CUNVxDTG","ASM1SRL12""400LF27K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF27K1CUNVxDTS","ASM1SRL12""400LF27K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF27K1CUNVxJ24_","ASM1SRL12""500LF27K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF27K1CUNVxJ48_","ASM1SRL12""500LF27K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF27K1CUNVxJ96_","ASM1SRL12""500LF27K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF27K1CUNVxJ120_","ASM1SRL12""500LF27K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF27K1CUNVxDTG","ASM1SRL12""500LF27K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF27K1CUNVxDTS","ASM1SRL12""500LF27K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF27K1CUNVxJ24_","ASM1SRL16""100LF27K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF27K1CUNVxJ48_","ASM1SRL16""100LF27K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF27K1CUNVxJ96_","ASM1SRL16""100LF27K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF27K1CUNVxJ120_","ASM1SRL16""100LF27K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF27K1CUNVxDTG","ASM1SRL16""100LF27K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF27K1CUNVxDTS","ASM1SRL16""100LF27K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF27K1CUNVxJ24_","ASM1SRL16""200LF27K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF27K1CUNVxJ48_","ASM1SRL16""200LF27K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF27K1CUNVxJ96_","ASM1SRL16""200LF27K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF27K1CUNVxJ120_","ASM1SRL16""200LF27K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF27K1CUNVxDTG","ASM1SRL16""200LF27K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF27K1CUNVxDTS","ASM1SRL16""200LF27K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF27K1CUNVxJ24_","ASM1SRL16""300LF27K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF27K1CUNVxJ48_","ASM1SRL16""300LF27K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF27K1CUNVxJ96_","ASM1SRL16""300LF27K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF27K1CUNVxJ120_","ASM1SRL16""300LF27K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF27K1CUNVxDTG","ASM1SRL16""300LF27K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF27K1CUNVxDTS","ASM1SRL16""300LF27K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF27K1CUNVxJ24_","ASM1SRL16""400LF27K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF27K1CUNVxJ48_","ASM1SRL16""400LF27K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF27K1CUNVxJ96_","ASM1SRL16""400LF27K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF27K1CUNVxJ120_","ASM1SRL16""400LF27K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF27K1CUNVxDTG","ASM1SRL16""400LF27K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF27K1CUNVxDTS","ASM1SRL16""400LF27K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF27K1CUNVxJ24_","ASM1SRL16""500LF27K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF27K1CUNVxJ48_","ASM1SRL16""500LF27K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF27K1CUNVxJ96_","ASM1SRL16""500LF27K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF27K1CUNVxJ120_","ASM1SRL16""500LF27K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF27K1CUNVxDTG","ASM1SRL16""500LF27K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF27K1CUNVxDTS","ASM1SRL16""500LF27K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF27K1CUNVxJ24_","ASM1SAS8""100LF27K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF27K1CUNVxJ48_","ASM1SAS8""100LF27K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF27K1CUNVxJ96_","ASM1SAS8""100LF27K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF27K1CUNVxJ120_","ASM1SAS8""100LF27K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF27K1CUNVxDTG","ASM1SAS8""100LF27K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF27K1CUNVxDTS","ASM1SAS8""100LF27K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF27K1CUNVxJ24_","ASM1SAS8""200LF27K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF27K1CUNVxJ48_","ASM1SAS8""200LF27K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF27K1CUNVxJ96_","ASM1SAS8""200LF27K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF27K1CUNVxJ120_","ASM1SAS8""200LF27K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF27K1CUNVxDTG","ASM1SAS8""200LF27K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF27K1CUNVxDTS","ASM1SAS8""200LF27K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF27K1CUNVxJ24_","ASM1SAS8""300LF27K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF27K1CUNVxJ48_","ASM1SAS8""300LF27K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF27K1CUNVxJ96_","ASM1SAS8""300LF27K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF27K1CUNVxJ120_","ASM1SAS8""300LF27K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF27K1CUNVxDTG","ASM1SAS8""300LF27K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF27K1CUNVxDTS","ASM1SAS8""300LF27K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF27K1CUNVxJ24_","ASM1SAS8""400LF27K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF27K1CUNVxJ48_","ASM1SAS8""400LF27K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF27K1CUNVxJ96_","ASM1SAS8""400LF27K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF27K1CUNVxJ120_","ASM1SAS8""400LF27K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF27K1CUNVxDTG","ASM1SAS8""400LF27K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF27K1CUNVxDTS","ASM1SAS8""400LF27K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF27K1CUNVxJ24_","ASM1SAS8""500LF27K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF27K1CUNVxJ48_","ASM1SAS8""500LF27K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF27K1CUNVxJ96_","ASM1SAS8""500LF27K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF27K1CUNVxJ120_","ASM1SAS8""500LF27K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF27K1CUNVxDTG","ASM1SAS8""500LF27K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF27K1CUNVxDTS","ASM1SAS8""500LF27K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF27K1CUNVxJ24_","ASM1SAS12""100LF27K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF27K1CUNVxJ48_","ASM1SAS12""100LF27K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF27K1CUNVxJ96_","ASM1SAS12""100LF27K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF27K1CUNVxJ120_","ASM1SAS12""100LF27K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF27K1CUNVxDTG","ASM1SAS12""100LF27K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF27K1CUNVxDTS","ASM1SAS12""100LF27K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF27K1CUNVxJ24_","ASM1SAS12""200LF27K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF27K1CUNVxJ48_","ASM1SAS12""200LF27K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF27K1CUNVxJ96_","ASM1SAS12""200LF27K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF27K1CUNVxJ120_","ASM1SAS12""200LF27K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF27K1CUNVxDTG","ASM1SAS12""200LF27K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF27K1CUNVxDTS","ASM1SAS12""200LF27K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF27K1CUNVxJ24_","ASM1SAS12""300LF27K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF27K1CUNVxJ48_","ASM1SAS12""300LF27K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF27K1CUNVxJ96_","ASM1SAS12""300LF27K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF27K1CUNVxJ120_","ASM1SAS12""300LF27K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF27K1CUNVxDTG","ASM1SAS12""300LF27K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF27K1CUNVxDTS","ASM1SAS12""300LF27K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF27K1CUNVxJ24_","ASM1SAS12""400LF27K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF27K1CUNVxJ48_","ASM1SAS12""400LF27K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF27K1CUNVxJ96_","ASM1SAS12""400LF27K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF27K1CUNVxJ120_","ASM1SAS12""400LF27K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF27K1CUNVxDTG","ASM1SAS12""400LF27K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF27K1CUNVxDTS","ASM1SAS12""400LF27K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF27K1CUNVxJ24_","ASM1SAS12""500LF27K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF27K1CUNVxJ48_","ASM1SAS12""500LF27K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF27K1CUNVxJ96_","ASM1SAS12""500LF27K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF27K1CUNVxJ120_","ASM1SAS12""500LF27K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF27K1CUNVxDTG","ASM1SAS12""500LF27K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF27K1CUNVxDTS","ASM1SAS12""500LF27K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF27K1CUNVxJ24_","ASM1SAS16""100LF27K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF27K1CUNVxJ48_","ASM1SAS16""100LF27K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF27K1CUNVxJ96_","ASM1SAS16""100LF27K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF27K1CUNVxJ120_","ASM1SAS16""100LF27K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF27K1CUNVxDTG","ASM1SAS16""100LF27K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF27K1CUNVxDTS","ASM1SAS16""100LF27K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF27K1CUNVxJ24_","ASM1SAS16""200LF27K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF27K1CUNVxJ48_","ASM1SAS16""200LF27K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF27K1CUNVxJ96_","ASM1SAS16""200LF27K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF27K1CUNVxJ120_","ASM1SAS16""200LF27K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF27K1CUNVxDTG","ASM1SAS16""200LF27K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF27K1CUNVxDTS","ASM1SAS16""200LF27K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF27K1CUNVxJ24_","ASM1SAS16""300LF27K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF27K1CUNVxJ48_","ASM1SAS16""300LF27K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF27K1CUNVxJ96_","ASM1SAS16""300LF27K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF27K1CUNVxJ120_","ASM1SAS16""300LF27K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF27K1CUNVxDTG","ASM1SAS16""300LF27K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF27K1CUNVxDTS","ASM1SAS16""300LF27K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF27K1CUNVxJ24_","ASM1SAS16""400LF27K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF27K1CUNVxJ48_","ASM1SAS16""400LF27K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF27K1CUNVxJ96_","ASM1SAS16""400LF27K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF27K1CUNVxJ120_","ASM1SAS16""400LF27K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF27K1CUNVxDTG","ASM1SAS16""400LF27K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF27K1CUNVxDTS","ASM1SAS16""400LF27K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF27K1CUNVxJ24_","ASM1SAS16""500LF27K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF27K1CUNVxJ48_","ASM1SAS16""500LF27K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF27K1CUNVxJ96_","ASM1SAS16""500LF27K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF27K1CUNVxJ120_","ASM1SAS16""500LF27K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF27K1CUNVxDTG","ASM1SAS16""500LF27K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF27K1CUNVxDTS","ASM1SAS16""500LF27K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF27K1CUNVxJ24_","ASM1SBW8""100LF27K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF27K1CUNVxJ48_","ASM1SBW8""100LF27K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF27K1CUNVxJ96_","ASM1SBW8""100LF27K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF27K1CUNVxJ120_","ASM1SBW8""100LF27K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF27K1CUNVxDTG","ASM1SBW8""100LF27K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF27K1CUNVxDTS","ASM1SBW8""100LF27K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF27K1CUNVxJ24_","ASM1SBW8""200LF27K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF27K1CUNVxJ48_","ASM1SBW8""200LF27K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF27K1CUNVxJ96_","ASM1SBW8""200LF27K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF27K1CUNVxJ120_","ASM1SBW8""200LF27K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF27K1CUNVxDTG","ASM1SBW8""200LF27K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF27K1CUNVxDTS","ASM1SBW8""200LF27K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF27K1CUNVxJ24_","ASM1SBW8""300LF27K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF27K1CUNVxJ48_","ASM1SBW8""300LF27K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF27K1CUNVxJ96_","ASM1SBW8""300LF27K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF27K1CUNVxJ120_","ASM1SBW8""300LF27K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF27K1CUNVxDTG","ASM1SBW8""300LF27K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF27K1CUNVxDTS","ASM1SBW8""300LF27K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF27K1CUNVxJ24_","ASM1SBW8""400LF27K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF27K1CUNVxJ48_","ASM1SBW8""400LF27K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF27K1CUNVxJ96_","ASM1SBW8""400LF27K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF27K1CUNVxJ120_","ASM1SBW8""400LF27K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF27K1CUNVxDTG","ASM1SBW8""400LF27K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF27K1CUNVxDTS","ASM1SBW8""400LF27K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF27K1CUNVxJ24_","ASM1SBW8""500LF27K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF27K1CUNVxJ48_","ASM1SBW8""500LF27K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF27K1CUNVxJ96_","ASM1SBW8""500LF27K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF27K1CUNVxJ120_","ASM1SBW8""500LF27K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF27K1CUNVxDTG","ASM1SBW8""500LF27K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF27K1CUNVxDTS","ASM1SBW8""500LF27K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF27K1CUNVxJ24_","ASM1SBW12""100LF27K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF27K1CUNVxJ48_","ASM1SBW12""100LF27K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF27K1CUNVxJ96_","ASM1SBW12""100LF27K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF27K1CUNVxJ120_","ASM1SBW12""100LF27K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF27K1CUNVxDTG","ASM1SBW12""100LF27K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF27K1CUNVxDTS","ASM1SBW12""100LF27K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF27K1CUNVxJ24_","ASM1SBW12""200LF27K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF27K1CUNVxJ48_","ASM1SBW12""200LF27K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF27K1CUNVxJ96_","ASM1SBW12""200LF27K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF27K1CUNVxJ120_","ASM1SBW12""200LF27K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF27K1CUNVxDTG","ASM1SBW12""200LF27K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF27K1CUNVxDTS","ASM1SBW12""200LF27K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF27K1CUNVxJ24_","ASM1SBW12""300LF27K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF27K1CUNVxJ48_","ASM1SBW12""300LF27K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF27K1CUNVxJ96_","ASM1SBW12""300LF27K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF27K1CUNVxJ120_","ASM1SBW12""300LF27K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF27K1CUNVxDTG","ASM1SBW12""300LF27K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF27K1CUNVxDTS","ASM1SBW12""300LF27K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF27K1CUNVxJ24_","ASM1SBW12""400LF27K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF27K1CUNVxJ48_","ASM1SBW12""400LF27K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF27K1CUNVxJ96_","ASM1SBW12""400LF27K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF27K1CUNVxJ120_","ASM1SBW12""400LF27K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF27K1CUNVxDTG","ASM1SBW12""400LF27K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF27K1CUNVxDTS","ASM1SBW12""400LF27K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF27K1CUNVxJ24_","ASM1SBW12""500LF27K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF27K1CUNVxJ48_","ASM1SBW12""500LF27K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF27K1CUNVxJ96_","ASM1SBW12""500LF27K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF27K1CUNVxJ120_","ASM1SBW12""500LF27K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF27K1CUNVxDTG","ASM1SBW12""500LF27K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF27K1CUNVxDTS","ASM1SBW12""500LF27K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF27K1CUNVxJ24_","ASM1SBW16""100LF27K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF27K1CUNVxJ48_","ASM1SBW16""100LF27K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF27K1CUNVxJ96_","ASM1SBW16""100LF27K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF27K1CUNVxJ120_","ASM1SBW16""100LF27K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF27K1CUNVxDTG","ASM1SBW16""100LF27K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF27K1CUNVxDTS","ASM1SBW16""100LF27K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF27K1CUNVxJ24_","ASM1SBW16""200LF27K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF27K1CUNVxJ48_","ASM1SBW16""200LF27K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF27K1CUNVxJ96_","ASM1SBW16""200LF27K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF27K1CUNVxJ120_","ASM1SBW16""200LF27K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF27K1CUNVxDTG","ASM1SBW16""200LF27K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF27K1CUNVxDTS","ASM1SBW16""200LF27K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF27K1CUNVxJ24_","ASM1SBW16""300LF27K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF27K1CUNVxJ48_","ASM1SBW16""300LF27K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF27K1CUNVxJ96_","ASM1SBW16""300LF27K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF27K1CUNVxJ120_","ASM1SBW16""300LF27K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF27K1CUNVxDTG","ASM1SBW16""300LF27K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF27K1CUNVxDTS","ASM1SBW16""300LF27K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF27K1CUNVxJ24_","ASM1SBW16""400LF27K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF27K1CUNVxJ48_","ASM1SBW16""400LF27K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF27K1CUNVxJ96_","ASM1SBW16""400LF27K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF27K1CUNVxJ120_","ASM1SBW16""400LF27K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF27K1CUNVxDTG","ASM1SBW16""400LF27K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF27K1CUNVxDTS","ASM1SBW16""400LF27K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF27K1CUNVxJ24_","ASM1SBW16""500LF27K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF27K1CUNVxJ48_","ASM1SBW16""500LF27K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF27K1CUNVxJ96_","ASM1SBW16""500LF27K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF27K1CUNVxJ120_","ASM1SBW16""500LF27K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF27K1CUNVxDTG","ASM1SBW16""500LF27K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF27K1CUNVxDTS","ASM1SBW16""500LF27K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF927K1CUNVxJ24_","ASM1SRL8""100LF927K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF927K1CUNVxJ48_","ASM1SRL8""100LF927K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF927K1CUNVxJ96_","ASM1SRL8""100LF927K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF927K1CUNVxJ120_","ASM1SRL8""100LF927K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF927K1CUNVxDTG","ASM1SRL8""100LF927K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF927K1CUNVxDTS","ASM1SRL8""100LF927K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF927K1CUNVxJ24_","ASM1SRL8""200LF927K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF927K1CUNVxJ48_","ASM1SRL8""200LF927K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF927K1CUNVxJ96_","ASM1SRL8""200LF927K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF927K1CUNVxJ120_","ASM1SRL8""200LF927K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF927K1CUNVxDTG","ASM1SRL8""200LF927K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF927K1CUNVxDTS","ASM1SRL8""200LF927K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF927K1CUNVxJ24_","ASM1SRL8""300LF927K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF927K1CUNVxJ48_","ASM1SRL8""300LF927K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF927K1CUNVxJ96_","ASM1SRL8""300LF927K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF927K1CUNVxJ120_","ASM1SRL8""300LF927K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF927K1CUNVxDTG","ASM1SRL8""300LF927K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF927K1CUNVxDTS","ASM1SRL8""300LF927K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF927K1CUNVxJ24_","ASM1SRL8""400LF927K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF927K1CUNVxJ48_","ASM1SRL8""400LF927K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF927K1CUNVxJ96_","ASM1SRL8""400LF927K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF927K1CUNVxJ120_","ASM1SRL8""400LF927K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF927K1CUNVxDTG","ASM1SRL8""400LF927K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF927K1CUNVxDTS","ASM1SRL8""400LF927K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF927K1CUNVxJ24_","ASM1SRL8""500LF927K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF927K1CUNVxJ48_","ASM1SRL8""500LF927K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF927K1CUNVxJ96_","ASM1SRL8""500LF927K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF927K1CUNVxJ120_","ASM1SRL8""500LF927K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF927K1CUNVxDTG","ASM1SRL8""500LF927K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF927K1CUNVxDTS","ASM1SRL8""500LF927K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF927K1CUNVxJ24_","ASM1SRL12""100LF927K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF927K1CUNVxJ48_","ASM1SRL12""100LF927K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF927K1CUNVxJ96_","ASM1SRL12""100LF927K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF927K1CUNVxJ120_","ASM1SRL12""100LF927K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF927K1CUNVxDTG","ASM1SRL12""100LF927K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF927K1CUNVxDTS","ASM1SRL12""100LF927K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF927K1CUNVxJ24_","ASM1SRL12""200LF927K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF927K1CUNVxJ48_","ASM1SRL12""200LF927K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF927K1CUNVxJ96_","ASM1SRL12""200LF927K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF927K1CUNVxJ120_","ASM1SRL12""200LF927K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF927K1CUNVxDTG","ASM1SRL12""200LF927K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF927K1CUNVxDTS","ASM1SRL12""200LF927K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF927K1CUNVxJ24_","ASM1SRL12""300LF927K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF927K1CUNVxJ48_","ASM1SRL12""300LF927K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF927K1CUNVxJ96_","ASM1SRL12""300LF927K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF927K1CUNVxJ120_","ASM1SRL12""300LF927K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF927K1CUNVxDTG","ASM1SRL12""300LF927K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF927K1CUNVxDTS","ASM1SRL12""300LF927K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF927K1CUNVxJ24_","ASM1SRL12""400LF927K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF927K1CUNVxJ48_","ASM1SRL12""400LF927K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF927K1CUNVxJ96_","ASM1SRL12""400LF927K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF927K1CUNVxJ120_","ASM1SRL12""400LF927K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF927K1CUNVxDTG","ASM1SRL12""400LF927K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF927K1CUNVxDTS","ASM1SRL12""400LF927K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF927K1CUNVxJ24_","ASM1SRL12""500LF927K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF927K1CUNVxJ48_","ASM1SRL12""500LF927K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF927K1CUNVxJ96_","ASM1SRL12""500LF927K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF927K1CUNVxJ120_","ASM1SRL12""500LF927K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF927K1CUNVxDTG","ASM1SRL12""500LF927K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF927K1CUNVxDTS","ASM1SRL12""500LF927K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF927K1CUNVxJ24_","ASM1SRL16""100LF927K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF927K1CUNVxJ48_","ASM1SRL16""100LF927K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF927K1CUNVxJ96_","ASM1SRL16""100LF927K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF927K1CUNVxJ120_","ASM1SRL16""100LF927K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF927K1CUNVxDTG","ASM1SRL16""100LF927K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF927K1CUNVxDTS","ASM1SRL16""100LF927K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF927K1CUNVxJ24_","ASM1SRL16""200LF927K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF927K1CUNVxJ48_","ASM1SRL16""200LF927K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF927K1CUNVxJ96_","ASM1SRL16""200LF927K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF927K1CUNVxJ120_","ASM1SRL16""200LF927K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF927K1CUNVxDTG","ASM1SRL16""200LF927K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF927K1CUNVxDTS","ASM1SRL16""200LF927K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF927K1CUNVxJ24_","ASM1SRL16""300LF927K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF927K1CUNVxJ48_","ASM1SRL16""300LF927K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF927K1CUNVxJ96_","ASM1SRL16""300LF927K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF927K1CUNVxJ120_","ASM1SRL16""300LF927K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF927K1CUNVxDTG","ASM1SRL16""300LF927K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF927K1CUNVxDTS","ASM1SRL16""300LF927K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF927K1CUNVxJ24_","ASM1SRL16""400LF927K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF927K1CUNVxJ48_","ASM1SRL16""400LF927K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF927K1CUNVxJ96_","ASM1SRL16""400LF927K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF927K1CUNVxJ120_","ASM1SRL16""400LF927K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF927K1CUNVxDTG","ASM1SRL16""400LF927K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF927K1CUNVxDTS","ASM1SRL16""400LF927K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF927K1CUNVxJ24_","ASM1SRL16""500LF927K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF927K1CUNVxJ48_","ASM1SRL16""500LF927K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF927K1CUNVxJ96_","ASM1SRL16""500LF927K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF927K1CUNVxJ120_","ASM1SRL16""500LF927K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF927K1CUNVxDTG","ASM1SRL16""500LF927K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF927K1CUNVxDTS","ASM1SRL16""500LF927K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF927K1CUNVxJ24_","ASM1SAS8""100LF927K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF927K1CUNVxJ48_","ASM1SAS8""100LF927K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF927K1CUNVxJ96_","ASM1SAS8""100LF927K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF927K1CUNVxJ120_","ASM1SAS8""100LF927K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF927K1CUNVxDTG","ASM1SAS8""100LF927K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF927K1CUNVxDTS","ASM1SAS8""100LF927K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF927K1CUNVxJ24_","ASM1SAS8""200LF927K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF927K1CUNVxJ48_","ASM1SAS8""200LF927K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF927K1CUNVxJ96_","ASM1SAS8""200LF927K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF927K1CUNVxJ120_","ASM1SAS8""200LF927K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF927K1CUNVxDTG","ASM1SAS8""200LF927K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF927K1CUNVxDTS","ASM1SAS8""200LF927K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF927K1CUNVxJ24_","ASM1SAS8""300LF927K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF927K1CUNVxJ48_","ASM1SAS8""300LF927K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF927K1CUNVxJ96_","ASM1SAS8""300LF927K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF927K1CUNVxJ120_","ASM1SAS8""300LF927K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF927K1CUNVxDTG","ASM1SAS8""300LF927K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF927K1CUNVxDTS","ASM1SAS8""300LF927K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF927K1CUNVxJ24_","ASM1SAS8""400LF927K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF927K1CUNVxJ48_","ASM1SAS8""400LF927K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF927K1CUNVxJ96_","ASM1SAS8""400LF927K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF927K1CUNVxJ120_","ASM1SAS8""400LF927K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF927K1CUNVxDTG","ASM1SAS8""400LF927K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF927K1CUNVxDTS","ASM1SAS8""400LF927K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF927K1CUNVxJ24_","ASM1SAS8""500LF927K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF927K1CUNVxJ48_","ASM1SAS8""500LF927K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF927K1CUNVxJ96_","ASM1SAS8""500LF927K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF927K1CUNVxJ120_","ASM1SAS8""500LF927K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF927K1CUNVxDTG","ASM1SAS8""500LF927K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF927K1CUNVxDTS","ASM1SAS8""500LF927K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF927K1CUNVxJ24_","ASM1SAS12""100LF927K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF927K1CUNVxJ48_","ASM1SAS12""100LF927K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF927K1CUNVxJ96_","ASM1SAS12""100LF927K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF927K1CUNVxJ120_","ASM1SAS12""100LF927K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF927K1CUNVxDTG","ASM1SAS12""100LF927K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF927K1CUNVxDTS","ASM1SAS12""100LF927K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF927K1CUNVxJ24_","ASM1SAS12""200LF927K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF927K1CUNVxJ48_","ASM1SAS12""200LF927K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF927K1CUNVxJ96_","ASM1SAS12""200LF927K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF927K1CUNVxJ120_","ASM1SAS12""200LF927K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF927K1CUNVxDTG","ASM1SAS12""200LF927K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF927K1CUNVxDTS","ASM1SAS12""200LF927K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF927K1CUNVxJ24_","ASM1SAS12""300LF927K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF927K1CUNVxJ48_","ASM1SAS12""300LF927K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF927K1CUNVxJ96_","ASM1SAS12""300LF927K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF927K1CUNVxJ120_","ASM1SAS12""300LF927K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF927K1CUNVxDTG","ASM1SAS12""300LF927K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF927K1CUNVxDTS","ASM1SAS12""300LF927K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF927K1CUNVxJ24_","ASM1SAS12""400LF927K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF927K1CUNVxJ48_","ASM1SAS12""400LF927K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF927K1CUNVxJ96_","ASM1SAS12""400LF927K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF927K1CUNVxJ120_","ASM1SAS12""400LF927K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF927K1CUNVxDTG","ASM1SAS12""400LF927K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF927K1CUNVxDTS","ASM1SAS12""400LF927K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF927K1CUNVxJ24_","ASM1SAS12""500LF927K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF927K1CUNVxJ48_","ASM1SAS12""500LF927K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF927K1CUNVxJ96_","ASM1SAS12""500LF927K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF927K1CUNVxJ120_","ASM1SAS12""500LF927K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF927K1CUNVxDTG","ASM1SAS12""500LF927K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF927K1CUNVxDTS","ASM1SAS12""500LF927K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF927K1CUNVxJ24_","ASM1SAS16""100LF927K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF927K1CUNVxJ48_","ASM1SAS16""100LF927K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF927K1CUNVxJ96_","ASM1SAS16""100LF927K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF927K1CUNVxJ120_","ASM1SAS16""100LF927K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF927K1CUNVxDTG","ASM1SAS16""100LF927K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF927K1CUNVxDTS","ASM1SAS16""100LF927K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF927K1CUNVxJ24_","ASM1SAS16""200LF927K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF927K1CUNVxJ48_","ASM1SAS16""200LF927K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF927K1CUNVxJ96_","ASM1SAS16""200LF927K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF927K1CUNVxJ120_","ASM1SAS16""200LF927K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF927K1CUNVxDTG","ASM1SAS16""200LF927K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF927K1CUNVxDTS","ASM1SAS16""200LF927K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF927K1CUNVxJ24_","ASM1SAS16""300LF927K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF927K1CUNVxJ48_","ASM1SAS16""300LF927K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF927K1CUNVxJ96_","ASM1SAS16""300LF927K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF927K1CUNVxJ120_","ASM1SAS16""300LF927K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF927K1CUNVxDTG","ASM1SAS16""300LF927K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF927K1CUNVxDTS","ASM1SAS16""300LF927K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF927K1CUNVxJ24_","ASM1SAS16""400LF927K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF927K1CUNVxJ48_","ASM1SAS16""400LF927K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF927K1CUNVxJ96_","ASM1SAS16""400LF927K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF927K1CUNVxJ120_","ASM1SAS16""400LF927K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF927K1CUNVxDTG","ASM1SAS16""400LF927K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF927K1CUNVxDTS","ASM1SAS16""400LF927K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF927K1CUNVxJ24_","ASM1SAS16""500LF927K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF927K1CUNVxJ48_","ASM1SAS16""500LF927K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF927K1CUNVxJ96_","ASM1SAS16""500LF927K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF927K1CUNVxJ120_","ASM1SAS16""500LF927K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF927K1CUNVxDTG","ASM1SAS16""500LF927K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF927K1CUNVxDTS","ASM1SAS16""500LF927K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF927K1CUNVxJ24_","ASM1SBW8""100LF927K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF927K1CUNVxJ48_","ASM1SBW8""100LF927K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF927K1CUNVxJ96_","ASM1SBW8""100LF927K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF927K1CUNVxJ120_","ASM1SBW8""100LF927K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF927K1CUNVxDTG","ASM1SBW8""100LF927K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF927K1CUNVxDTS","ASM1SBW8""100LF927K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF927K1CUNVxJ24_","ASM1SBW8""200LF927K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF927K1CUNVxJ48_","ASM1SBW8""200LF927K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF927K1CUNVxJ96_","ASM1SBW8""200LF927K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF927K1CUNVxJ120_","ASM1SBW8""200LF927K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF927K1CUNVxDTG","ASM1SBW8""200LF927K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF927K1CUNVxDTS","ASM1SBW8""200LF927K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF927K1CUNVxJ24_","ASM1SBW8""300LF927K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF927K1CUNVxJ48_","ASM1SBW8""300LF927K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF927K1CUNVxJ96_","ASM1SBW8""300LF927K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF927K1CUNVxJ120_","ASM1SBW8""300LF927K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF927K1CUNVxDTG","ASM1SBW8""300LF927K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF927K1CUNVxDTS","ASM1SBW8""300LF927K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF927K1CUNVxJ24_","ASM1SBW8""400LF927K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF927K1CUNVxJ48_","ASM1SBW8""400LF927K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF927K1CUNVxJ96_","ASM1SBW8""400LF927K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF927K1CUNVxJ120_","ASM1SBW8""400LF927K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF927K1CUNVxDTG","ASM1SBW8""400LF927K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF927K1CUNVxDTS","ASM1SBW8""400LF927K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF927K1CUNVxJ24_","ASM1SBW8""500LF927K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF927K1CUNVxJ48_","ASM1SBW8""500LF927K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF927K1CUNVxJ96_","ASM1SBW8""500LF927K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF927K1CUNVxJ120_","ASM1SBW8""500LF927K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF927K1CUNVxDTG","ASM1SBW8""500LF927K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF927K1CUNVxDTS","ASM1SBW8""500LF927K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF927K1CUNVxJ24_","ASM1SBW12""100LF927K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF927K1CUNVxJ48_","ASM1SBW12""100LF927K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF927K1CUNVxJ96_","ASM1SBW12""100LF927K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF927K1CUNVxJ120_","ASM1SBW12""100LF927K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF927K1CUNVxDTG","ASM1SBW12""100LF927K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF927K1CUNVxDTS","ASM1SBW12""100LF927K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF927K1CUNVxJ24_","ASM1SBW12""200LF927K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF927K1CUNVxJ48_","ASM1SBW12""200LF927K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF927K1CUNVxJ96_","ASM1SBW12""200LF927K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF927K1CUNVxJ120_","ASM1SBW12""200LF927K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF927K1CUNVxDTG","ASM1SBW12""200LF927K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF927K1CUNVxDTS","ASM1SBW12""200LF927K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF927K1CUNVxJ24_","ASM1SBW12""300LF927K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF927K1CUNVxJ48_","ASM1SBW12""300LF927K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF927K1CUNVxJ96_","ASM1SBW12""300LF927K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF927K1CUNVxJ120_","ASM1SBW12""300LF927K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF927K1CUNVxDTG","ASM1SBW12""300LF927K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF927K1CUNVxDTS","ASM1SBW12""300LF927K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF927K1CUNVxJ24_","ASM1SBW12""400LF927K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF927K1CUNVxJ48_","ASM1SBW12""400LF927K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF927K1CUNVxJ96_","ASM1SBW12""400LF927K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF927K1CUNVxJ120_","ASM1SBW12""400LF927K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF927K1CUNVxDTG","ASM1SBW12""400LF927K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF927K1CUNVxDTS","ASM1SBW12""400LF927K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF927K1CUNVxJ24_","ASM1SBW12""500LF927K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF927K1CUNVxJ48_","ASM1SBW12""500LF927K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF927K1CUNVxJ96_","ASM1SBW12""500LF927K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF927K1CUNVxJ120_","ASM1SBW12""500LF927K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF927K1CUNVxDTG","ASM1SBW12""500LF927K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF927K1CUNVxDTS","ASM1SBW12""500LF927K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF927K1CUNVxJ24_","ASM1SBW16""100LF927K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF927K1CUNVxJ48_","ASM1SBW16""100LF927K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF927K1CUNVxJ96_","ASM1SBW16""100LF927K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF927K1CUNVxJ120_","ASM1SBW16""100LF927K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF927K1CUNVxDTG","ASM1SBW16""100LF927K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF927K1CUNVxDTS","ASM1SBW16""100LF927K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF927K1CUNVxJ24_","ASM1SBW16""200LF927K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF927K1CUNVxJ48_","ASM1SBW16""200LF927K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF927K1CUNVxJ96_","ASM1SBW16""200LF927K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF927K1CUNVxJ120_","ASM1SBW16""200LF927K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF927K1CUNVxDTG","ASM1SBW16""200LF927K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF927K1CUNVxDTS","ASM1SBW16""200LF927K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF927K1CUNVxJ24_","ASM1SBW16""300LF927K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF927K1CUNVxJ48_","ASM1SBW16""300LF927K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF927K1CUNVxJ96_","ASM1SBW16""300LF927K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF927K1CUNVxJ120_","ASM1SBW16""300LF927K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF927K1CUNVxDTG","ASM1SBW16""300LF927K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF927K1CUNVxDTS","ASM1SBW16""300LF927K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF927K1CUNVxJ24_","ASM1SBW16""400LF927K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF927K1CUNVxJ48_","ASM1SBW16""400LF927K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF927K1CUNVxJ96_","ASM1SBW16""400LF927K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF927K1CUNVxJ120_","ASM1SBW16""400LF927K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF927K1CUNVxDTG","ASM1SBW16""400LF927K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF927K1CUNVxDTS","ASM1SBW16""400LF927K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF927K1CUNVxJ24_","ASM1SBW16""500LF927K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF927K1CUNVxJ48_","ASM1SBW16""500LF927K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF927K1CUNVxJ96_","ASM1SBW16""500LF927K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF927K1CUNVxJ120_","ASM1SBW16""500LF927K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF927K1CUNVxDTG","ASM1SBW16""500LF927K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF927K1CUNVxDTS","ASM1SBW16""500LF927K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF30K1CUNVxJ24_","ASM1SRL8""100LF30K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF30K1CUNVxJ48_","ASM1SRL8""100LF30K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF30K1CUNVxJ96_","ASM1SRL8""100LF30K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF30K1CUNVxJ120_","ASM1SRL8""100LF30K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF30K1CUNVxDTG","ASM1SRL8""100LF30K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF30K1CUNVxDTS","ASM1SRL8""100LF30K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF30K1CUNVxJ24_","ASM1SRL8""200LF30K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF30K1CUNVxJ48_","ASM1SRL8""200LF30K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF30K1CUNVxJ96_","ASM1SRL8""200LF30K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF30K1CUNVxJ120_","ASM1SRL8""200LF30K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF30K1CUNVxDTG","ASM1SRL8""200LF30K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF30K1CUNVxDTS","ASM1SRL8""200LF30K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF30K1CUNVxJ24_","ASM1SRL8""300LF30K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF30K1CUNVxJ48_","ASM1SRL8""300LF30K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF30K1CUNVxJ96_","ASM1SRL8""300LF30K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF30K1CUNVxJ120_","ASM1SRL8""300LF30K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF30K1CUNVxDTG","ASM1SRL8""300LF30K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF30K1CUNVxDTS","ASM1SRL8""300LF30K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF30K1CUNVxJ24_","ASM1SRL8""400LF30K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF30K1CUNVxJ48_","ASM1SRL8""400LF30K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF30K1CUNVxJ96_","ASM1SRL8""400LF30K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF30K1CUNVxJ120_","ASM1SRL8""400LF30K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF30K1CUNVxDTG","ASM1SRL8""400LF30K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF30K1CUNVxDTS","ASM1SRL8""400LF30K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF30K1CUNVxJ24_","ASM1SRL8""500LF30K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF30K1CUNVxJ48_","ASM1SRL8""500LF30K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF30K1CUNVxJ96_","ASM1SRL8""500LF30K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF30K1CUNVxJ120_","ASM1SRL8""500LF30K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF30K1CUNVxDTG","ASM1SRL8""500LF30K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF30K1CUNVxDTS","ASM1SRL8""500LF30K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF30K1CUNVxJ24_","ASM1SRL12""100LF30K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF30K1CUNVxJ48_","ASM1SRL12""100LF30K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF30K1CUNVxJ96_","ASM1SRL12""100LF30K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF30K1CUNVxJ120_","ASM1SRL12""100LF30K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF30K1CUNVxDTG","ASM1SRL12""100LF30K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF30K1CUNVxDTS","ASM1SRL12""100LF30K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF30K1CUNVxJ24_","ASM1SRL12""200LF30K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF30K1CUNVxJ48_","ASM1SRL12""200LF30K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF30K1CUNVxJ96_","ASM1SRL12""200LF30K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF30K1CUNVxJ120_","ASM1SRL12""200LF30K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF30K1CUNVxDTG","ASM1SRL12""200LF30K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF30K1CUNVxDTS","ASM1SRL12""200LF30K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF30K1CUNVxJ24_","ASM1SRL12""300LF30K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF30K1CUNVxJ48_","ASM1SRL12""300LF30K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF30K1CUNVxJ96_","ASM1SRL12""300LF30K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF30K1CUNVxJ120_","ASM1SRL12""300LF30K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF30K1CUNVxDTG","ASM1SRL12""300LF30K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF30K1CUNVxDTS","ASM1SRL12""300LF30K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF30K1CUNVxJ24_","ASM1SRL12""400LF30K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF30K1CUNVxJ48_","ASM1SRL12""400LF30K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF30K1CUNVxJ96_","ASM1SRL12""400LF30K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF30K1CUNVxJ120_","ASM1SRL12""400LF30K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF30K1CUNVxDTG","ASM1SRL12""400LF30K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF30K1CUNVxDTS","ASM1SRL12""400LF30K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF30K1CUNVxJ24_","ASM1SRL12""500LF30K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF30K1CUNVxJ48_","ASM1SRL12""500LF30K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF30K1CUNVxJ96_","ASM1SRL12""500LF30K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF30K1CUNVxJ120_","ASM1SRL12""500LF30K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF30K1CUNVxDTG","ASM1SRL12""500LF30K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF30K1CUNVxDTS","ASM1SRL12""500LF30K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF30K1CUNVxJ24_","ASM1SRL16""100LF30K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF30K1CUNVxJ48_","ASM1SRL16""100LF30K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF30K1CUNVxJ96_","ASM1SRL16""100LF30K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF30K1CUNVxJ120_","ASM1SRL16""100LF30K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF30K1CUNVxDTG","ASM1SRL16""100LF30K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF30K1CUNVxDTS","ASM1SRL16""100LF30K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF30K1CUNVxJ24_","ASM1SRL16""200LF30K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF30K1CUNVxJ48_","ASM1SRL16""200LF30K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF30K1CUNVxJ96_","ASM1SRL16""200LF30K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF30K1CUNVxJ120_","ASM1SRL16""200LF30K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF30K1CUNVxDTG","ASM1SRL16""200LF30K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF30K1CUNVxDTS","ASM1SRL16""200LF30K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF30K1CUNVxJ24_","ASM1SRL16""300LF30K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF30K1CUNVxJ48_","ASM1SRL16""300LF30K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF30K1CUNVxJ96_","ASM1SRL16""300LF30K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF30K1CUNVxJ120_","ASM1SRL16""300LF30K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF30K1CUNVxDTG","ASM1SRL16""300LF30K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF30K1CUNVxDTS","ASM1SRL16""300LF30K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF30K1CUNVxJ24_","ASM1SRL16""400LF30K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF30K1CUNVxJ48_","ASM1SRL16""400LF30K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF30K1CUNVxJ96_","ASM1SRL16""400LF30K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF30K1CUNVxJ120_","ASM1SRL16""400LF30K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF30K1CUNVxDTG","ASM1SRL16""400LF30K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF30K1CUNVxDTS","ASM1SRL16""400LF30K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF30K1CUNVxJ24_","ASM1SRL16""500LF30K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF30K1CUNVxJ48_","ASM1SRL16""500LF30K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF30K1CUNVxJ96_","ASM1SRL16""500LF30K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF30K1CUNVxJ120_","ASM1SRL16""500LF30K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF30K1CUNVxDTG","ASM1SRL16""500LF30K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF30K1CUNVxDTS","ASM1SRL16""500LF30K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF30K1CUNVxJ24_","ASM1SAS8""100LF30K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF30K1CUNVxJ48_","ASM1SAS8""100LF30K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF30K1CUNVxJ96_","ASM1SAS8""100LF30K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF30K1CUNVxJ120_","ASM1SAS8""100LF30K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF30K1CUNVxDTG","ASM1SAS8""100LF30K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF30K1CUNVxDTS","ASM1SAS8""100LF30K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF30K1CUNVxJ24_","ASM1SAS8""200LF30K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF30K1CUNVxJ48_","ASM1SAS8""200LF30K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF30K1CUNVxJ96_","ASM1SAS8""200LF30K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF30K1CUNVxJ120_","ASM1SAS8""200LF30K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF30K1CUNVxDTG","ASM1SAS8""200LF30K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF30K1CUNVxDTS","ASM1SAS8""200LF30K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF30K1CUNVxJ24_","ASM1SAS8""300LF30K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF30K1CUNVxJ48_","ASM1SAS8""300LF30K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF30K1CUNVxJ96_","ASM1SAS8""300LF30K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF30K1CUNVxJ120_","ASM1SAS8""300LF30K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF30K1CUNVxDTG","ASM1SAS8""300LF30K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF30K1CUNVxDTS","ASM1SAS8""300LF30K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF30K1CUNVxJ24_","ASM1SAS8""400LF30K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF30K1CUNVxJ48_","ASM1SAS8""400LF30K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF30K1CUNVxJ96_","ASM1SAS8""400LF30K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF30K1CUNVxJ120_","ASM1SAS8""400LF30K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF30K1CUNVxDTG","ASM1SAS8""400LF30K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF30K1CUNVxDTS","ASM1SAS8""400LF30K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF30K1CUNVxJ24_","ASM1SAS8""500LF30K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF30K1CUNVxJ48_","ASM1SAS8""500LF30K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF30K1CUNVxJ96_","ASM1SAS8""500LF30K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF30K1CUNVxJ120_","ASM1SAS8""500LF30K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF30K1CUNVxDTG","ASM1SAS8""500LF30K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF30K1CUNVxDTS","ASM1SAS8""500LF30K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF30K1CUNVxJ24_","ASM1SAS12""100LF30K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF30K1CUNVxJ48_","ASM1SAS12""100LF30K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF30K1CUNVxJ96_","ASM1SAS12""100LF30K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF30K1CUNVxJ120_","ASM1SAS12""100LF30K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF30K1CUNVxDTG","ASM1SAS12""100LF30K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF30K1CUNVxDTS","ASM1SAS12""100LF30K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF30K1CUNVxJ24_","ASM1SAS12""200LF30K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF30K1CUNVxJ48_","ASM1SAS12""200LF30K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF30K1CUNVxJ96_","ASM1SAS12""200LF30K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF30K1CUNVxJ120_","ASM1SAS12""200LF30K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF30K1CUNVxDTG","ASM1SAS12""200LF30K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF30K1CUNVxDTS","ASM1SAS12""200LF30K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF30K1CUNVxJ24_","ASM1SAS12""300LF30K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF30K1CUNVxJ48_","ASM1SAS12""300LF30K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF30K1CUNVxJ96_","ASM1SAS12""300LF30K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF30K1CUNVxJ120_","ASM1SAS12""300LF30K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF30K1CUNVxDTG","ASM1SAS12""300LF30K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF30K1CUNVxDTS","ASM1SAS12""300LF30K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF30K1CUNVxJ24_","ASM1SAS12""400LF30K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF30K1CUNVxJ48_","ASM1SAS12""400LF30K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF30K1CUNVxJ96_","ASM1SAS12""400LF30K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF30K1CUNVxJ120_","ASM1SAS12""400LF30K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF30K1CUNVxDTG","ASM1SAS12""400LF30K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF30K1CUNVxDTS","ASM1SAS12""400LF30K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF30K1CUNVxJ24_","ASM1SAS12""500LF30K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF30K1CUNVxJ48_","ASM1SAS12""500LF30K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF30K1CUNVxJ96_","ASM1SAS12""500LF30K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF30K1CUNVxJ120_","ASM1SAS12""500LF30K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF30K1CUNVxDTG","ASM1SAS12""500LF30K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF30K1CUNVxDTS","ASM1SAS12""500LF30K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF30K1CUNVxJ24_","ASM1SAS16""100LF30K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF30K1CUNVxJ48_","ASM1SAS16""100LF30K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF30K1CUNVxJ96_","ASM1SAS16""100LF30K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF30K1CUNVxJ120_","ASM1SAS16""100LF30K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF30K1CUNVxDTG","ASM1SAS16""100LF30K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF30K1CUNVxDTS","ASM1SAS16""100LF30K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF30K1CUNVxJ24_","ASM1SAS16""200LF30K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF30K1CUNVxJ48_","ASM1SAS16""200LF30K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF30K1CUNVxJ96_","ASM1SAS16""200LF30K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF30K1CUNVxJ120_","ASM1SAS16""200LF30K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF30K1CUNVxDTG","ASM1SAS16""200LF30K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF30K1CUNVxDTS","ASM1SAS16""200LF30K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF30K1CUNVxJ24_","ASM1SAS16""300LF30K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF30K1CUNVxJ48_","ASM1SAS16""300LF30K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF30K1CUNVxJ96_","ASM1SAS16""300LF30K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF30K1CUNVxJ120_","ASM1SAS16""300LF30K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF30K1CUNVxDTG","ASM1SAS16""300LF30K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF30K1CUNVxDTS","ASM1SAS16""300LF30K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF30K1CUNVxJ24_","ASM1SAS16""400LF30K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF30K1CUNVxJ48_","ASM1SAS16""400LF30K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF30K1CUNVxJ96_","ASM1SAS16""400LF30K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF30K1CUNVxJ120_","ASM1SAS16""400LF30K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF30K1CUNVxDTG","ASM1SAS16""400LF30K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF30K1CUNVxDTS","ASM1SAS16""400LF30K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF30K1CUNVxJ24_","ASM1SAS16""500LF30K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF30K1CUNVxJ48_","ASM1SAS16""500LF30K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF30K1CUNVxJ96_","ASM1SAS16""500LF30K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF30K1CUNVxJ120_","ASM1SAS16""500LF30K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF30K1CUNVxDTG","ASM1SAS16""500LF30K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF30K1CUNVxDTS","ASM1SAS16""500LF30K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF30K1CUNVxJ24_","ASM1SBW8""100LF30K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF30K1CUNVxJ48_","ASM1SBW8""100LF30K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF30K1CUNVxJ96_","ASM1SBW8""100LF30K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF30K1CUNVxJ120_","ASM1SBW8""100LF30K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF30K1CUNVxDTG","ASM1SBW8""100LF30K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF30K1CUNVxDTS","ASM1SBW8""100LF30K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF30K1CUNVxJ24_","ASM1SBW8""200LF30K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF30K1CUNVxJ48_","ASM1SBW8""200LF30K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF30K1CUNVxJ96_","ASM1SBW8""200LF30K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF30K1CUNVxJ120_","ASM1SBW8""200LF30K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF30K1CUNVxDTG","ASM1SBW8""200LF30K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF30K1CUNVxDTS","ASM1SBW8""200LF30K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF30K1CUNVxJ24_","ASM1SBW8""300LF30K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF30K1CUNVxJ48_","ASM1SBW8""300LF30K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF30K1CUNVxJ96_","ASM1SBW8""300LF30K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF30K1CUNVxJ120_","ASM1SBW8""300LF30K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF30K1CUNVxDTG","ASM1SBW8""300LF30K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF30K1CUNVxDTS","ASM1SBW8""300LF30K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF30K1CUNVxJ24_","ASM1SBW8""400LF30K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF30K1CUNVxJ48_","ASM1SBW8""400LF30K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF30K1CUNVxJ96_","ASM1SBW8""400LF30K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF30K1CUNVxJ120_","ASM1SBW8""400LF30K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF30K1CUNVxDTG","ASM1SBW8""400LF30K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF30K1CUNVxDTS","ASM1SBW8""400LF30K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF30K1CUNVxJ24_","ASM1SBW8""500LF30K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF30K1CUNVxJ48_","ASM1SBW8""500LF30K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF30K1CUNVxJ96_","ASM1SBW8""500LF30K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF30K1CUNVxJ120_","ASM1SBW8""500LF30K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF30K1CUNVxDTG","ASM1SBW8""500LF30K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF30K1CUNVxDTS","ASM1SBW8""500LF30K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF30K1CUNVxJ24_","ASM1SBW12""100LF30K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF30K1CUNVxJ48_","ASM1SBW12""100LF30K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF30K1CUNVxJ96_","ASM1SBW12""100LF30K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF30K1CUNVxJ120_","ASM1SBW12""100LF30K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF30K1CUNVxDTG","ASM1SBW12""100LF30K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF30K1CUNVxDTS","ASM1SBW12""100LF30K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF30K1CUNVxJ24_","ASM1SBW12""200LF30K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF30K1CUNVxJ48_","ASM1SBW12""200LF30K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF30K1CUNVxJ96_","ASM1SBW12""200LF30K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF30K1CUNVxJ120_","ASM1SBW12""200LF30K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF30K1CUNVxDTG","ASM1SBW12""200LF30K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF30K1CUNVxDTS","ASM1SBW12""200LF30K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF30K1CUNVxJ24_","ASM1SBW12""300LF30K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF30K1CUNVxJ48_","ASM1SBW12""300LF30K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF30K1CUNVxJ96_","ASM1SBW12""300LF30K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF30K1CUNVxJ120_","ASM1SBW12""300LF30K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF30K1CUNVxDTG","ASM1SBW12""300LF30K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF30K1CUNVxDTS","ASM1SBW12""300LF30K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF30K1CUNVxJ24_","ASM1SBW12""400LF30K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF30K1CUNVxJ48_","ASM1SBW12""400LF30K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF30K1CUNVxJ96_","ASM1SBW12""400LF30K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF30K1CUNVxJ120_","ASM1SBW12""400LF30K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF30K1CUNVxDTG","ASM1SBW12""400LF30K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF30K1CUNVxDTS","ASM1SBW12""400LF30K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF30K1CUNVxJ24_","ASM1SBW12""500LF30K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF30K1CUNVxJ48_","ASM1SBW12""500LF30K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF30K1CUNVxJ96_","ASM1SBW12""500LF30K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF30K1CUNVxJ120_","ASM1SBW12""500LF30K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF30K1CUNVxDTG","ASM1SBW12""500LF30K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF30K1CUNVxDTS","ASM1SBW12""500LF30K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF30K1CUNVxJ24_","ASM1SBW16""100LF30K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF30K1CUNVxJ48_","ASM1SBW16""100LF30K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF30K1CUNVxJ96_","ASM1SBW16""100LF30K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF30K1CUNVxJ120_","ASM1SBW16""100LF30K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF30K1CUNVxDTG","ASM1SBW16""100LF30K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF30K1CUNVxDTS","ASM1SBW16""100LF30K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF30K1CUNVxJ24_","ASM1SBW16""200LF30K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF30K1CUNVxJ48_","ASM1SBW16""200LF30K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF30K1CUNVxJ96_","ASM1SBW16""200LF30K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF30K1CUNVxJ120_","ASM1SBW16""200LF30K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF30K1CUNVxDTG","ASM1SBW16""200LF30K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF30K1CUNVxDTS","ASM1SBW16""200LF30K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF30K1CUNVxJ24_","ASM1SBW16""300LF30K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF30K1CUNVxJ48_","ASM1SBW16""300LF30K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF30K1CUNVxJ96_","ASM1SBW16""300LF30K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF30K1CUNVxJ120_","ASM1SBW16""300LF30K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF30K1CUNVxDTG","ASM1SBW16""300LF30K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF30K1CUNVxDTS","ASM1SBW16""300LF30K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF30K1CUNVxJ24_","ASM1SBW16""400LF30K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF30K1CUNVxJ48_","ASM1SBW16""400LF30K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF30K1CUNVxJ96_","ASM1SBW16""400LF30K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF30K1CUNVxJ120_","ASM1SBW16""400LF30K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF30K1CUNVxDTG","ASM1SBW16""400LF30K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF30K1CUNVxDTS","ASM1SBW16""400LF30K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF30K1CUNVxJ24_","ASM1SBW16""500LF30K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF30K1CUNVxJ48_","ASM1SBW16""500LF30K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF30K1CUNVxJ96_","ASM1SBW16""500LF30K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF30K1CUNVxJ120_","ASM1SBW16""500LF30K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF30K1CUNVxDTG","ASM1SBW16""500LF30K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF30K1CUNVxDTS","ASM1SBW16""500LF30K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF930K1CUNVxJ24_","ASM1SRL8""100LF930K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF930K1CUNVxJ48_","ASM1SRL8""100LF930K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF930K1CUNVxJ96_","ASM1SRL8""100LF930K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF930K1CUNVxJ120_","ASM1SRL8""100LF930K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF930K1CUNVxDTG","ASM1SRL8""100LF930K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF930K1CUNVxDTS","ASM1SRL8""100LF930K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF930K1CUNVxJ24_","ASM1SRL8""200LF930K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF930K1CUNVxJ48_","ASM1SRL8""200LF930K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF930K1CUNVxJ96_","ASM1SRL8""200LF930K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF930K1CUNVxJ120_","ASM1SRL8""200LF930K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF930K1CUNVxDTG","ASM1SRL8""200LF930K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF930K1CUNVxDTS","ASM1SRL8""200LF930K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF930K1CUNVxJ24_","ASM1SRL8""300LF930K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF930K1CUNVxJ48_","ASM1SRL8""300LF930K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF930K1CUNVxJ96_","ASM1SRL8""300LF930K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF930K1CUNVxJ120_","ASM1SRL8""300LF930K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF930K1CUNVxDTG","ASM1SRL8""300LF930K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF930K1CUNVxDTS","ASM1SRL8""300LF930K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF930K1CUNVxJ24_","ASM1SRL8""400LF930K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF930K1CUNVxJ48_","ASM1SRL8""400LF930K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF930K1CUNVxJ96_","ASM1SRL8""400LF930K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF930K1CUNVxJ120_","ASM1SRL8""400LF930K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF930K1CUNVxDTG","ASM1SRL8""400LF930K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF930K1CUNVxDTS","ASM1SRL8""400LF930K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF930K1CUNVxJ24_","ASM1SRL8""500LF930K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF930K1CUNVxJ48_","ASM1SRL8""500LF930K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF930K1CUNVxJ96_","ASM1SRL8""500LF930K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF930K1CUNVxJ120_","ASM1SRL8""500LF930K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF930K1CUNVxDTG","ASM1SRL8""500LF930K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF930K1CUNVxDTS","ASM1SRL8""500LF930K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF930K1CUNVxJ24_","ASM1SRL12""100LF930K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF930K1CUNVxJ48_","ASM1SRL12""100LF930K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF930K1CUNVxJ96_","ASM1SRL12""100LF930K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF930K1CUNVxJ120_","ASM1SRL12""100LF930K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF930K1CUNVxDTG","ASM1SRL12""100LF930K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF930K1CUNVxDTS","ASM1SRL12""100LF930K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF930K1CUNVxJ24_","ASM1SRL12""200LF930K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF930K1CUNVxJ48_","ASM1SRL12""200LF930K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF930K1CUNVxJ96_","ASM1SRL12""200LF930K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF930K1CUNVxJ120_","ASM1SRL12""200LF930K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF930K1CUNVxDTG","ASM1SRL12""200LF930K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF930K1CUNVxDTS","ASM1SRL12""200LF930K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF930K1CUNVxJ24_","ASM1SRL12""300LF930K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF930K1CUNVxJ48_","ASM1SRL12""300LF930K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF930K1CUNVxJ96_","ASM1SRL12""300LF930K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF930K1CUNVxJ120_","ASM1SRL12""300LF930K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF930K1CUNVxDTG","ASM1SRL12""300LF930K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF930K1CUNVxDTS","ASM1SRL12""300LF930K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF930K1CUNVxJ24_","ASM1SRL12""400LF930K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF930K1CUNVxJ48_","ASM1SRL12""400LF930K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF930K1CUNVxJ96_","ASM1SRL12""400LF930K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF930K1CUNVxJ120_","ASM1SRL12""400LF930K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF930K1CUNVxDTG","ASM1SRL12""400LF930K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF930K1CUNVxDTS","ASM1SRL12""400LF930K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF930K1CUNVxJ24_","ASM1SRL12""500LF930K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF930K1CUNVxJ48_","ASM1SRL12""500LF930K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF930K1CUNVxJ96_","ASM1SRL12""500LF930K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF930K1CUNVxJ120_","ASM1SRL12""500LF930K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF930K1CUNVxDTG","ASM1SRL12""500LF930K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF930K1CUNVxDTS","ASM1SRL12""500LF930K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF930K1CUNVxJ24_","ASM1SRL16""100LF930K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF930K1CUNVxJ48_","ASM1SRL16""100LF930K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF930K1CUNVxJ96_","ASM1SRL16""100LF930K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF930K1CUNVxJ120_","ASM1SRL16""100LF930K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF930K1CUNVxDTG","ASM1SRL16""100LF930K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF930K1CUNVxDTS","ASM1SRL16""100LF930K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF930K1CUNVxJ24_","ASM1SRL16""200LF930K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF930K1CUNVxJ48_","ASM1SRL16""200LF930K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF930K1CUNVxJ96_","ASM1SRL16""200LF930K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF930K1CUNVxJ120_","ASM1SRL16""200LF930K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF930K1CUNVxDTG","ASM1SRL16""200LF930K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF930K1CUNVxDTS","ASM1SRL16""200LF930K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF930K1CUNVxJ24_","ASM1SRL16""300LF930K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF930K1CUNVxJ48_","ASM1SRL16""300LF930K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF930K1CUNVxJ96_","ASM1SRL16""300LF930K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF930K1CUNVxJ120_","ASM1SRL16""300LF930K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF930K1CUNVxDTG","ASM1SRL16""300LF930K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF930K1CUNVxDTS","ASM1SRL16""300LF930K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF930K1CUNVxJ24_","ASM1SRL16""400LF930K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF930K1CUNVxJ48_","ASM1SRL16""400LF930K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF930K1CUNVxJ96_","ASM1SRL16""400LF930K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF930K1CUNVxJ120_","ASM1SRL16""400LF930K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF930K1CUNVxDTG","ASM1SRL16""400LF930K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF930K1CUNVxDTS","ASM1SRL16""400LF930K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF930K1CUNVxJ24_","ASM1SRL16""500LF930K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF930K1CUNVxJ48_","ASM1SRL16""500LF930K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF930K1CUNVxJ96_","ASM1SRL16""500LF930K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF930K1CUNVxJ120_","ASM1SRL16""500LF930K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF930K1CUNVxDTG","ASM1SRL16""500LF930K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF930K1CUNVxDTS","ASM1SRL16""500LF930K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF930K1CUNVxJ24_","ASM1SAS8""100LF930K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF930K1CUNVxJ48_","ASM1SAS8""100LF930K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF930K1CUNVxJ96_","ASM1SAS8""100LF930K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF930K1CUNVxJ120_","ASM1SAS8""100LF930K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF930K1CUNVxDTG","ASM1SAS8""100LF930K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF930K1CUNVxDTS","ASM1SAS8""100LF930K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF930K1CUNVxJ24_","ASM1SAS8""200LF930K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF930K1CUNVxJ48_","ASM1SAS8""200LF930K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF930K1CUNVxJ96_","ASM1SAS8""200LF930K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF930K1CUNVxJ120_","ASM1SAS8""200LF930K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF930K1CUNVxDTG","ASM1SAS8""200LF930K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF930K1CUNVxDTS","ASM1SAS8""200LF930K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF930K1CUNVxJ24_","ASM1SAS8""300LF930K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF930K1CUNVxJ48_","ASM1SAS8""300LF930K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF930K1CUNVxJ96_","ASM1SAS8""300LF930K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF930K1CUNVxJ120_","ASM1SAS8""300LF930K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF930K1CUNVxDTG","ASM1SAS8""300LF930K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF930K1CUNVxDTS","ASM1SAS8""300LF930K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF930K1CUNVxJ24_","ASM1SAS8""400LF930K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF930K1CUNVxJ48_","ASM1SAS8""400LF930K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF930K1CUNVxJ96_","ASM1SAS8""400LF930K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF930K1CUNVxJ120_","ASM1SAS8""400LF930K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF930K1CUNVxDTG","ASM1SAS8""400LF930K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF930K1CUNVxDTS","ASM1SAS8""400LF930K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF930K1CUNVxJ24_","ASM1SAS8""500LF930K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF930K1CUNVxJ48_","ASM1SAS8""500LF930K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF930K1CUNVxJ96_","ASM1SAS8""500LF930K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF930K1CUNVxJ120_","ASM1SAS8""500LF930K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF930K1CUNVxDTG","ASM1SAS8""500LF930K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF930K1CUNVxDTS","ASM1SAS8""500LF930K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF930K1CUNVxJ24_","ASM1SAS12""100LF930K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF930K1CUNVxJ48_","ASM1SAS12""100LF930K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF930K1CUNVxJ96_","ASM1SAS12""100LF930K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF930K1CUNVxJ120_","ASM1SAS12""100LF930K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF930K1CUNVxDTG","ASM1SAS12""100LF930K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF930K1CUNVxDTS","ASM1SAS12""100LF930K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF930K1CUNVxJ24_","ASM1SAS12""200LF930K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF930K1CUNVxJ48_","ASM1SAS12""200LF930K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF930K1CUNVxJ96_","ASM1SAS12""200LF930K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF930K1CUNVxJ120_","ASM1SAS12""200LF930K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF930K1CUNVxDTG","ASM1SAS12""200LF930K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF930K1CUNVxDTS","ASM1SAS12""200LF930K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF930K1CUNVxJ24_","ASM1SAS12""300LF930K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF930K1CUNVxJ48_","ASM1SAS12""300LF930K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF930K1CUNVxJ96_","ASM1SAS12""300LF930K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF930K1CUNVxJ120_","ASM1SAS12""300LF930K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF930K1CUNVxDTG","ASM1SAS12""300LF930K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF930K1CUNVxDTS","ASM1SAS12""300LF930K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF930K1CUNVxJ24_","ASM1SAS12""400LF930K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF930K1CUNVxJ48_","ASM1SAS12""400LF930K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF930K1CUNVxJ96_","ASM1SAS12""400LF930K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF930K1CUNVxJ120_","ASM1SAS12""400LF930K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF930K1CUNVxDTG","ASM1SAS12""400LF930K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF930K1CUNVxDTS","ASM1SAS12""400LF930K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF930K1CUNVxJ24_","ASM1SAS12""500LF930K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF930K1CUNVxJ48_","ASM1SAS12""500LF930K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF930K1CUNVxJ96_","ASM1SAS12""500LF930K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF930K1CUNVxJ120_","ASM1SAS12""500LF930K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF930K1CUNVxDTG","ASM1SAS12""500LF930K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF930K1CUNVxDTS","ASM1SAS12""500LF930K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF930K1CUNVxJ24_","ASM1SAS16""100LF930K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF930K1CUNVxJ48_","ASM1SAS16""100LF930K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF930K1CUNVxJ96_","ASM1SAS16""100LF930K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF930K1CUNVxJ120_","ASM1SAS16""100LF930K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF930K1CUNVxDTG","ASM1SAS16""100LF930K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF930K1CUNVxDTS","ASM1SAS16""100LF930K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF930K1CUNVxJ24_","ASM1SAS16""200LF930K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF930K1CUNVxJ48_","ASM1SAS16""200LF930K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF930K1CUNVxJ96_","ASM1SAS16""200LF930K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF930K1CUNVxJ120_","ASM1SAS16""200LF930K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF930K1CUNVxDTG","ASM1SAS16""200LF930K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF930K1CUNVxDTS","ASM1SAS16""200LF930K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF930K1CUNVxJ24_","ASM1SAS16""300LF930K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF930K1CUNVxJ48_","ASM1SAS16""300LF930K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF930K1CUNVxJ96_","ASM1SAS16""300LF930K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF930K1CUNVxJ120_","ASM1SAS16""300LF930K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF930K1CUNVxDTG","ASM1SAS16""300LF930K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF930K1CUNVxDTS","ASM1SAS16""300LF930K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF930K1CUNVxJ24_","ASM1SAS16""400LF930K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF930K1CUNVxJ48_","ASM1SAS16""400LF930K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF930K1CUNVxJ96_","ASM1SAS16""400LF930K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF930K1CUNVxJ120_","ASM1SAS16""400LF930K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF930K1CUNVxDTG","ASM1SAS16""400LF930K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF930K1CUNVxDTS","ASM1SAS16""400LF930K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF930K1CUNVxJ24_","ASM1SAS16""500LF930K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF930K1CUNVxJ48_","ASM1SAS16""500LF930K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF930K1CUNVxJ96_","ASM1SAS16""500LF930K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF930K1CUNVxJ120_","ASM1SAS16""500LF930K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF930K1CUNVxDTG","ASM1SAS16""500LF930K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF930K1CUNVxDTS","ASM1SAS16""500LF930K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF930K1CUNVxJ24_","ASM1SBW8""100LF930K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF930K1CUNVxJ48_","ASM1SBW8""100LF930K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF930K1CUNVxJ96_","ASM1SBW8""100LF930K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF930K1CUNVxJ120_","ASM1SBW8""100LF930K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF930K1CUNVxDTG","ASM1SBW8""100LF930K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF930K1CUNVxDTS","ASM1SBW8""100LF930K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF930K1CUNVxJ24_","ASM1SBW8""200LF930K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF930K1CUNVxJ48_","ASM1SBW8""200LF930K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF930K1CUNVxJ96_","ASM1SBW8""200LF930K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF930K1CUNVxJ120_","ASM1SBW8""200LF930K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF930K1CUNVxDTG","ASM1SBW8""200LF930K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF930K1CUNVxDTS","ASM1SBW8""200LF930K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF930K1CUNVxJ24_","ASM1SBW8""300LF930K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF930K1CUNVxJ48_","ASM1SBW8""300LF930K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF930K1CUNVxJ96_","ASM1SBW8""300LF930K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF930K1CUNVxJ120_","ASM1SBW8""300LF930K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF930K1CUNVxDTG","ASM1SBW8""300LF930K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF930K1CUNVxDTS","ASM1SBW8""300LF930K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF930K1CUNVxJ24_","ASM1SBW8""400LF930K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF930K1CUNVxJ48_","ASM1SBW8""400LF930K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF930K1CUNVxJ96_","ASM1SBW8""400LF930K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF930K1CUNVxJ120_","ASM1SBW8""400LF930K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF930K1CUNVxDTG","ASM1SBW8""400LF930K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF930K1CUNVxDTS","ASM1SBW8""400LF930K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF930K1CUNVxJ24_","ASM1SBW8""500LF930K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF930K1CUNVxJ48_","ASM1SBW8""500LF930K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF930K1CUNVxJ96_","ASM1SBW8""500LF930K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF930K1CUNVxJ120_","ASM1SBW8""500LF930K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF930K1CUNVxDTG","ASM1SBW8""500LF930K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF930K1CUNVxDTS","ASM1SBW8""500LF930K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF930K1CUNVxJ24_","ASM1SBW12""100LF930K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF930K1CUNVxJ48_","ASM1SBW12""100LF930K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF930K1CUNVxJ96_","ASM1SBW12""100LF930K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF930K1CUNVxJ120_","ASM1SBW12""100LF930K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF930K1CUNVxDTG","ASM1SBW12""100LF930K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF930K1CUNVxDTS","ASM1SBW12""100LF930K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF930K1CUNVxJ24_","ASM1SBW12""200LF930K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF930K1CUNVxJ48_","ASM1SBW12""200LF930K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF930K1CUNVxJ96_","ASM1SBW12""200LF930K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF930K1CUNVxJ120_","ASM1SBW12""200LF930K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF930K1CUNVxDTG","ASM1SBW12""200LF930K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF930K1CUNVxDTS","ASM1SBW12""200LF930K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF930K1CUNVxJ24_","ASM1SBW12""300LF930K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF930K1CUNVxJ48_","ASM1SBW12""300LF930K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF930K1CUNVxJ96_","ASM1SBW12""300LF930K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF930K1CUNVxJ120_","ASM1SBW12""300LF930K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF930K1CUNVxDTG","ASM1SBW12""300LF930K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF930K1CUNVxDTS","ASM1SBW12""300LF930K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF930K1CUNVxJ24_","ASM1SBW12""400LF930K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF930K1CUNVxJ48_","ASM1SBW12""400LF930K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF930K1CUNVxJ96_","ASM1SBW12""400LF930K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF930K1CUNVxJ120_","ASM1SBW12""400LF930K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF930K1CUNVxDTG","ASM1SBW12""400LF930K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF930K1CUNVxDTS","ASM1SBW12""400LF930K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF930K1CUNVxJ24_","ASM1SBW12""500LF930K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF930K1CUNVxJ48_","ASM1SBW12""500LF930K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF930K1CUNVxJ96_","ASM1SBW12""500LF930K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF930K1CUNVxJ120_","ASM1SBW12""500LF930K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF930K1CUNVxDTG","ASM1SBW12""500LF930K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF930K1CUNVxDTS","ASM1SBW12""500LF930K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF930K1CUNVxJ24_","ASM1SBW16""100LF930K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF930K1CUNVxJ48_","ASM1SBW16""100LF930K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF930K1CUNVxJ96_","ASM1SBW16""100LF930K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF930K1CUNVxJ120_","ASM1SBW16""100LF930K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF930K1CUNVxDTG","ASM1SBW16""100LF930K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF930K1CUNVxDTS","ASM1SBW16""100LF930K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF930K1CUNVxJ24_","ASM1SBW16""200LF930K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF930K1CUNVxJ48_","ASM1SBW16""200LF930K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF930K1CUNVxJ96_","ASM1SBW16""200LF930K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF930K1CUNVxJ120_","ASM1SBW16""200LF930K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF930K1CUNVxDTG","ASM1SBW16""200LF930K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF930K1CUNVxDTS","ASM1SBW16""200LF930K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF930K1CUNVxJ24_","ASM1SBW16""300LF930K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF930K1CUNVxJ48_","ASM1SBW16""300LF930K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF930K1CUNVxJ96_","ASM1SBW16""300LF930K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF930K1CUNVxJ120_","ASM1SBW16""300LF930K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF930K1CUNVxDTG","ASM1SBW16""300LF930K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF930K1CUNVxDTS","ASM1SBW16""300LF930K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF930K1CUNVxJ24_","ASM1SBW16""400LF930K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF930K1CUNVxJ48_","ASM1SBW16""400LF930K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF930K1CUNVxJ96_","ASM1SBW16""400LF930K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF930K1CUNVxJ120_","ASM1SBW16""400LF930K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF930K1CUNVxDTG","ASM1SBW16""400LF930K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF930K1CUNVxDTS","ASM1SBW16""400LF930K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF930K1CUNVxJ24_","ASM1SBW16""500LF930K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF930K1CUNVxJ48_","ASM1SBW16""500LF930K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF930K1CUNVxJ96_","ASM1SBW16""500LF930K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF930K1CUNVxJ120_","ASM1SBW16""500LF930K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF930K1CUNVxDTG","ASM1SBW16""500LF930K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF930K1CUNVxDTS","ASM1SBW16""500LF930K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF35K1CUNVxJ24_","ASM1SRL8""100LF35K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF35K1CUNVxJ48_","ASM1SRL8""100LF35K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF35K1CUNVxJ96_","ASM1SRL8""100LF35K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF35K1CUNVxJ120_","ASM1SRL8""100LF35K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF35K1CUNVxDTG","ASM1SRL8""100LF35K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF35K1CUNVxDTS","ASM1SRL8""100LF35K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF35K1CUNVxJ24_","ASM1SRL8""200LF35K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF35K1CUNVxJ48_","ASM1SRL8""200LF35K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF35K1CUNVxJ96_","ASM1SRL8""200LF35K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF35K1CUNVxJ120_","ASM1SRL8""200LF35K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF35K1CUNVxDTG","ASM1SRL8""200LF35K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF35K1CUNVxDTS","ASM1SRL8""200LF35K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF35K1CUNVxJ24_","ASM1SRL8""300LF35K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF35K1CUNVxJ48_","ASM1SRL8""300LF35K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF35K1CUNVxJ96_","ASM1SRL8""300LF35K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF35K1CUNVxJ120_","ASM1SRL8""300LF35K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF35K1CUNVxDTG","ASM1SRL8""300LF35K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF35K1CUNVxDTS","ASM1SRL8""300LF35K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF35K1CUNVxJ24_","ASM1SRL8""400LF35K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF35K1CUNVxJ48_","ASM1SRL8""400LF35K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF35K1CUNVxJ96_","ASM1SRL8""400LF35K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF35K1CUNVxJ120_","ASM1SRL8""400LF35K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF35K1CUNVxDTG","ASM1SRL8""400LF35K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF35K1CUNVxDTS","ASM1SRL8""400LF35K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF35K1CUNVxJ24_","ASM1SRL8""500LF35K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF35K1CUNVxJ48_","ASM1SRL8""500LF35K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF35K1CUNVxJ96_","ASM1SRL8""500LF35K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF35K1CUNVxJ120_","ASM1SRL8""500LF35K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF35K1CUNVxDTG","ASM1SRL8""500LF35K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF35K1CUNVxDTS","ASM1SRL8""500LF35K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF35K1CUNVxJ24_","ASM1SRL12""100LF35K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF35K1CUNVxJ48_","ASM1SRL12""100LF35K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF35K1CUNVxJ96_","ASM1SRL12""100LF35K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF35K1CUNVxJ120_","ASM1SRL12""100LF35K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF35K1CUNVxDTG","ASM1SRL12""100LF35K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF35K1CUNVxDTS","ASM1SRL12""100LF35K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF35K1CUNVxJ24_","ASM1SRL12""200LF35K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF35K1CUNVxJ48_","ASM1SRL12""200LF35K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF35K1CUNVxJ96_","ASM1SRL12""200LF35K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF35K1CUNVxJ120_","ASM1SRL12""200LF35K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF35K1CUNVxDTG","ASM1SRL12""200LF35K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF35K1CUNVxDTS","ASM1SRL12""200LF35K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF35K1CUNVxJ24_","ASM1SRL12""300LF35K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF35K1CUNVxJ48_","ASM1SRL12""300LF35K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF35K1CUNVxJ96_","ASM1SRL12""300LF35K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF35K1CUNVxJ120_","ASM1SRL12""300LF35K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF35K1CUNVxDTG","ASM1SRL12""300LF35K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF35K1CUNVxDTS","ASM1SRL12""300LF35K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF35K1CUNVxJ24_","ASM1SRL12""400LF35K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF35K1CUNVxJ48_","ASM1SRL12""400LF35K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF35K1CUNVxJ96_","ASM1SRL12""400LF35K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF35K1CUNVxJ120_","ASM1SRL12""400LF35K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF35K1CUNVxDTG","ASM1SRL12""400LF35K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF35K1CUNVxDTS","ASM1SRL12""400LF35K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF35K1CUNVxJ24_","ASM1SRL12""500LF35K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF35K1CUNVxJ48_","ASM1SRL12""500LF35K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF35K1CUNVxJ96_","ASM1SRL12""500LF35K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF35K1CUNVxJ120_","ASM1SRL12""500LF35K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF35K1CUNVxDTG","ASM1SRL12""500LF35K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF35K1CUNVxDTS","ASM1SRL12""500LF35K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF35K1CUNVxJ24_","ASM1SRL16""100LF35K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF35K1CUNVxJ48_","ASM1SRL16""100LF35K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF35K1CUNVxJ96_","ASM1SRL16""100LF35K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF35K1CUNVxJ120_","ASM1SRL16""100LF35K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF35K1CUNVxDTG","ASM1SRL16""100LF35K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF35K1CUNVxDTS","ASM1SRL16""100LF35K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF35K1CUNVxJ24_","ASM1SRL16""200LF35K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF35K1CUNVxJ48_","ASM1SRL16""200LF35K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF35K1CUNVxJ96_","ASM1SRL16""200LF35K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF35K1CUNVxJ120_","ASM1SRL16""200LF35K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF35K1CUNVxDTG","ASM1SRL16""200LF35K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF35K1CUNVxDTS","ASM1SRL16""200LF35K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF35K1CUNVxJ24_","ASM1SRL16""300LF35K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF35K1CUNVxJ48_","ASM1SRL16""300LF35K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF35K1CUNVxJ96_","ASM1SRL16""300LF35K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF35K1CUNVxJ120_","ASM1SRL16""300LF35K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF35K1CUNVxDTG","ASM1SRL16""300LF35K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF35K1CUNVxDTS","ASM1SRL16""300LF35K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF35K1CUNVxJ24_","ASM1SRL16""400LF35K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF35K1CUNVxJ48_","ASM1SRL16""400LF35K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF35K1CUNVxJ96_","ASM1SRL16""400LF35K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF35K1CUNVxJ120_","ASM1SRL16""400LF35K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF35K1CUNVxDTG","ASM1SRL16""400LF35K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF35K1CUNVxDTS","ASM1SRL16""400LF35K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF35K1CUNVxJ24_","ASM1SRL16""500LF35K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF35K1CUNVxJ48_","ASM1SRL16""500LF35K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF35K1CUNVxJ96_","ASM1SRL16""500LF35K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF35K1CUNVxJ120_","ASM1SRL16""500LF35K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF35K1CUNVxDTG","ASM1SRL16""500LF35K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF35K1CUNVxDTS","ASM1SRL16""500LF35K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF35K1CUNVxJ24_","ASM1SAS8""100LF35K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF35K1CUNVxJ48_","ASM1SAS8""100LF35K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF35K1CUNVxJ96_","ASM1SAS8""100LF35K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF35K1CUNVxJ120_","ASM1SAS8""100LF35K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF35K1CUNVxDTG","ASM1SAS8""100LF35K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF35K1CUNVxDTS","ASM1SAS8""100LF35K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF35K1CUNVxJ24_","ASM1SAS8""200LF35K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF35K1CUNVxJ48_","ASM1SAS8""200LF35K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF35K1CUNVxJ96_","ASM1SAS8""200LF35K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF35K1CUNVxJ120_","ASM1SAS8""200LF35K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF35K1CUNVxDTG","ASM1SAS8""200LF35K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF35K1CUNVxDTS","ASM1SAS8""200LF35K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF35K1CUNVxJ24_","ASM1SAS8""300LF35K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF35K1CUNVxJ48_","ASM1SAS8""300LF35K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF35K1CUNVxJ96_","ASM1SAS8""300LF35K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF35K1CUNVxJ120_","ASM1SAS8""300LF35K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF35K1CUNVxDTG","ASM1SAS8""300LF35K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF35K1CUNVxDTS","ASM1SAS8""300LF35K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF35K1CUNVxJ24_","ASM1SAS8""400LF35K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF35K1CUNVxJ48_","ASM1SAS8""400LF35K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF35K1CUNVxJ96_","ASM1SAS8""400LF35K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF35K1CUNVxJ120_","ASM1SAS8""400LF35K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF35K1CUNVxDTG","ASM1SAS8""400LF35K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF35K1CUNVxDTS","ASM1SAS8""400LF35K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF35K1CUNVxJ24_","ASM1SAS8""500LF35K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF35K1CUNVxJ48_","ASM1SAS8""500LF35K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF35K1CUNVxJ96_","ASM1SAS8""500LF35K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF35K1CUNVxJ120_","ASM1SAS8""500LF35K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF35K1CUNVxDTG","ASM1SAS8""500LF35K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF35K1CUNVxDTS","ASM1SAS8""500LF35K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF35K1CUNVxJ24_","ASM1SAS12""100LF35K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF35K1CUNVxJ48_","ASM1SAS12""100LF35K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF35K1CUNVxJ96_","ASM1SAS12""100LF35K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF35K1CUNVxJ120_","ASM1SAS12""100LF35K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF35K1CUNVxDTG","ASM1SAS12""100LF35K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF35K1CUNVxDTS","ASM1SAS12""100LF35K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF35K1CUNVxJ24_","ASM1SAS12""200LF35K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF35K1CUNVxJ48_","ASM1SAS12""200LF35K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF35K1CUNVxJ96_","ASM1SAS12""200LF35K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF35K1CUNVxJ120_","ASM1SAS12""200LF35K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF35K1CUNVxDTG","ASM1SAS12""200LF35K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF35K1CUNVxDTS","ASM1SAS12""200LF35K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF35K1CUNVxJ24_","ASM1SAS12""300LF35K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF35K1CUNVxJ48_","ASM1SAS12""300LF35K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF35K1CUNVxJ96_","ASM1SAS12""300LF35K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF35K1CUNVxJ120_","ASM1SAS12""300LF35K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF35K1CUNVxDTG","ASM1SAS12""300LF35K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF35K1CUNVxDTS","ASM1SAS12""300LF35K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF35K1CUNVxJ24_","ASM1SAS12""400LF35K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF35K1CUNVxJ48_","ASM1SAS12""400LF35K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF35K1CUNVxJ96_","ASM1SAS12""400LF35K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF35K1CUNVxJ120_","ASM1SAS12""400LF35K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF35K1CUNVxDTG","ASM1SAS12""400LF35K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF35K1CUNVxDTS","ASM1SAS12""400LF35K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF35K1CUNVxJ24_","ASM1SAS12""500LF35K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF35K1CUNVxJ48_","ASM1SAS12""500LF35K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF35K1CUNVxJ96_","ASM1SAS12""500LF35K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF35K1CUNVxJ120_","ASM1SAS12""500LF35K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF35K1CUNVxDTG","ASM1SAS12""500LF35K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF35K1CUNVxDTS","ASM1SAS12""500LF35K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF35K1CUNVxJ24_","ASM1SAS16""100LF35K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF35K1CUNVxJ48_","ASM1SAS16""100LF35K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF35K1CUNVxJ96_","ASM1SAS16""100LF35K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF35K1CUNVxJ120_","ASM1SAS16""100LF35K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF35K1CUNVxDTG","ASM1SAS16""100LF35K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF35K1CUNVxDTS","ASM1SAS16""100LF35K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF35K1CUNVxJ24_","ASM1SAS16""200LF35K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF35K1CUNVxJ48_","ASM1SAS16""200LF35K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF35K1CUNVxJ96_","ASM1SAS16""200LF35K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF35K1CUNVxJ120_","ASM1SAS16""200LF35K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF35K1CUNVxDTG","ASM1SAS16""200LF35K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF35K1CUNVxDTS","ASM1SAS16""200LF35K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF35K1CUNVxJ24_","ASM1SAS16""300LF35K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF35K1CUNVxJ48_","ASM1SAS16""300LF35K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF35K1CUNVxJ96_","ASM1SAS16""300LF35K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF35K1CUNVxJ120_","ASM1SAS16""300LF35K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF35K1CUNVxDTG","ASM1SAS16""300LF35K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF35K1CUNVxDTS","ASM1SAS16""300LF35K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF35K1CUNVxJ24_","ASM1SAS16""400LF35K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF35K1CUNVxJ48_","ASM1SAS16""400LF35K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF35K1CUNVxJ96_","ASM1SAS16""400LF35K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF35K1CUNVxJ120_","ASM1SAS16""400LF35K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF35K1CUNVxDTG","ASM1SAS16""400LF35K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF35K1CUNVxDTS","ASM1SAS16""400LF35K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF35K1CUNVxJ24_","ASM1SAS16""500LF35K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF35K1CUNVxJ48_","ASM1SAS16""500LF35K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF35K1CUNVxJ96_","ASM1SAS16""500LF35K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF35K1CUNVxJ120_","ASM1SAS16""500LF35K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF35K1CUNVxDTG","ASM1SAS16""500LF35K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF35K1CUNVxDTS","ASM1SAS16""500LF35K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF35K1CUNVxJ24_","ASM1SBW8""100LF35K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF35K1CUNVxJ48_","ASM1SBW8""100LF35K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF35K1CUNVxJ96_","ASM1SBW8""100LF35K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF35K1CUNVxJ120_","ASM1SBW8""100LF35K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF35K1CUNVxDTG","ASM1SBW8""100LF35K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF35K1CUNVxDTS","ASM1SBW8""100LF35K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF35K1CUNVxJ24_","ASM1SBW8""200LF35K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF35K1CUNVxJ48_","ASM1SBW8""200LF35K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF35K1CUNVxJ96_","ASM1SBW8""200LF35K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF35K1CUNVxJ120_","ASM1SBW8""200LF35K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF35K1CUNVxDTG","ASM1SBW8""200LF35K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF35K1CUNVxDTS","ASM1SBW8""200LF35K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF35K1CUNVxJ24_","ASM1SBW8""300LF35K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF35K1CUNVxJ48_","ASM1SBW8""300LF35K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF35K1CUNVxJ96_","ASM1SBW8""300LF35K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF35K1CUNVxJ120_","ASM1SBW8""300LF35K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF35K1CUNVxDTG","ASM1SBW8""300LF35K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF35K1CUNVxDTS","ASM1SBW8""300LF35K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF35K1CUNVxJ24_","ASM1SBW8""400LF35K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF35K1CUNVxJ48_","ASM1SBW8""400LF35K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF35K1CUNVxJ96_","ASM1SBW8""400LF35K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF35K1CUNVxJ120_","ASM1SBW8""400LF35K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF35K1CUNVxDTG","ASM1SBW8""400LF35K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF35K1CUNVxDTS","ASM1SBW8""400LF35K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF35K1CUNVxJ24_","ASM1SBW8""500LF35K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF35K1CUNVxJ48_","ASM1SBW8""500LF35K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF35K1CUNVxJ96_","ASM1SBW8""500LF35K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF35K1CUNVxJ120_","ASM1SBW8""500LF35K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF35K1CUNVxDTG","ASM1SBW8""500LF35K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF35K1CUNVxDTS","ASM1SBW8""500LF35K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF35K1CUNVxJ24_","ASM1SBW12""100LF35K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF35K1CUNVxJ48_","ASM1SBW12""100LF35K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF35K1CUNVxJ96_","ASM1SBW12""100LF35K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF35K1CUNVxJ120_","ASM1SBW12""100LF35K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF35K1CUNVxDTG","ASM1SBW12""100LF35K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF35K1CUNVxDTS","ASM1SBW12""100LF35K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF35K1CUNVxJ24_","ASM1SBW12""200LF35K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF35K1CUNVxJ48_","ASM1SBW12""200LF35K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF35K1CUNVxJ96_","ASM1SBW12""200LF35K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF35K1CUNVxJ120_","ASM1SBW12""200LF35K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF35K1CUNVxDTG","ASM1SBW12""200LF35K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF35K1CUNVxDTS","ASM1SBW12""200LF35K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF35K1CUNVxJ24_","ASM1SBW12""300LF35K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF35K1CUNVxJ48_","ASM1SBW12""300LF35K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF35K1CUNVxJ96_","ASM1SBW12""300LF35K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF35K1CUNVxJ120_","ASM1SBW12""300LF35K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF35K1CUNVxDTG","ASM1SBW12""300LF35K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF35K1CUNVxDTS","ASM1SBW12""300LF35K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF35K1CUNVxJ24_","ASM1SBW12""400LF35K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF35K1CUNVxJ48_","ASM1SBW12""400LF35K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF35K1CUNVxJ96_","ASM1SBW12""400LF35K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF35K1CUNVxJ120_","ASM1SBW12""400LF35K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF35K1CUNVxDTG","ASM1SBW12""400LF35K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF35K1CUNVxDTS","ASM1SBW12""400LF35K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF35K1CUNVxJ24_","ASM1SBW12""500LF35K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF35K1CUNVxJ48_","ASM1SBW12""500LF35K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF35K1CUNVxJ96_","ASM1SBW12""500LF35K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF35K1CUNVxJ120_","ASM1SBW12""500LF35K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF35K1CUNVxDTG","ASM1SBW12""500LF35K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF35K1CUNVxDTS","ASM1SBW12""500LF35K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF35K1CUNVxJ24_","ASM1SBW16""100LF35K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF35K1CUNVxJ48_","ASM1SBW16""100LF35K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF35K1CUNVxJ96_","ASM1SBW16""100LF35K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF35K1CUNVxJ120_","ASM1SBW16""100LF35K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF35K1CUNVxDTG","ASM1SBW16""100LF35K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF35K1CUNVxDTS","ASM1SBW16""100LF35K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF35K1CUNVxJ24_","ASM1SBW16""200LF35K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF35K1CUNVxJ48_","ASM1SBW16""200LF35K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF35K1CUNVxJ96_","ASM1SBW16""200LF35K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF35K1CUNVxJ120_","ASM1SBW16""200LF35K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF35K1CUNVxDTG","ASM1SBW16""200LF35K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF35K1CUNVxDTS","ASM1SBW16""200LF35K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF35K1CUNVxJ24_","ASM1SBW16""300LF35K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF35K1CUNVxJ48_","ASM1SBW16""300LF35K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF35K1CUNVxJ96_","ASM1SBW16""300LF35K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF35K1CUNVxJ120_","ASM1SBW16""300LF35K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF35K1CUNVxDTG","ASM1SBW16""300LF35K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF35K1CUNVxDTS","ASM1SBW16""300LF35K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF35K1CUNVxJ24_","ASM1SBW16""400LF35K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF35K1CUNVxJ48_","ASM1SBW16""400LF35K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF35K1CUNVxJ96_","ASM1SBW16""400LF35K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF35K1CUNVxJ120_","ASM1SBW16""400LF35K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF35K1CUNVxDTG","ASM1SBW16""400LF35K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF35K1CUNVxDTS","ASM1SBW16""400LF35K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF35K1CUNVxJ24_","ASM1SBW16""500LF35K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF35K1CUNVxJ48_","ASM1SBW16""500LF35K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF35K1CUNVxJ96_","ASM1SBW16""500LF35K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF35K1CUNVxJ120_","ASM1SBW16""500LF35K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF35K1CUNVxDTG","ASM1SBW16""500LF35K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF35K1CUNVxDTS","ASM1SBW16""500LF35K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF935K1CUNVxJ24_","ASM1SRL8""100LF935K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF935K1CUNVxJ48_","ASM1SRL8""100LF935K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF935K1CUNVxJ96_","ASM1SRL8""100LF935K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF935K1CUNVxJ120_","ASM1SRL8""100LF935K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF935K1CUNVxDTG","ASM1SRL8""100LF935K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF935K1CUNVxDTS","ASM1SRL8""100LF935K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF935K1CUNVxJ24_","ASM1SRL8""200LF935K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF935K1CUNVxJ48_","ASM1SRL8""200LF935K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF935K1CUNVxJ96_","ASM1SRL8""200LF935K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF935K1CUNVxJ120_","ASM1SRL8""200LF935K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF935K1CUNVxDTG","ASM1SRL8""200LF935K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF935K1CUNVxDTS","ASM1SRL8""200LF935K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF935K1CUNVxJ24_","ASM1SRL8""300LF935K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF935K1CUNVxJ48_","ASM1SRL8""300LF935K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF935K1CUNVxJ96_","ASM1SRL8""300LF935K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF935K1CUNVxJ120_","ASM1SRL8""300LF935K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF935K1CUNVxDTG","ASM1SRL8""300LF935K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF935K1CUNVxDTS","ASM1SRL8""300LF935K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF935K1CUNVxJ24_","ASM1SRL8""400LF935K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF935K1CUNVxJ48_","ASM1SRL8""400LF935K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF935K1CUNVxJ96_","ASM1SRL8""400LF935K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF935K1CUNVxJ120_","ASM1SRL8""400LF935K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF935K1CUNVxDTG","ASM1SRL8""400LF935K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF935K1CUNVxDTS","ASM1SRL8""400LF935K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF935K1CUNVxJ24_","ASM1SRL8""500LF935K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF935K1CUNVxJ48_","ASM1SRL8""500LF935K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF935K1CUNVxJ96_","ASM1SRL8""500LF935K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF935K1CUNVxJ120_","ASM1SRL8""500LF935K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF935K1CUNVxDTG","ASM1SRL8""500LF935K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF935K1CUNVxDTS","ASM1SRL8""500LF935K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF935K1CUNVxJ24_","ASM1SRL12""100LF935K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF935K1CUNVxJ48_","ASM1SRL12""100LF935K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF935K1CUNVxJ96_","ASM1SRL12""100LF935K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF935K1CUNVxJ120_","ASM1SRL12""100LF935K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF935K1CUNVxDTG","ASM1SRL12""100LF935K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF935K1CUNVxDTS","ASM1SRL12""100LF935K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF935K1CUNVxJ24_","ASM1SRL12""200LF935K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF935K1CUNVxJ48_","ASM1SRL12""200LF935K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF935K1CUNVxJ96_","ASM1SRL12""200LF935K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF935K1CUNVxJ120_","ASM1SRL12""200LF935K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF935K1CUNVxDTG","ASM1SRL12""200LF935K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF935K1CUNVxDTS","ASM1SRL12""200LF935K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF935K1CUNVxJ24_","ASM1SRL12""300LF935K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF935K1CUNVxJ48_","ASM1SRL12""300LF935K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF935K1CUNVxJ96_","ASM1SRL12""300LF935K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF935K1CUNVxJ120_","ASM1SRL12""300LF935K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF935K1CUNVxDTG","ASM1SRL12""300LF935K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF935K1CUNVxDTS","ASM1SRL12""300LF935K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF935K1CUNVxJ24_","ASM1SRL12""400LF935K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF935K1CUNVxJ48_","ASM1SRL12""400LF935K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF935K1CUNVxJ96_","ASM1SRL12""400LF935K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF935K1CUNVxJ120_","ASM1SRL12""400LF935K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF935K1CUNVxDTG","ASM1SRL12""400LF935K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF935K1CUNVxDTS","ASM1SRL12""400LF935K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF935K1CUNVxJ24_","ASM1SRL12""500LF935K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF935K1CUNVxJ48_","ASM1SRL12""500LF935K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF935K1CUNVxJ96_","ASM1SRL12""500LF935K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF935K1CUNVxJ120_","ASM1SRL12""500LF935K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF935K1CUNVxDTG","ASM1SRL12""500LF935K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF935K1CUNVxDTS","ASM1SRL12""500LF935K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF935K1CUNVxJ24_","ASM1SRL16""100LF935K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF935K1CUNVxJ48_","ASM1SRL16""100LF935K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF935K1CUNVxJ96_","ASM1SRL16""100LF935K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF935K1CUNVxJ120_","ASM1SRL16""100LF935K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF935K1CUNVxDTG","ASM1SRL16""100LF935K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF935K1CUNVxDTS","ASM1SRL16""100LF935K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF935K1CUNVxJ24_","ASM1SRL16""200LF935K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF935K1CUNVxJ48_","ASM1SRL16""200LF935K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF935K1CUNVxJ96_","ASM1SRL16""200LF935K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF935K1CUNVxJ120_","ASM1SRL16""200LF935K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF935K1CUNVxDTG","ASM1SRL16""200LF935K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF935K1CUNVxDTS","ASM1SRL16""200LF935K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF935K1CUNVxJ24_","ASM1SRL16""300LF935K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF935K1CUNVxJ48_","ASM1SRL16""300LF935K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF935K1CUNVxJ96_","ASM1SRL16""300LF935K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF935K1CUNVxJ120_","ASM1SRL16""300LF935K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF935K1CUNVxDTG","ASM1SRL16""300LF935K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF935K1CUNVxDTS","ASM1SRL16""300LF935K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF935K1CUNVxJ24_","ASM1SRL16""400LF935K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF935K1CUNVxJ48_","ASM1SRL16""400LF935K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF935K1CUNVxJ96_","ASM1SRL16""400LF935K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF935K1CUNVxJ120_","ASM1SRL16""400LF935K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF935K1CUNVxDTG","ASM1SRL16""400LF935K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF935K1CUNVxDTS","ASM1SRL16""400LF935K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF935K1CUNVxJ24_","ASM1SRL16""500LF935K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF935K1CUNVxJ48_","ASM1SRL16""500LF935K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF935K1CUNVxJ96_","ASM1SRL16""500LF935K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF935K1CUNVxJ120_","ASM1SRL16""500LF935K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF935K1CUNVxDTG","ASM1SRL16""500LF935K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF935K1CUNVxDTS","ASM1SRL16""500LF935K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF935K1CUNVxJ24_","ASM1SAS8""100LF935K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF935K1CUNVxJ48_","ASM1SAS8""100LF935K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF935K1CUNVxJ96_","ASM1SAS8""100LF935K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF935K1CUNVxJ120_","ASM1SAS8""100LF935K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF935K1CUNVxDTG","ASM1SAS8""100LF935K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF935K1CUNVxDTS","ASM1SAS8""100LF935K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF935K1CUNVxJ24_","ASM1SAS8""200LF935K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF935K1CUNVxJ48_","ASM1SAS8""200LF935K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF935K1CUNVxJ96_","ASM1SAS8""200LF935K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF935K1CUNVxJ120_","ASM1SAS8""200LF935K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF935K1CUNVxDTG","ASM1SAS8""200LF935K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF935K1CUNVxDTS","ASM1SAS8""200LF935K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF935K1CUNVxJ24_","ASM1SAS8""300LF935K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF935K1CUNVxJ48_","ASM1SAS8""300LF935K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF935K1CUNVxJ96_","ASM1SAS8""300LF935K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF935K1CUNVxJ120_","ASM1SAS8""300LF935K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF935K1CUNVxDTG","ASM1SAS8""300LF935K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF935K1CUNVxDTS","ASM1SAS8""300LF935K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF935K1CUNVxJ24_","ASM1SAS8""400LF935K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF935K1CUNVxJ48_","ASM1SAS8""400LF935K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF935K1CUNVxJ96_","ASM1SAS8""400LF935K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF935K1CUNVxJ120_","ASM1SAS8""400LF935K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF935K1CUNVxDTG","ASM1SAS8""400LF935K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF935K1CUNVxDTS","ASM1SAS8""400LF935K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF935K1CUNVxJ24_","ASM1SAS8""500LF935K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF935K1CUNVxJ48_","ASM1SAS8""500LF935K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF935K1CUNVxJ96_","ASM1SAS8""500LF935K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF935K1CUNVxJ120_","ASM1SAS8""500LF935K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF935K1CUNVxDTG","ASM1SAS8""500LF935K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF935K1CUNVxDTS","ASM1SAS8""500LF935K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF935K1CUNVxJ24_","ASM1SAS12""100LF935K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF935K1CUNVxJ48_","ASM1SAS12""100LF935K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF935K1CUNVxJ96_","ASM1SAS12""100LF935K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF935K1CUNVxJ120_","ASM1SAS12""100LF935K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF935K1CUNVxDTG","ASM1SAS12""100LF935K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF935K1CUNVxDTS","ASM1SAS12""100LF935K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF935K1CUNVxJ24_","ASM1SAS12""200LF935K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF935K1CUNVxJ48_","ASM1SAS12""200LF935K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF935K1CUNVxJ96_","ASM1SAS12""200LF935K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF935K1CUNVxJ120_","ASM1SAS12""200LF935K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF935K1CUNVxDTG","ASM1SAS12""200LF935K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF935K1CUNVxDTS","ASM1SAS12""200LF935K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF935K1CUNVxJ24_","ASM1SAS12""300LF935K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF935K1CUNVxJ48_","ASM1SAS12""300LF935K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF935K1CUNVxJ96_","ASM1SAS12""300LF935K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF935K1CUNVxJ120_","ASM1SAS12""300LF935K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF935K1CUNVxDTG","ASM1SAS12""300LF935K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF935K1CUNVxDTS","ASM1SAS12""300LF935K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF935K1CUNVxJ24_","ASM1SAS12""400LF935K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF935K1CUNVxJ48_","ASM1SAS12""400LF935K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF935K1CUNVxJ96_","ASM1SAS12""400LF935K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF935K1CUNVxJ120_","ASM1SAS12""400LF935K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF935K1CUNVxDTG","ASM1SAS12""400LF935K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF935K1CUNVxDTS","ASM1SAS12""400LF935K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF935K1CUNVxJ24_","ASM1SAS12""500LF935K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF935K1CUNVxJ48_","ASM1SAS12""500LF935K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF935K1CUNVxJ96_","ASM1SAS12""500LF935K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF935K1CUNVxJ120_","ASM1SAS12""500LF935K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF935K1CUNVxDTG","ASM1SAS12""500LF935K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF935K1CUNVxDTS","ASM1SAS12""500LF935K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF935K1CUNVxJ24_","ASM1SAS16""100LF935K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF935K1CUNVxJ48_","ASM1SAS16""100LF935K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF935K1CUNVxJ96_","ASM1SAS16""100LF935K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF935K1CUNVxJ120_","ASM1SAS16""100LF935K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF935K1CUNVxDTG","ASM1SAS16""100LF935K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF935K1CUNVxDTS","ASM1SAS16""100LF935K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF935K1CUNVxJ24_","ASM1SAS16""200LF935K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF935K1CUNVxJ48_","ASM1SAS16""200LF935K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF935K1CUNVxJ96_","ASM1SAS16""200LF935K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF935K1CUNVxJ120_","ASM1SAS16""200LF935K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF935K1CUNVxDTG","ASM1SAS16""200LF935K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF935K1CUNVxDTS","ASM1SAS16""200LF935K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF935K1CUNVxJ24_","ASM1SAS16""300LF935K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF935K1CUNVxJ48_","ASM1SAS16""300LF935K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF935K1CUNVxJ96_","ASM1SAS16""300LF935K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF935K1CUNVxJ120_","ASM1SAS16""300LF935K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF935K1CUNVxDTG","ASM1SAS16""300LF935K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF935K1CUNVxDTS","ASM1SAS16""300LF935K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF935K1CUNVxJ24_","ASM1SAS16""400LF935K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF935K1CUNVxJ48_","ASM1SAS16""400LF935K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF935K1CUNVxJ96_","ASM1SAS16""400LF935K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF935K1CUNVxJ120_","ASM1SAS16""400LF935K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF935K1CUNVxDTG","ASM1SAS16""400LF935K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF935K1CUNVxDTS","ASM1SAS16""400LF935K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF935K1CUNVxJ24_","ASM1SAS16""500LF935K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF935K1CUNVxJ48_","ASM1SAS16""500LF935K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF935K1CUNVxJ96_","ASM1SAS16""500LF935K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF935K1CUNVxJ120_","ASM1SAS16""500LF935K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF935K1CUNVxDTG","ASM1SAS16""500LF935K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF935K1CUNVxDTS","ASM1SAS16""500LF935K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF935K1CUNVxJ24_","ASM1SBW8""100LF935K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF935K1CUNVxJ48_","ASM1SBW8""100LF935K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF935K1CUNVxJ96_","ASM1SBW8""100LF935K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF935K1CUNVxJ120_","ASM1SBW8""100LF935K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF935K1CUNVxDTG","ASM1SBW8""100LF935K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF935K1CUNVxDTS","ASM1SBW8""100LF935K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF935K1CUNVxJ24_","ASM1SBW8""200LF935K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF935K1CUNVxJ48_","ASM1SBW8""200LF935K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF935K1CUNVxJ96_","ASM1SBW8""200LF935K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF935K1CUNVxJ120_","ASM1SBW8""200LF935K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF935K1CUNVxDTG","ASM1SBW8""200LF935K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF935K1CUNVxDTS","ASM1SBW8""200LF935K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF935K1CUNVxJ24_","ASM1SBW8""300LF935K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF935K1CUNVxJ48_","ASM1SBW8""300LF935K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF935K1CUNVxJ96_","ASM1SBW8""300LF935K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF935K1CUNVxJ120_","ASM1SBW8""300LF935K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF935K1CUNVxDTG","ASM1SBW8""300LF935K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF935K1CUNVxDTS","ASM1SBW8""300LF935K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF935K1CUNVxJ24_","ASM1SBW8""400LF935K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF935K1CUNVxJ48_","ASM1SBW8""400LF935K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF935K1CUNVxJ96_","ASM1SBW8""400LF935K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF935K1CUNVxJ120_","ASM1SBW8""400LF935K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF935K1CUNVxDTG","ASM1SBW8""400LF935K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF935K1CUNVxDTS","ASM1SBW8""400LF935K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF935K1CUNVxJ24_","ASM1SBW8""500LF935K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF935K1CUNVxJ48_","ASM1SBW8""500LF935K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF935K1CUNVxJ96_","ASM1SBW8""500LF935K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF935K1CUNVxJ120_","ASM1SBW8""500LF935K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF935K1CUNVxDTG","ASM1SBW8""500LF935K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF935K1CUNVxDTS","ASM1SBW8""500LF935K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF935K1CUNVxJ24_","ASM1SBW12""100LF935K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF935K1CUNVxJ48_","ASM1SBW12""100LF935K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF935K1CUNVxJ96_","ASM1SBW12""100LF935K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF935K1CUNVxJ120_","ASM1SBW12""100LF935K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF935K1CUNVxDTG","ASM1SBW12""100LF935K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF935K1CUNVxDTS","ASM1SBW12""100LF935K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF935K1CUNVxJ24_","ASM1SBW12""200LF935K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF935K1CUNVxJ48_","ASM1SBW12""200LF935K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF935K1CUNVxJ96_","ASM1SBW12""200LF935K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF935K1CUNVxJ120_","ASM1SBW12""200LF935K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF935K1CUNVxDTG","ASM1SBW12""200LF935K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF935K1CUNVxDTS","ASM1SBW12""200LF935K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF935K1CUNVxJ24_","ASM1SBW12""300LF935K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF935K1CUNVxJ48_","ASM1SBW12""300LF935K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF935K1CUNVxJ96_","ASM1SBW12""300LF935K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF935K1CUNVxJ120_","ASM1SBW12""300LF935K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF935K1CUNVxDTG","ASM1SBW12""300LF935K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF935K1CUNVxDTS","ASM1SBW12""300LF935K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF935K1CUNVxJ24_","ASM1SBW12""400LF935K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF935K1CUNVxJ48_","ASM1SBW12""400LF935K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF935K1CUNVxJ96_","ASM1SBW12""400LF935K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF935K1CUNVxJ120_","ASM1SBW12""400LF935K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF935K1CUNVxDTG","ASM1SBW12""400LF935K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF935K1CUNVxDTS","ASM1SBW12""400LF935K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF935K1CUNVxJ24_","ASM1SBW12""500LF935K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF935K1CUNVxJ48_","ASM1SBW12""500LF935K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF935K1CUNVxJ96_","ASM1SBW12""500LF935K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF935K1CUNVxJ120_","ASM1SBW12""500LF935K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF935K1CUNVxDTG","ASM1SBW12""500LF935K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF935K1CUNVxDTS","ASM1SBW12""500LF935K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF935K1CUNVxJ24_","ASM1SBW16""100LF935K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF935K1CUNVxJ48_","ASM1SBW16""100LF935K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF935K1CUNVxJ96_","ASM1SBW16""100LF935K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF935K1CUNVxJ120_","ASM1SBW16""100LF935K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF935K1CUNVxDTG","ASM1SBW16""100LF935K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF935K1CUNVxDTS","ASM1SBW16""100LF935K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF935K1CUNVxJ24_","ASM1SBW16""200LF935K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF935K1CUNVxJ48_","ASM1SBW16""200LF935K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF935K1CUNVxJ96_","ASM1SBW16""200LF935K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF935K1CUNVxJ120_","ASM1SBW16""200LF935K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF935K1CUNVxDTG","ASM1SBW16""200LF935K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF935K1CUNVxDTS","ASM1SBW16""200LF935K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF935K1CUNVxJ24_","ASM1SBW16""300LF935K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF935K1CUNVxJ48_","ASM1SBW16""300LF935K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF935K1CUNVxJ96_","ASM1SBW16""300LF935K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF935K1CUNVxJ120_","ASM1SBW16""300LF935K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF935K1CUNVxDTG","ASM1SBW16""300LF935K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF935K1CUNVxDTS","ASM1SBW16""300LF935K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF935K1CUNVxJ24_","ASM1SBW16""400LF935K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF935K1CUNVxJ48_","ASM1SBW16""400LF935K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF935K1CUNVxJ96_","ASM1SBW16""400LF935K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF935K1CUNVxJ120_","ASM1SBW16""400LF935K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF935K1CUNVxDTG","ASM1SBW16""400LF935K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF935K1CUNVxDTS","ASM1SBW16""400LF935K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF935K1CUNVxJ24_","ASM1SBW16""500LF935K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF935K1CUNVxJ48_","ASM1SBW16""500LF935K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF935K1CUNVxJ96_","ASM1SBW16""500LF935K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF935K1CUNVxJ120_","ASM1SBW16""500LF935K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF935K1CUNVxDTG","ASM1SBW16""500LF935K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF935K1CUNVxDTS","ASM1SBW16""500LF935K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF40K1CUNVxJ24_","ASM1SRL8""100LF40K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF40K1CUNVxJ48_","ASM1SRL8""100LF40K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF40K1CUNVxJ96_","ASM1SRL8""100LF40K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF40K1CUNVxJ120_","ASM1SRL8""100LF40K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF40K1CUNVxDTG","ASM1SRL8""100LF40K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF40K1CUNVxDTS","ASM1SRL8""100LF40K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF40K1CUNVxJ24_","ASM1SRL8""200LF40K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF40K1CUNVxJ48_","ASM1SRL8""200LF40K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF40K1CUNVxJ96_","ASM1SRL8""200LF40K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF40K1CUNVxJ120_","ASM1SRL8""200LF40K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF40K1CUNVxDTG","ASM1SRL8""200LF40K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF40K1CUNVxDTS","ASM1SRL8""200LF40K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF40K1CUNVxJ24_","ASM1SRL8""300LF40K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF40K1CUNVxJ48_","ASM1SRL8""300LF40K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF40K1CUNVxJ96_","ASM1SRL8""300LF40K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF40K1CUNVxJ120_","ASM1SRL8""300LF40K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF40K1CUNVxDTG","ASM1SRL8""300LF40K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF40K1CUNVxDTS","ASM1SRL8""300LF40K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF40K1CUNVxJ24_","ASM1SRL8""400LF40K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF40K1CUNVxJ48_","ASM1SRL8""400LF40K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF40K1CUNVxJ96_","ASM1SRL8""400LF40K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF40K1CUNVxJ120_","ASM1SRL8""400LF40K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF40K1CUNVxDTG","ASM1SRL8""400LF40K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF40K1CUNVxDTS","ASM1SRL8""400LF40K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF40K1CUNVxJ24_","ASM1SRL8""500LF40K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF40K1CUNVxJ48_","ASM1SRL8""500LF40K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF40K1CUNVxJ96_","ASM1SRL8""500LF40K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF40K1CUNVxJ120_","ASM1SRL8""500LF40K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF40K1CUNVxDTG","ASM1SRL8""500LF40K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF40K1CUNVxDTS","ASM1SRL8""500LF40K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF40K1CUNVxJ24_","ASM1SRL12""100LF40K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF40K1CUNVxJ48_","ASM1SRL12""100LF40K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF40K1CUNVxJ96_","ASM1SRL12""100LF40K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF40K1CUNVxJ120_","ASM1SRL12""100LF40K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF40K1CUNVxDTG","ASM1SRL12""100LF40K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF40K1CUNVxDTS","ASM1SRL12""100LF40K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF40K1CUNVxJ24_","ASM1SRL12""200LF40K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF40K1CUNVxJ48_","ASM1SRL12""200LF40K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF40K1CUNVxJ96_","ASM1SRL12""200LF40K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF40K1CUNVxJ120_","ASM1SRL12""200LF40K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF40K1CUNVxDTG","ASM1SRL12""200LF40K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF40K1CUNVxDTS","ASM1SRL12""200LF40K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF40K1CUNVxJ24_","ASM1SRL12""300LF40K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF40K1CUNVxJ48_","ASM1SRL12""300LF40K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF40K1CUNVxJ96_","ASM1SRL12""300LF40K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF40K1CUNVxJ120_","ASM1SRL12""300LF40K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF40K1CUNVxDTG","ASM1SRL12""300LF40K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF40K1CUNVxDTS","ASM1SRL12""300LF40K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF40K1CUNVxJ24_","ASM1SRL12""400LF40K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF40K1CUNVxJ48_","ASM1SRL12""400LF40K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF40K1CUNVxJ96_","ASM1SRL12""400LF40K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF40K1CUNVxJ120_","ASM1SRL12""400LF40K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF40K1CUNVxDTG","ASM1SRL12""400LF40K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF40K1CUNVxDTS","ASM1SRL12""400LF40K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF40K1CUNVxJ24_","ASM1SRL12""500LF40K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF40K1CUNVxJ48_","ASM1SRL12""500LF40K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF40K1CUNVxJ96_","ASM1SRL12""500LF40K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF40K1CUNVxJ120_","ASM1SRL12""500LF40K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF40K1CUNVxDTG","ASM1SRL12""500LF40K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF40K1CUNVxDTS","ASM1SRL12""500LF40K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF40K1CUNVxJ24_","ASM1SRL16""100LF40K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF40K1CUNVxJ48_","ASM1SRL16""100LF40K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF40K1CUNVxJ96_","ASM1SRL16""100LF40K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF40K1CUNVxJ120_","ASM1SRL16""100LF40K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF40K1CUNVxDTG","ASM1SRL16""100LF40K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF40K1CUNVxDTS","ASM1SRL16""100LF40K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF40K1CUNVxJ24_","ASM1SRL16""200LF40K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF40K1CUNVxJ48_","ASM1SRL16""200LF40K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF40K1CUNVxJ96_","ASM1SRL16""200LF40K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF40K1CUNVxJ120_","ASM1SRL16""200LF40K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF40K1CUNVxDTG","ASM1SRL16""200LF40K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF40K1CUNVxDTS","ASM1SRL16""200LF40K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF40K1CUNVxJ24_","ASM1SRL16""300LF40K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF40K1CUNVxJ48_","ASM1SRL16""300LF40K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF40K1CUNVxJ96_","ASM1SRL16""300LF40K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF40K1CUNVxJ120_","ASM1SRL16""300LF40K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF40K1CUNVxDTG","ASM1SRL16""300LF40K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF40K1CUNVxDTS","ASM1SRL16""300LF40K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF40K1CUNVxJ24_","ASM1SRL16""400LF40K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF40K1CUNVxJ48_","ASM1SRL16""400LF40K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF40K1CUNVxJ96_","ASM1SRL16""400LF40K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF40K1CUNVxJ120_","ASM1SRL16""400LF40K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF40K1CUNVxDTG","ASM1SRL16""400LF40K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF40K1CUNVxDTS","ASM1SRL16""400LF40K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF40K1CUNVxJ24_","ASM1SRL16""500LF40K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF40K1CUNVxJ48_","ASM1SRL16""500LF40K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF40K1CUNVxJ96_","ASM1SRL16""500LF40K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF40K1CUNVxJ120_","ASM1SRL16""500LF40K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF40K1CUNVxDTG","ASM1SRL16""500LF40K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF40K1CUNVxDTS","ASM1SRL16""500LF40K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF40K1CUNVxJ24_","ASM1SAS8""100LF40K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF40K1CUNVxJ48_","ASM1SAS8""100LF40K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF40K1CUNVxJ96_","ASM1SAS8""100LF40K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF40K1CUNVxJ120_","ASM1SAS8""100LF40K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF40K1CUNVxDTG","ASM1SAS8""100LF40K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF40K1CUNVxDTS","ASM1SAS8""100LF40K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF40K1CUNVxJ24_","ASM1SAS8""200LF40K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF40K1CUNVxJ48_","ASM1SAS8""200LF40K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF40K1CUNVxJ96_","ASM1SAS8""200LF40K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF40K1CUNVxJ120_","ASM1SAS8""200LF40K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF40K1CUNVxDTG","ASM1SAS8""200LF40K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF40K1CUNVxDTS","ASM1SAS8""200LF40K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF40K1CUNVxJ24_","ASM1SAS8""300LF40K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF40K1CUNVxJ48_","ASM1SAS8""300LF40K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF40K1CUNVxJ96_","ASM1SAS8""300LF40K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF40K1CUNVxJ120_","ASM1SAS8""300LF40K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF40K1CUNVxDTG","ASM1SAS8""300LF40K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF40K1CUNVxDTS","ASM1SAS8""300LF40K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF40K1CUNVxJ24_","ASM1SAS8""400LF40K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF40K1CUNVxJ48_","ASM1SAS8""400LF40K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF40K1CUNVxJ96_","ASM1SAS8""400LF40K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF40K1CUNVxJ120_","ASM1SAS8""400LF40K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF40K1CUNVxDTG","ASM1SAS8""400LF40K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF40K1CUNVxDTS","ASM1SAS8""400LF40K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF40K1CUNVxJ24_","ASM1SAS8""500LF40K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF40K1CUNVxJ48_","ASM1SAS8""500LF40K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF40K1CUNVxJ96_","ASM1SAS8""500LF40K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF40K1CUNVxJ120_","ASM1SAS8""500LF40K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF40K1CUNVxDTG","ASM1SAS8""500LF40K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF40K1CUNVxDTS","ASM1SAS8""500LF40K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF40K1CUNVxJ24_","ASM1SAS12""100LF40K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF40K1CUNVxJ48_","ASM1SAS12""100LF40K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF40K1CUNVxJ96_","ASM1SAS12""100LF40K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF40K1CUNVxJ120_","ASM1SAS12""100LF40K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF40K1CUNVxDTG","ASM1SAS12""100LF40K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF40K1CUNVxDTS","ASM1SAS12""100LF40K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF40K1CUNVxJ24_","ASM1SAS12""200LF40K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF40K1CUNVxJ48_","ASM1SAS12""200LF40K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF40K1CUNVxJ96_","ASM1SAS12""200LF40K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF40K1CUNVxJ120_","ASM1SAS12""200LF40K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF40K1CUNVxDTG","ASM1SAS12""200LF40K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF40K1CUNVxDTS","ASM1SAS12""200LF40K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF40K1CUNVxJ24_","ASM1SAS12""300LF40K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF40K1CUNVxJ48_","ASM1SAS12""300LF40K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF40K1CUNVxJ96_","ASM1SAS12""300LF40K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF40K1CUNVxJ120_","ASM1SAS12""300LF40K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF40K1CUNVxDTG","ASM1SAS12""300LF40K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF40K1CUNVxDTS","ASM1SAS12""300LF40K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF40K1CUNVxJ24_","ASM1SAS12""400LF40K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF40K1CUNVxJ48_","ASM1SAS12""400LF40K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF40K1CUNVxJ96_","ASM1SAS12""400LF40K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF40K1CUNVxJ120_","ASM1SAS12""400LF40K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF40K1CUNVxDTG","ASM1SAS12""400LF40K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF40K1CUNVxDTS","ASM1SAS12""400LF40K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF40K1CUNVxJ24_","ASM1SAS12""500LF40K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF40K1CUNVxJ48_","ASM1SAS12""500LF40K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF40K1CUNVxJ96_","ASM1SAS12""500LF40K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF40K1CUNVxJ120_","ASM1SAS12""500LF40K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF40K1CUNVxDTG","ASM1SAS12""500LF40K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF40K1CUNVxDTS","ASM1SAS12""500LF40K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF40K1CUNVxJ24_","ASM1SAS16""100LF40K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF40K1CUNVxJ48_","ASM1SAS16""100LF40K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF40K1CUNVxJ96_","ASM1SAS16""100LF40K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF40K1CUNVxJ120_","ASM1SAS16""100LF40K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF40K1CUNVxDTG","ASM1SAS16""100LF40K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF40K1CUNVxDTS","ASM1SAS16""100LF40K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF40K1CUNVxJ24_","ASM1SAS16""200LF40K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF40K1CUNVxJ48_","ASM1SAS16""200LF40K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF40K1CUNVxJ96_","ASM1SAS16""200LF40K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF40K1CUNVxJ120_","ASM1SAS16""200LF40K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF40K1CUNVxDTG","ASM1SAS16""200LF40K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF40K1CUNVxDTS","ASM1SAS16""200LF40K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF40K1CUNVxJ24_","ASM1SAS16""300LF40K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF40K1CUNVxJ48_","ASM1SAS16""300LF40K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF40K1CUNVxJ96_","ASM1SAS16""300LF40K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF40K1CUNVxJ120_","ASM1SAS16""300LF40K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF40K1CUNVxDTG","ASM1SAS16""300LF40K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF40K1CUNVxDTS","ASM1SAS16""300LF40K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF40K1CUNVxJ24_","ASM1SAS16""400LF40K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF40K1CUNVxJ48_","ASM1SAS16""400LF40K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF40K1CUNVxJ96_","ASM1SAS16""400LF40K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF40K1CUNVxJ120_","ASM1SAS16""400LF40K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF40K1CUNVxDTG","ASM1SAS16""400LF40K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF40K1CUNVxDTS","ASM1SAS16""400LF40K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF40K1CUNVxJ24_","ASM1SAS16""500LF40K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF40K1CUNVxJ48_","ASM1SAS16""500LF40K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF40K1CUNVxJ96_","ASM1SAS16""500LF40K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF40K1CUNVxJ120_","ASM1SAS16""500LF40K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF40K1CUNVxDTG","ASM1SAS16""500LF40K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF40K1CUNVxDTS","ASM1SAS16""500LF40K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF40K1CUNVxJ24_","ASM1SBW8""100LF40K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF40K1CUNVxJ48_","ASM1SBW8""100LF40K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF40K1CUNVxJ96_","ASM1SBW8""100LF40K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF40K1CUNVxJ120_","ASM1SBW8""100LF40K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF40K1CUNVxDTG","ASM1SBW8""100LF40K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF40K1CUNVxDTS","ASM1SBW8""100LF40K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF40K1CUNVxJ24_","ASM1SBW8""200LF40K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF40K1CUNVxJ48_","ASM1SBW8""200LF40K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF40K1CUNVxJ96_","ASM1SBW8""200LF40K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF40K1CUNVxJ120_","ASM1SBW8""200LF40K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF40K1CUNVxDTG","ASM1SBW8""200LF40K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF40K1CUNVxDTS","ASM1SBW8""200LF40K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF40K1CUNVxJ24_","ASM1SBW8""300LF40K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF40K1CUNVxJ48_","ASM1SBW8""300LF40K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF40K1CUNVxJ96_","ASM1SBW8""300LF40K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF40K1CUNVxJ120_","ASM1SBW8""300LF40K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF40K1CUNVxDTG","ASM1SBW8""300LF40K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF40K1CUNVxDTS","ASM1SBW8""300LF40K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF40K1CUNVxJ24_","ASM1SBW8""400LF40K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF40K1CUNVxJ48_","ASM1SBW8""400LF40K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF40K1CUNVxJ96_","ASM1SBW8""400LF40K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF40K1CUNVxJ120_","ASM1SBW8""400LF40K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF40K1CUNVxDTG","ASM1SBW8""400LF40K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF40K1CUNVxDTS","ASM1SBW8""400LF40K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF40K1CUNVxJ24_","ASM1SBW8""500LF40K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF40K1CUNVxJ48_","ASM1SBW8""500LF40K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF40K1CUNVxJ96_","ASM1SBW8""500LF40K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF40K1CUNVxJ120_","ASM1SBW8""500LF40K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF40K1CUNVxDTG","ASM1SBW8""500LF40K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF40K1CUNVxDTS","ASM1SBW8""500LF40K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF40K1CUNVxJ24_","ASM1SBW12""100LF40K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF40K1CUNVxJ48_","ASM1SBW12""100LF40K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF40K1CUNVxJ96_","ASM1SBW12""100LF40K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF40K1CUNVxJ120_","ASM1SBW12""100LF40K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF40K1CUNVxDTG","ASM1SBW12""100LF40K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF40K1CUNVxDTS","ASM1SBW12""100LF40K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF40K1CUNVxJ24_","ASM1SBW12""200LF40K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF40K1CUNVxJ48_","ASM1SBW12""200LF40K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF40K1CUNVxJ96_","ASM1SBW12""200LF40K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF40K1CUNVxJ120_","ASM1SBW12""200LF40K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF40K1CUNVxDTG","ASM1SBW12""200LF40K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF40K1CUNVxDTS","ASM1SBW12""200LF40K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF40K1CUNVxJ24_","ASM1SBW12""300LF40K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF40K1CUNVxJ48_","ASM1SBW12""300LF40K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF40K1CUNVxJ96_","ASM1SBW12""300LF40K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF40K1CUNVxJ120_","ASM1SBW12""300LF40K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF40K1CUNVxDTG","ASM1SBW12""300LF40K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF40K1CUNVxDTS","ASM1SBW12""300LF40K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF40K1CUNVxJ24_","ASM1SBW12""400LF40K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF40K1CUNVxJ48_","ASM1SBW12""400LF40K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF40K1CUNVxJ96_","ASM1SBW12""400LF40K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF40K1CUNVxJ120_","ASM1SBW12""400LF40K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF40K1CUNVxDTG","ASM1SBW12""400LF40K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF40K1CUNVxDTS","ASM1SBW12""400LF40K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF40K1CUNVxJ24_","ASM1SBW12""500LF40K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF40K1CUNVxJ48_","ASM1SBW12""500LF40K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF40K1CUNVxJ96_","ASM1SBW12""500LF40K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF40K1CUNVxJ120_","ASM1SBW12""500LF40K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF40K1CUNVxDTG","ASM1SBW12""500LF40K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF40K1CUNVxDTS","ASM1SBW12""500LF40K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF40K1CUNVxJ24_","ASM1SBW16""100LF40K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF40K1CUNVxJ48_","ASM1SBW16""100LF40K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF40K1CUNVxJ96_","ASM1SBW16""100LF40K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF40K1CUNVxJ120_","ASM1SBW16""100LF40K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF40K1CUNVxDTG","ASM1SBW16""100LF40K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF40K1CUNVxDTS","ASM1SBW16""100LF40K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF40K1CUNVxJ24_","ASM1SBW16""200LF40K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF40K1CUNVxJ48_","ASM1SBW16""200LF40K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF40K1CUNVxJ96_","ASM1SBW16""200LF40K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF40K1CUNVxJ120_","ASM1SBW16""200LF40K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF40K1CUNVxDTG","ASM1SBW16""200LF40K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF40K1CUNVxDTS","ASM1SBW16""200LF40K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF40K1CUNVxJ24_","ASM1SBW16""300LF40K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF40K1CUNVxJ48_","ASM1SBW16""300LF40K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF40K1CUNVxJ96_","ASM1SBW16""300LF40K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF40K1CUNVxJ120_","ASM1SBW16""300LF40K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF40K1CUNVxDTG","ASM1SBW16""300LF40K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF40K1CUNVxDTS","ASM1SBW16""300LF40K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF40K1CUNVxJ24_","ASM1SBW16""400LF40K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF40K1CUNVxJ48_","ASM1SBW16""400LF40K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF40K1CUNVxJ96_","ASM1SBW16""400LF40K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF40K1CUNVxJ120_","ASM1SBW16""400LF40K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF40K1CUNVxDTG","ASM1SBW16""400LF40K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF40K1CUNVxDTS","ASM1SBW16""400LF40K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF40K1CUNVxJ24_","ASM1SBW16""500LF40K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF40K1CUNVxJ48_","ASM1SBW16""500LF40K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF40K1CUNVxJ96_","ASM1SBW16""500LF40K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF40K1CUNVxJ120_","ASM1SBW16""500LF40K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF40K1CUNVxDTG","ASM1SBW16""500LF40K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF40K1CUNVxDTS","ASM1SBW16""500LF40K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF940K1CUNVxJ24_","ASM1SRL8""100LF940K1CUNVxJ24_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF940K1CUNVxJ48_","ASM1SRL8""100LF940K1CUNVxJ48_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF940K1CUNVxJ96_","ASM1SRL8""100LF940K1CUNVxJ96_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF940K1CUNVxJ120_","ASM1SRL8""100LF940K1CUNVxJ120_",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF940K1CUNVxDTG","ASM1SRL8""100LF940K1CUNVxDTG",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""100LF940K1CUNVxDTS","ASM1SRL8""100LF940K1CUNVxDTS",Regress Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF940K1CUNVxJ24_","ASM1SRL8""200LF940K1CUNVxJ24_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF940K1CUNVxJ48_","ASM1SRL8""200LF940K1CUNVxJ48_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF940K1CUNVxJ96_","ASM1SRL8""200LF940K1CUNVxJ96_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF940K1CUNVxJ120_","ASM1SRL8""200LF940K1CUNVxJ120_",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF940K1CUNVxDTG","ASM1SRL8""200LF940K1CUNVxDTG",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""200LF940K1CUNVxDTS","ASM1SRL8""200LF940K1CUNVxDTS",Regress Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF940K1CUNVxJ24_","ASM1SRL8""300LF940K1CUNVxJ24_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF940K1CUNVxJ48_","ASM1SRL8""300LF940K1CUNVxJ48_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF940K1CUNVxJ96_","ASM1SRL8""300LF940K1CUNVxJ96_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF940K1CUNVxJ120_","ASM1SRL8""300LF940K1CUNVxJ120_",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF940K1CUNVxDTG","ASM1SRL8""300LF940K1CUNVxDTG",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""300LF940K1CUNVxDTS","ASM1SRL8""300LF940K1CUNVxDTS",Regress Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF940K1CUNVxJ24_","ASM1SRL8""400LF940K1CUNVxJ24_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF940K1CUNVxJ48_","ASM1SRL8""400LF940K1CUNVxJ48_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF940K1CUNVxJ96_","ASM1SRL8""400LF940K1CUNVxJ96_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF940K1CUNVxJ120_","ASM1SRL8""400LF940K1CUNVxJ120_",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF940K1CUNVxDTG","ASM1SRL8""400LF940K1CUNVxDTG",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""400LF940K1CUNVxDTS","ASM1SRL8""400LF940K1CUNVxDTS",Regress Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF940K1CUNVxJ24_","ASM1SRL8""500LF940K1CUNVxJ24_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF940K1CUNVxJ48_","ASM1SRL8""500LF940K1CUNVxJ48_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF940K1CUNVxJ96_","ASM1SRL8""500LF940K1CUNVxJ96_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF940K1CUNVxJ120_","ASM1SRL8""500LF940K1CUNVxJ120_",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF940K1CUNVxDTG","ASM1SRL8""500LF940K1CUNVxDTG",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL8""500LF940K1CUNVxDTS","ASM1SRL8""500LF940K1CUNVxDTS",Regress Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF940K1CUNVxJ24_","ASM1SRL12""100LF940K1CUNVxJ24_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF940K1CUNVxJ48_","ASM1SRL12""100LF940K1CUNVxJ48_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF940K1CUNVxJ96_","ASM1SRL12""100LF940K1CUNVxJ96_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF940K1CUNVxJ120_","ASM1SRL12""100LF940K1CUNVxJ120_",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF940K1CUNVxDTG","ASM1SRL12""100LF940K1CUNVxDTG",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""100LF940K1CUNVxDTS","ASM1SRL12""100LF940K1CUNVxDTS",Regress Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF940K1CUNVxJ24_","ASM1SRL12""200LF940K1CUNVxJ24_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF940K1CUNVxJ48_","ASM1SRL12""200LF940K1CUNVxJ48_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF940K1CUNVxJ96_","ASM1SRL12""200LF940K1CUNVxJ96_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF940K1CUNVxJ120_","ASM1SRL12""200LF940K1CUNVxJ120_",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF940K1CUNVxDTG","ASM1SRL12""200LF940K1CUNVxDTG",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""200LF940K1CUNVxDTS","ASM1SRL12""200LF940K1CUNVxDTS",Regress Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF940K1CUNVxJ24_","ASM1SRL12""300LF940K1CUNVxJ24_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF940K1CUNVxJ48_","ASM1SRL12""300LF940K1CUNVxJ48_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF940K1CUNVxJ96_","ASM1SRL12""300LF940K1CUNVxJ96_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF940K1CUNVxJ120_","ASM1SRL12""300LF940K1CUNVxJ120_",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF940K1CUNVxDTG","ASM1SRL12""300LF940K1CUNVxDTG",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""300LF940K1CUNVxDTS","ASM1SRL12""300LF940K1CUNVxDTS",Regress Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF940K1CUNVxJ24_","ASM1SRL12""400LF940K1CUNVxJ24_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF940K1CUNVxJ48_","ASM1SRL12""400LF940K1CUNVxJ48_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF940K1CUNVxJ96_","ASM1SRL12""400LF940K1CUNVxJ96_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF940K1CUNVxJ120_","ASM1SRL12""400LF940K1CUNVxJ120_",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF940K1CUNVxDTG","ASM1SRL12""400LF940K1CUNVxDTG",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""400LF940K1CUNVxDTS","ASM1SRL12""400LF940K1CUNVxDTS",Regress Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF940K1CUNVxJ24_","ASM1SRL12""500LF940K1CUNVxJ24_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF940K1CUNVxJ48_","ASM1SRL12""500LF940K1CUNVxJ48_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF940K1CUNVxJ96_","ASM1SRL12""500LF940K1CUNVxJ96_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF940K1CUNVxJ120_","ASM1SRL12""500LF940K1CUNVxJ120_",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF940K1CUNVxDTG","ASM1SRL12""500LF940K1CUNVxDTG",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL12""500LF940K1CUNVxDTS","ASM1SRL12""500LF940K1CUNVxDTS",Regress Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF940K1CUNVxJ24_","ASM1SRL16""100LF940K1CUNVxJ24_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF940K1CUNVxJ48_","ASM1SRL16""100LF940K1CUNVxJ48_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF940K1CUNVxJ96_","ASM1SRL16""100LF940K1CUNVxJ96_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF940K1CUNVxJ120_","ASM1SRL16""100LF940K1CUNVxJ120_",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF940K1CUNVxDTG","ASM1SRL16""100LF940K1CUNVxDTG",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""100LF940K1CUNVxDTS","ASM1SRL16""100LF940K1CUNVxDTS",Regress Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-RL-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF940K1CUNVxJ24_","ASM1SRL16""200LF940K1CUNVxJ24_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF940K1CUNVxJ48_","ASM1SRL16""200LF940K1CUNVxJ48_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF940K1CUNVxJ96_","ASM1SRL16""200LF940K1CUNVxJ96_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF940K1CUNVxJ120_","ASM1SRL16""200LF940K1CUNVxJ120_",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF940K1CUNVxDTG","ASM1SRL16""200LF940K1CUNVxDTG",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""200LF940K1CUNVxDTS","ASM1SRL16""200LF940K1CUNVxDTS",Regress Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-RL-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF940K1CUNVxJ24_","ASM1SRL16""300LF940K1CUNVxJ24_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF940K1CUNVxJ48_","ASM1SRL16""300LF940K1CUNVxJ48_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF940K1CUNVxJ96_","ASM1SRL16""300LF940K1CUNVxJ96_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF940K1CUNVxJ120_","ASM1SRL16""300LF940K1CUNVxJ120_",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF940K1CUNVxDTG","ASM1SRL16""300LF940K1CUNVxDTG",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""300LF940K1CUNVxDTS","ASM1SRL16""300LF940K1CUNVxDTS",Regress Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-RL-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF940K1CUNVxJ24_","ASM1SRL16""400LF940K1CUNVxJ24_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF940K1CUNVxJ48_","ASM1SRL16""400LF940K1CUNVxJ48_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF940K1CUNVxJ96_","ASM1SRL16""400LF940K1CUNVxJ96_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF940K1CUNVxJ120_","ASM1SRL16""400LF940K1CUNVxJ120_",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF940K1CUNVxDTG","ASM1SRL16""400LF940K1CUNVxDTG",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""400LF940K1CUNVxDTS","ASM1SRL16""400LF940K1CUNVxDTS",Regress Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-RL-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF940K1CUNVxJ24_","ASM1SRL16""500LF940K1CUNVxJ24_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF940K1CUNVxJ48_","ASM1SRL16""500LF940K1CUNVxJ48_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF940K1CUNVxJ96_","ASM1SRL16""500LF940K1CUNVxJ96_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF940K1CUNVxJ120_","ASM1SRL16""500LF940K1CUNVxJ120_",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF940K1CUNVxDTG","ASM1SRL16""500LF940K1CUNVxDTG",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SRL16""500LF940K1CUNVxDTS","ASM1SRL16""500LF940K1CUNVxDTS",Regress Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-RL-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF940K1CUNVxJ24_","ASM1SAS8""100LF940K1CUNVxJ24_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF940K1CUNVxJ48_","ASM1SAS8""100LF940K1CUNVxJ48_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF940K1CUNVxJ96_","ASM1SAS8""100LF940K1CUNVxJ96_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF940K1CUNVxJ120_","ASM1SAS8""100LF940K1CUNVxJ120_",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF940K1CUNVxDTG","ASM1SAS8""100LF940K1CUNVxDTG",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""100LF940K1CUNVxDTS","ASM1SAS8""100LF940K1CUNVxDTS",Asymmetric Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF940K1CUNVxJ24_","ASM1SAS8""200LF940K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF940K1CUNVxJ48_","ASM1SAS8""200LF940K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF940K1CUNVxJ96_","ASM1SAS8""200LF940K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF940K1CUNVxJ120_","ASM1SAS8""200LF940K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF940K1CUNVxDTG","ASM1SAS8""200LF940K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""200LF940K1CUNVxDTS","ASM1SAS8""200LF940K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF940K1CUNVxJ24_","ASM1SAS8""300LF940K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF940K1CUNVxJ48_","ASM1SAS8""300LF940K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF940K1CUNVxJ96_","ASM1SAS8""300LF940K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF940K1CUNVxJ120_","ASM1SAS8""300LF940K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF940K1CUNVxDTG","ASM1SAS8""300LF940K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""300LF940K1CUNVxDTS","ASM1SAS8""300LF940K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF940K1CUNVxJ24_","ASM1SAS8""400LF940K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF940K1CUNVxJ48_","ASM1SAS8""400LF940K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF940K1CUNVxJ96_","ASM1SAS8""400LF940K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF940K1CUNVxJ120_","ASM1SAS8""400LF940K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF940K1CUNVxDTG","ASM1SAS8""400LF940K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""400LF940K1CUNVxDTS","ASM1SAS8""400LF940K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF940K1CUNVxJ24_","ASM1SAS8""500LF940K1CUNVxJ24_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF940K1CUNVxJ48_","ASM1SAS8""500LF940K1CUNVxJ48_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF940K1CUNVxJ96_","ASM1SAS8""500LF940K1CUNVxJ96_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF940K1CUNVxJ120_","ASM1SAS8""500LF940K1CUNVxJ120_",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF940K1CUNVxDTG","ASM1SAS8""500LF940K1CUNVxDTG",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS8""500LF940K1CUNVxDTS","ASM1SAS8""500LF940K1CUNVxDTS",Asymmetric Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF940K1CUNVxJ24_","ASM1SAS12""100LF940K1CUNVxJ24_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF940K1CUNVxJ48_","ASM1SAS12""100LF940K1CUNVxJ48_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF940K1CUNVxJ96_","ASM1SAS12""100LF940K1CUNVxJ96_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF940K1CUNVxJ120_","ASM1SAS12""100LF940K1CUNVxJ120_",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF940K1CUNVxDTG","ASM1SAS12""100LF940K1CUNVxDTG",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""100LF940K1CUNVxDTS","ASM1SAS12""100LF940K1CUNVxDTS",Asymmetric Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF940K1CUNVxJ24_","ASM1SAS12""200LF940K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF940K1CUNVxJ48_","ASM1SAS12""200LF940K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF940K1CUNVxJ96_","ASM1SAS12""200LF940K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF940K1CUNVxJ120_","ASM1SAS12""200LF940K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF940K1CUNVxDTG","ASM1SAS12""200LF940K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""200LF940K1CUNVxDTS","ASM1SAS12""200LF940K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF940K1CUNVxJ24_","ASM1SAS12""300LF940K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF940K1CUNVxJ48_","ASM1SAS12""300LF940K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF940K1CUNVxJ96_","ASM1SAS12""300LF940K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF940K1CUNVxJ120_","ASM1SAS12""300LF940K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF940K1CUNVxDTG","ASM1SAS12""300LF940K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""300LF940K1CUNVxDTS","ASM1SAS12""300LF940K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF940K1CUNVxJ24_","ASM1SAS12""400LF940K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF940K1CUNVxJ48_","ASM1SAS12""400LF940K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF940K1CUNVxJ96_","ASM1SAS12""400LF940K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF940K1CUNVxJ120_","ASM1SAS12""400LF940K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF940K1CUNVxDTG","ASM1SAS12""400LF940K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""400LF940K1CUNVxDTS","ASM1SAS12""400LF940K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF940K1CUNVxJ24_","ASM1SAS12""500LF940K1CUNVxJ24_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF940K1CUNVxJ48_","ASM1SAS12""500LF940K1CUNVxJ48_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF940K1CUNVxJ96_","ASM1SAS12""500LF940K1CUNVxJ96_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF940K1CUNVxJ120_","ASM1SAS12""500LF940K1CUNVxJ120_",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF940K1CUNVxDTG","ASM1SAS12""500LF940K1CUNVxDTG",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS12""500LF940K1CUNVxDTS","ASM1SAS12""500LF940K1CUNVxDTS",Asymmetric Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF940K1CUNVxJ24_","ASM1SAS16""100LF940K1CUNVxJ24_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF940K1CUNVxJ48_","ASM1SAS16""100LF940K1CUNVxJ48_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF940K1CUNVxJ96_","ASM1SAS16""100LF940K1CUNVxJ96_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF940K1CUNVxJ120_","ASM1SAS16""100LF940K1CUNVxJ120_",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF940K1CUNVxDTG","ASM1SAS16""100LF940K1CUNVxDTG",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""100LF940K1CUNVxDTS","ASM1SAS16""100LF940K1CUNVxDTS",Asymmetric Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-AS-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF940K1CUNVxJ24_","ASM1SAS16""200LF940K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF940K1CUNVxJ48_","ASM1SAS16""200LF940K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF940K1CUNVxJ96_","ASM1SAS16""200LF940K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF940K1CUNVxJ120_","ASM1SAS16""200LF940K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF940K1CUNVxDTG","ASM1SAS16""200LF940K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""200LF940K1CUNVxDTS","ASM1SAS16""200LF940K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-AS-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF940K1CUNVxJ24_","ASM1SAS16""300LF940K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF940K1CUNVxJ48_","ASM1SAS16""300LF940K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF940K1CUNVxJ96_","ASM1SAS16""300LF940K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF940K1CUNVxJ120_","ASM1SAS16""300LF940K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF940K1CUNVxDTG","ASM1SAS16""300LF940K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""300LF940K1CUNVxDTS","ASM1SAS16""300LF940K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-AS-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF940K1CUNVxJ24_","ASM1SAS16""400LF940K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF940K1CUNVxJ48_","ASM1SAS16""400LF940K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF940K1CUNVxJ96_","ASM1SAS16""400LF940K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF940K1CUNVxJ120_","ASM1SAS16""400LF940K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF940K1CUNVxDTG","ASM1SAS16""400LF940K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""400LF940K1CUNVxDTS","ASM1SAS16""400LF940K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-AS-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF940K1CUNVxJ24_","ASM1SAS16""500LF940K1CUNVxJ24_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF940K1CUNVxJ48_","ASM1SAS16""500LF940K1CUNVxJ48_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF940K1CUNVxJ96_","ASM1SAS16""500LF940K1CUNVxJ96_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF940K1CUNVxJ120_","ASM1SAS16""500LF940K1CUNVxJ120_",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF940K1CUNVxDTG","ASM1SAS16""500LF940K1CUNVxDTG",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SAS16""500LF940K1CUNVxDTS","ASM1SAS16""500LF940K1CUNVxDTS",Asymmetric Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-AS-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF940K1CUNVxJ24_","ASM1SBW8""100LF940K1CUNVxJ24_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF940K1CUNVxJ48_","ASM1SBW8""100LF940K1CUNVxJ48_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF940K1CUNVxJ96_","ASM1SBW8""100LF940K1CUNVxJ96_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF940K1CUNVxJ120_","ASM1SBW8""100LF940K1CUNVxJ120_",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF940K1CUNVxDTG","ASM1SBW8""100LF940K1CUNVxDTG",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""100LF940K1CUNVxDTS","ASM1SBW8""100LF940K1CUNVxDTS",Batwing Lens,8,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF940K1CUNVxJ24_","ASM1SBW8""200LF940K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF940K1CUNVxJ48_","ASM1SBW8""200LF940K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF940K1CUNVxJ96_","ASM1SBW8""200LF940K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF940K1CUNVxJ120_","ASM1SBW8""200LF940K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF940K1CUNVxDTG","ASM1SBW8""200LF940K1CUNVxDTG",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""200LF940K1CUNVxDTS","ASM1SBW8""200LF940K1CUNVxDTS",Batwing Lens,8,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF940K1CUNVxJ24_","ASM1SBW8""300LF940K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF940K1CUNVxJ48_","ASM1SBW8""300LF940K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF940K1CUNVxJ96_","ASM1SBW8""300LF940K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF940K1CUNVxJ120_","ASM1SBW8""300LF940K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF940K1CUNVxDTG","ASM1SBW8""300LF940K1CUNVxDTG",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""300LF940K1CUNVxDTS","ASM1SBW8""300LF940K1CUNVxDTS",Batwing Lens,8,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF940K1CUNVxJ24_","ASM1SBW8""400LF940K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF940K1CUNVxJ48_","ASM1SBW8""400LF940K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF940K1CUNVxJ96_","ASM1SBW8""400LF940K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF940K1CUNVxJ120_","ASM1SBW8""400LF940K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF940K1CUNVxDTG","ASM1SBW8""400LF940K1CUNVxDTG",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""400LF940K1CUNVxDTS","ASM1SBW8""400LF940K1CUNVxDTS",Batwing Lens,8,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF940K1CUNVxJ24_","ASM1SBW8""500LF940K1CUNVxJ24_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF940K1CUNVxJ48_","ASM1SBW8""500LF940K1CUNVxJ48_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF940K1CUNVxJ96_","ASM1SBW8""500LF940K1CUNVxJ96_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF940K1CUNVxJ120_","ASM1SBW8""500LF940K1CUNVxJ120_",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF940K1CUNVxDTG","ASM1SBW8""500LF940K1CUNVxDTG",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW8""500LF940K1CUNVxDTS","ASM1SBW8""500LF940K1CUNVxDTS",Batwing Lens,8,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF940K1CUNVxJ24_","ASM1SBW12""100LF940K1CUNVxJ24_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF940K1CUNVxJ48_","ASM1SBW12""100LF940K1CUNVxJ48_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF940K1CUNVxJ96_","ASM1SBW12""100LF940K1CUNVxJ96_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF940K1CUNVxJ120_","ASM1SBW12""100LF940K1CUNVxJ120_",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF940K1CUNVxDTG","ASM1SBW12""100LF940K1CUNVxDTG",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""100LF940K1CUNVxDTS","ASM1SBW12""100LF940K1CUNVxDTS",Batwing Lens,12,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF940K1CUNVxJ24_","ASM1SBW12""200LF940K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF940K1CUNVxJ48_","ASM1SBW12""200LF940K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF940K1CUNVxJ96_","ASM1SBW12""200LF940K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF940K1CUNVxJ120_","ASM1SBW12""200LF940K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF940K1CUNVxDTG","ASM1SBW12""200LF940K1CUNVxDTG",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""200LF940K1CUNVxDTS","ASM1SBW12""200LF940K1CUNVxDTS",Batwing Lens,12,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF940K1CUNVxJ24_","ASM1SBW12""300LF940K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF940K1CUNVxJ48_","ASM1SBW12""300LF940K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF940K1CUNVxJ96_","ASM1SBW12""300LF940K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF940K1CUNVxJ120_","ASM1SBW12""300LF940K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF940K1CUNVxDTG","ASM1SBW12""300LF940K1CUNVxDTG",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""300LF940K1CUNVxDTS","ASM1SBW12""300LF940K1CUNVxDTS",Batwing Lens,12,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF940K1CUNVxJ24_","ASM1SBW12""400LF940K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF940K1CUNVxJ48_","ASM1SBW12""400LF940K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF940K1CUNVxJ96_","ASM1SBW12""400LF940K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF940K1CUNVxJ120_","ASM1SBW12""400LF940K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF940K1CUNVxDTG","ASM1SBW12""400LF940K1CUNVxDTG",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""400LF940K1CUNVxDTS","ASM1SBW12""400LF940K1CUNVxDTS",Batwing Lens,12,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF940K1CUNVxJ24_","ASM1SBW12""500LF940K1CUNVxJ24_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF940K1CUNVxJ48_","ASM1SBW12""500LF940K1CUNVxJ48_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF940K1CUNVxJ96_","ASM1SBW12""500LF940K1CUNVxJ96_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF940K1CUNVxJ120_","ASM1SBW12""500LF940K1CUNVxJ120_",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF940K1CUNVxDTG","ASM1SBW12""500LF940K1CUNVxDTG",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW12""500LF940K1CUNVxDTS","ASM1SBW12""500LF940K1CUNVxDTS",Batwing Lens,12,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF940K1CUNVxJ24_","ASM1SBW16""100LF940K1CUNVxJ24_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",100,120,66.66666667,24,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF940K1CUNVxJ48_","ASM1SBW16""100LF940K1CUNVxJ48_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",100,120,66.66666667,48,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF940K1CUNVxJ96_","ASM1SBW16""100LF940K1CUNVxJ96_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",100,120,66.66666667,96,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF940K1CUNVxJ120_","ASM1SBW16""100LF940K1CUNVxJ120_",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",100,120,66.66666667,120,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF940K1CUNVxDTG","ASM1SBW16""100LF940K1CUNVxDTG",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""100LF940K1CUNVxDTS","ASM1SBW16""100LF940K1CUNVxDTS",Batwing Lens,16,"Direct Distribution 100 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,100,120,66.66666667,0,1.5,1.5 Watts per foot,ASM1S-BW-100LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF940K1CUNVxJ24_","ASM1SBW16""200LF940K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",200,120,80,24,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF940K1CUNVxJ48_","ASM1SBW16""200LF940K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",200,120,80,48,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF940K1CUNVxJ96_","ASM1SBW16""200LF940K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",200,120,80,96,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF940K1CUNVxJ120_","ASM1SBW16""200LF940K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",200,120,80,120,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF940K1CUNVxDTG","ASM1SBW16""200LF940K1CUNVxDTG",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""200LF940K1CUNVxDTS","ASM1SBW16""200LF940K1CUNVxDTS",Batwing Lens,16,Direct Distribution 200 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,200,120,80,0,2.5,2.5 Watts per foot,ASM1S-BW-200LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF940K1CUNVxJ24_","ASM1SBW16""300LF940K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",300,120,85.71428571,24,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF940K1CUNVxJ48_","ASM1SBW16""300LF940K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",300,120,85.71428571,48,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF940K1CUNVxJ96_","ASM1SBW16""300LF940K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",300,120,85.71428571,96,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF940K1CUNVxJ120_","ASM1SBW16""300LF940K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",300,120,85.71428571,120,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF940K1CUNVxDTG","ASM1SBW16""300LF940K1CUNVxDTG",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""300LF940K1CUNVxDTS","ASM1SBW16""300LF940K1CUNVxDTS",Batwing Lens,16,Direct Distribution 300 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,300,120,85.71428571,0,3.5,3.5 Watts per foot,ASM1S-BW-300LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF940K1CUNVxJ24_","ASM1SBW16""400LF940K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",400,120,94.11764706,24,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF940K1CUNVxJ48_","ASM1SBW16""400LF940K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",400,120,94.11764706,48,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF940K1CUNVxJ96_","ASM1SBW16""400LF940K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",400,120,94.11764706,96,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF940K1CUNVxJ120_","ASM1SBW16""400LF940K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",400,120,94.11764706,120,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF940K1CUNVxDTG","ASM1SBW16""400LF940K1CUNVxDTG",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""400LF940K1CUNVxDTS","ASM1SBW16""400LF940K1CUNVxDTS",Batwing Lens,16,Direct Distribution 400 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,400,120,94.11764706,0,4.25,4.25 Watts per foot,ASM1S-BW-400LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF940K1CUNVxJ24_","ASM1SBW16""500LF940K1CUNVxJ24_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,90.90909091,24,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF940K1CUNVxJ48_","ASM1SBW16""500LF940K1CUNVxJ48_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,90.90909091,48,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF940K1CUNVxJ96_","ASM1SBW16""500LF940K1CUNVxJ96_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,90.90909091,96,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF940K1CUNVxJ120_","ASM1SBW16""500LF940K1CUNVxJ120_",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,90.90909091,120,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF940K1CUNVxDTG","ASM1SBW16""500LF940K1CUNVxDTG",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Grid,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBW16""500LF940K1CUNVxDTS","ASM1SBW16""500LF940K1CUNVxDTS",Batwing Lens,16,Direct Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,Direct/Flush to Strut,500,120,90.90909091,0,5.5,5.5 Watts per foot,ASM1S-BW-500LF-35K-1C-UNV-4.ies,N/A
