,Model##OTHER##,Shielding Type##OTHER##,Fixture Height##OTHER##,Lumen Output Comment##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Color Temperature Note##OTHER##,Circuit##OTHER##,Voltage Comment##OTHER##,Driver Comment##OTHER##,Mounting##Other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,C Cable Integer##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Photometric Web File##OTHER##,Driver##Other##
"ASM1SBWSD8""125LF27K1CUNVxJ24_","ASM1SBWSD8""125LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF27K1CUNVxJ48_","ASM1SBWSD8""125LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF27K1CUNVxJ96_","ASM1SBWSD8""125LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF27K1CUNVxJ120_","ASM1SBWSD8""125LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF27K1CUNVxJ24_","ASM1SBWSD8""250LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF27K1CUNVxJ48_","ASM1SBWSD8""250LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF27K1CUNVxJ96_","ASM1SBWSD8""250LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF27K1CUNVxJ120_","ASM1SBWSD8""250LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF27K1CUNVxJ24_","ASM1SBWSD8""375LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF27K1CUNVxJ48_","ASM1SBWSD8""375LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF27K1CUNVxJ96_","ASM1SBWSD8""375LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF27K1CUNVxJ120_","ASM1SBWSD8""375LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF27K1CUNVxJ24_","ASM1SBWSD8""500LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF27K1CUNVxJ48_","ASM1SBWSD8""500LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF27K1CUNVxJ96_","ASM1SBWSD8""500LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF27K1CUNVxJ120_","ASM1SBWSD8""500LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF27K1CUNVxJ24_","ASM1SBWSD8""625LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF27K1CUNVxJ48_","ASM1SBWSD8""625LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF27K1CUNVxJ96_","ASM1SBWSD8""625LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF27K1CUNVxJ120_","ASM1SBWSD8""625LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF27K1CUNVxJ24_","ASM1SBWSD8""800LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF27K1CUNVxJ48_","ASM1SBWSD8""800LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF27K1CUNVxJ96_","ASM1SBWSD8""800LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF27K1CUNVxJ120_","ASM1SBWSD8""800LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF27K1CUNVxJ24_","ASM1SBWSD12""125LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF27K1CUNVxJ48_","ASM1SBWSD12""125LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF27K1CUNVxJ96_","ASM1SBWSD12""125LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF27K1CUNVxJ120_","ASM1SBWSD12""125LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF27K1CUNVxJ24_","ASM1SBWSD12""250LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF27K1CUNVxJ48_","ASM1SBWSD12""250LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF27K1CUNVxJ96_","ASM1SBWSD12""250LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF27K1CUNVxJ120_","ASM1SBWSD12""250LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF27K1CUNVxJ24_","ASM1SBWSD12""375LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF27K1CUNVxJ48_","ASM1SBWSD12""375LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF27K1CUNVxJ96_","ASM1SBWSD12""375LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF27K1CUNVxJ120_","ASM1SBWSD12""375LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF27K1CUNVxJ24_","ASM1SBWSD12""500LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF27K1CUNVxJ48_","ASM1SBWSD12""500LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF27K1CUNVxJ96_","ASM1SBWSD12""500LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF27K1CUNVxJ120_","ASM1SBWSD12""500LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF27K1CUNVxJ24_","ASM1SBWSD12""625LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF27K1CUNVxJ48_","ASM1SBWSD12""625LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF27K1CUNVxJ96_","ASM1SBWSD12""625LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF27K1CUNVxJ120_","ASM1SBWSD12""625LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF27K1CUNVxJ24_","ASM1SBWSD12""800LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF27K1CUNVxJ48_","ASM1SBWSD12""800LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF27K1CUNVxJ96_","ASM1SBWSD12""800LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF27K1CUNVxJ120_","ASM1SBWSD12""800LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF27K1CUNVxJ24_","ASM1SBWSD16""125LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF27K1CUNVxJ48_","ASM1SBWSD16""125LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF27K1CUNVxJ96_","ASM1SBWSD16""125LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF27K1CUNVxJ120_","ASM1SBWSD16""125LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF27K1CUNVxJ24_","ASM1SBWSD16""250LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF27K1CUNVxJ48_","ASM1SBWSD16""250LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF27K1CUNVxJ96_","ASM1SBWSD16""250LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF27K1CUNVxJ120_","ASM1SBWSD16""250LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF27K1CUNVxJ24_","ASM1SBWSD16""375LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF27K1CUNVxJ48_","ASM1SBWSD16""375LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF27K1CUNVxJ96_","ASM1SBWSD16""375LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF27K1CUNVxJ120_","ASM1SBWSD16""375LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF27K1CUNVxJ24_","ASM1SBWSD16""500LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF27K1CUNVxJ48_","ASM1SBWSD16""500LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF27K1CUNVxJ96_","ASM1SBWSD16""500LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF27K1CUNVxJ120_","ASM1SBWSD16""500LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF27K1CUNVxJ24_","ASM1SBWSD16""625LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF27K1CUNVxJ48_","ASM1SBWSD16""625LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF27K1CUNVxJ96_","ASM1SBWSD16""625LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF27K1CUNVxJ120_","ASM1SBWSD16""625LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF27K1CUNVxJ24_","ASM1SBWSD16""800LF27K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF27K1CUNVxJ48_","ASM1SBWSD16""800LF27K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF27K1CUNVxJ96_","ASM1SBWSD16""800LF27K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF27K1CUNVxJ120_","ASM1SBWSD16""800LF27K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF27K1CUNVxJ24_","ASM1SDCSD8""125LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF27K1CUNVxJ48_","ASM1SDCSD8""125LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF27K1CUNVxJ96_","ASM1SDCSD8""125LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF27K1CUNVxJ120_","ASM1SDCSD8""125LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF27K1CUNVxJ24_","ASM1SDCSD8""250LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF27K1CUNVxJ48_","ASM1SDCSD8""250LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF27K1CUNVxJ96_","ASM1SDCSD8""250LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF27K1CUNVxJ120_","ASM1SDCSD8""250LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF27K1CUNVxJ24_","ASM1SDCSD8""375LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF27K1CUNVxJ48_","ASM1SDCSD8""375LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF27K1CUNVxJ96_","ASM1SDCSD8""375LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF27K1CUNVxJ120_","ASM1SDCSD8""375LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF27K1CUNVxJ24_","ASM1SDCSD8""500LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF27K1CUNVxJ48_","ASM1SDCSD8""500LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF27K1CUNVxJ96_","ASM1SDCSD8""500LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF27K1CUNVxJ120_","ASM1SDCSD8""500LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF27K1CUNVxJ24_","ASM1SDCSD8""625LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF27K1CUNVxJ48_","ASM1SDCSD8""625LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF27K1CUNVxJ96_","ASM1SDCSD8""625LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF27K1CUNVxJ120_","ASM1SDCSD8""625LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF27K1CUNVxJ24_","ASM1SDCSD8""800LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF27K1CUNVxJ48_","ASM1SDCSD8""800LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF27K1CUNVxJ96_","ASM1SDCSD8""800LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF27K1CUNVxJ120_","ASM1SDCSD8""800LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF27K1CUNVxJ24_","ASM1SDCSD12""125LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF27K1CUNVxJ48_","ASM1SDCSD12""125LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF27K1CUNVxJ96_","ASM1SDCSD12""125LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF27K1CUNVxJ120_","ASM1SDCSD12""125LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF27K1CUNVxJ24_","ASM1SDCSD12""250LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF27K1CUNVxJ48_","ASM1SDCSD12""250LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF27K1CUNVxJ96_","ASM1SDCSD12""250LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF27K1CUNVxJ120_","ASM1SDCSD12""250LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF27K1CUNVxJ24_","ASM1SDCSD12""375LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF27K1CUNVxJ48_","ASM1SDCSD12""375LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF27K1CUNVxJ96_","ASM1SDCSD12""375LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF27K1CUNVxJ120_","ASM1SDCSD12""375LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF27K1CUNVxJ24_","ASM1SDCSD12""500LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF27K1CUNVxJ48_","ASM1SDCSD12""500LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF27K1CUNVxJ96_","ASM1SDCSD12""500LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF27K1CUNVxJ120_","ASM1SDCSD12""500LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF27K1CUNVxJ24_","ASM1SDCSD12""625LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF27K1CUNVxJ48_","ASM1SDCSD12""625LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF27K1CUNVxJ96_","ASM1SDCSD12""625LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF27K1CUNVxJ120_","ASM1SDCSD12""625LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF27K1CUNVxJ24_","ASM1SDCSD12""800LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF27K1CUNVxJ48_","ASM1SDCSD12""800LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF27K1CUNVxJ96_","ASM1SDCSD12""800LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF27K1CUNVxJ120_","ASM1SDCSD12""800LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF27K1CUNVxJ24_","ASM1SDCSD16""125LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF27K1CUNVxJ48_","ASM1SDCSD16""125LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF27K1CUNVxJ96_","ASM1SDCSD16""125LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF27K1CUNVxJ120_","ASM1SDCSD16""125LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF27K1CUNVxJ24_","ASM1SDCSD16""250LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF27K1CUNVxJ48_","ASM1SDCSD16""250LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF27K1CUNVxJ96_","ASM1SDCSD16""250LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF27K1CUNVxJ120_","ASM1SDCSD16""250LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF27K1CUNVxJ24_","ASM1SDCSD16""375LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF27K1CUNVxJ48_","ASM1SDCSD16""375LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF27K1CUNVxJ96_","ASM1SDCSD16""375LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF27K1CUNVxJ120_","ASM1SDCSD16""375LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF27K1CUNVxJ24_","ASM1SDCSD16""500LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF27K1CUNVxJ48_","ASM1SDCSD16""500LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF27K1CUNVxJ96_","ASM1SDCSD16""500LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF27K1CUNVxJ120_","ASM1SDCSD16""500LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF27K1CUNVxJ24_","ASM1SDCSD16""625LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF27K1CUNVxJ48_","ASM1SDCSD16""625LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF27K1CUNVxJ96_","ASM1SDCSD16""625LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF27K1CUNVxJ120_","ASM1SDCSD16""625LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF27K1CUNVxJ24_","ASM1SDCSD16""800LF27K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF27K1CUNVxJ48_","ASM1SDCSD16""800LF27K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF27K1CUNVxJ96_","ASM1SDCSD16""800LF27K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF27K1CUNVxJ120_","ASM1SDCSD16""800LF27K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF927K1CUNVxJ24_","ASM1SBWSD8""125LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF927K1CUNVxJ48_","ASM1SBWSD8""125LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF927K1CUNVxJ96_","ASM1SBWSD8""125LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF927K1CUNVxJ120_","ASM1SBWSD8""125LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF927K1CUNVxJ24_","ASM1SBWSD8""250LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF927K1CUNVxJ48_","ASM1SBWSD8""250LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF927K1CUNVxJ96_","ASM1SBWSD8""250LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF927K1CUNVxJ120_","ASM1SBWSD8""250LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF927K1CUNVxJ24_","ASM1SBWSD8""375LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF927K1CUNVxJ48_","ASM1SBWSD8""375LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF927K1CUNVxJ96_","ASM1SBWSD8""375LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF927K1CUNVxJ120_","ASM1SBWSD8""375LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF927K1CUNVxJ24_","ASM1SBWSD8""500LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF927K1CUNVxJ48_","ASM1SBWSD8""500LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF927K1CUNVxJ96_","ASM1SBWSD8""500LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF927K1CUNVxJ120_","ASM1SBWSD8""500LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF927K1CUNVxJ24_","ASM1SBWSD8""625LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF927K1CUNVxJ48_","ASM1SBWSD8""625LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF927K1CUNVxJ96_","ASM1SBWSD8""625LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF927K1CUNVxJ120_","ASM1SBWSD8""625LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF927K1CUNVxJ24_","ASM1SBWSD8""800LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF927K1CUNVxJ48_","ASM1SBWSD8""800LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF927K1CUNVxJ96_","ASM1SBWSD8""800LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF927K1CUNVxJ120_","ASM1SBWSD8""800LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF927K1CUNVxJ24_","ASM1SBWSD12""125LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF927K1CUNVxJ48_","ASM1SBWSD12""125LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF927K1CUNVxJ96_","ASM1SBWSD12""125LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF927K1CUNVxJ120_","ASM1SBWSD12""125LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF927K1CUNVxJ24_","ASM1SBWSD12""250LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF927K1CUNVxJ48_","ASM1SBWSD12""250LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF927K1CUNVxJ96_","ASM1SBWSD12""250LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF927K1CUNVxJ120_","ASM1SBWSD12""250LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF927K1CUNVxJ24_","ASM1SBWSD12""375LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF927K1CUNVxJ48_","ASM1SBWSD12""375LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF927K1CUNVxJ96_","ASM1SBWSD12""375LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF927K1CUNVxJ120_","ASM1SBWSD12""375LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF927K1CUNVxJ24_","ASM1SBWSD12""500LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF927K1CUNVxJ48_","ASM1SBWSD12""500LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF927K1CUNVxJ96_","ASM1SBWSD12""500LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF927K1CUNVxJ120_","ASM1SBWSD12""500LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF927K1CUNVxJ24_","ASM1SBWSD12""625LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF927K1CUNVxJ48_","ASM1SBWSD12""625LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF927K1CUNVxJ96_","ASM1SBWSD12""625LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF927K1CUNVxJ120_","ASM1SBWSD12""625LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF927K1CUNVxJ24_","ASM1SBWSD12""800LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF927K1CUNVxJ48_","ASM1SBWSD12""800LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF927K1CUNVxJ96_","ASM1SBWSD12""800LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF927K1CUNVxJ120_","ASM1SBWSD12""800LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF927K1CUNVxJ24_","ASM1SBWSD16""125LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF927K1CUNVxJ48_","ASM1SBWSD16""125LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF927K1CUNVxJ96_","ASM1SBWSD16""125LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF927K1CUNVxJ120_","ASM1SBWSD16""125LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF927K1CUNVxJ24_","ASM1SBWSD16""250LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF927K1CUNVxJ48_","ASM1SBWSD16""250LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF927K1CUNVxJ96_","ASM1SBWSD16""250LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF927K1CUNVxJ120_","ASM1SBWSD16""250LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF927K1CUNVxJ24_","ASM1SBWSD16""375LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF927K1CUNVxJ48_","ASM1SBWSD16""375LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF927K1CUNVxJ96_","ASM1SBWSD16""375LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF927K1CUNVxJ120_","ASM1SBWSD16""375LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF927K1CUNVxJ24_","ASM1SBWSD16""500LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF927K1CUNVxJ48_","ASM1SBWSD16""500LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF927K1CUNVxJ96_","ASM1SBWSD16""500LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF927K1CUNVxJ120_","ASM1SBWSD16""500LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF927K1CUNVxJ24_","ASM1SBWSD16""625LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF927K1CUNVxJ48_","ASM1SBWSD16""625LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF927K1CUNVxJ96_","ASM1SBWSD16""625LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF927K1CUNVxJ120_","ASM1SBWSD16""625LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF927K1CUNVxJ24_","ASM1SBWSD16""800LF927K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF927K1CUNVxJ48_","ASM1SBWSD16""800LF927K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF927K1CUNVxJ96_","ASM1SBWSD16""800LF927K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF927K1CUNVxJ120_","ASM1SBWSD16""800LF927K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF927K1CUNVxJ24_","ASM1SDCSD8""125LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF927K1CUNVxJ48_","ASM1SDCSD8""125LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF927K1CUNVxJ96_","ASM1SDCSD8""125LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF927K1CUNVxJ120_","ASM1SDCSD8""125LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF927K1CUNVxJ24_","ASM1SDCSD8""250LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF927K1CUNVxJ48_","ASM1SDCSD8""250LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF927K1CUNVxJ96_","ASM1SDCSD8""250LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF927K1CUNVxJ120_","ASM1SDCSD8""250LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF927K1CUNVxJ24_","ASM1SDCSD8""375LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF927K1CUNVxJ48_","ASM1SDCSD8""375LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF927K1CUNVxJ96_","ASM1SDCSD8""375LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF927K1CUNVxJ120_","ASM1SDCSD8""375LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF927K1CUNVxJ24_","ASM1SDCSD8""500LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF927K1CUNVxJ48_","ASM1SDCSD8""500LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF927K1CUNVxJ96_","ASM1SDCSD8""500LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF927K1CUNVxJ120_","ASM1SDCSD8""500LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF927K1CUNVxJ24_","ASM1SDCSD8""625LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF927K1CUNVxJ48_","ASM1SDCSD8""625LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF927K1CUNVxJ96_","ASM1SDCSD8""625LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF927K1CUNVxJ120_","ASM1SDCSD8""625LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF927K1CUNVxJ24_","ASM1SDCSD8""800LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF927K1CUNVxJ48_","ASM1SDCSD8""800LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF927K1CUNVxJ96_","ASM1SDCSD8""800LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF927K1CUNVxJ120_","ASM1SDCSD8""800LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF927K1CUNVxJ24_","ASM1SDCSD12""125LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF927K1CUNVxJ48_","ASM1SDCSD12""125LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF927K1CUNVxJ96_","ASM1SDCSD12""125LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF927K1CUNVxJ120_","ASM1SDCSD12""125LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF927K1CUNVxJ24_","ASM1SDCSD12""250LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF927K1CUNVxJ48_","ASM1SDCSD12""250LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF927K1CUNVxJ96_","ASM1SDCSD12""250LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF927K1CUNVxJ120_","ASM1SDCSD12""250LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF927K1CUNVxJ24_","ASM1SDCSD12""375LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF927K1CUNVxJ48_","ASM1SDCSD12""375LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF927K1CUNVxJ96_","ASM1SDCSD12""375LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF927K1CUNVxJ120_","ASM1SDCSD12""375LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF927K1CUNVxJ24_","ASM1SDCSD12""500LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF927K1CUNVxJ48_","ASM1SDCSD12""500LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF927K1CUNVxJ96_","ASM1SDCSD12""500LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF927K1CUNVxJ120_","ASM1SDCSD12""500LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF927K1CUNVxJ24_","ASM1SDCSD12""625LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF927K1CUNVxJ48_","ASM1SDCSD12""625LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF927K1CUNVxJ96_","ASM1SDCSD12""625LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF927K1CUNVxJ120_","ASM1SDCSD12""625LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF927K1CUNVxJ24_","ASM1SDCSD12""800LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF927K1CUNVxJ48_","ASM1SDCSD12""800LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF927K1CUNVxJ96_","ASM1SDCSD12""800LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF927K1CUNVxJ120_","ASM1SDCSD12""800LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF927K1CUNVxJ24_","ASM1SDCSD16""125LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF927K1CUNVxJ48_","ASM1SDCSD16""125LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF927K1CUNVxJ96_","ASM1SDCSD16""125LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF927K1CUNVxJ120_","ASM1SDCSD16""125LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF927K1CUNVxJ24_","ASM1SDCSD16""250LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF927K1CUNVxJ48_","ASM1SDCSD16""250LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF927K1CUNVxJ96_","ASM1SDCSD16""250LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF927K1CUNVxJ120_","ASM1SDCSD16""250LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF927K1CUNVxJ24_","ASM1SDCSD16""375LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF927K1CUNVxJ48_","ASM1SDCSD16""375LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF927K1CUNVxJ96_","ASM1SDCSD16""375LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF927K1CUNVxJ120_","ASM1SDCSD16""375LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF927K1CUNVxJ24_","ASM1SDCSD16""500LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF927K1CUNVxJ48_","ASM1SDCSD16""500LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF927K1CUNVxJ96_","ASM1SDCSD16""500LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF927K1CUNVxJ120_","ASM1SDCSD16""500LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF927K1CUNVxJ24_","ASM1SDCSD16""625LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF927K1CUNVxJ48_","ASM1SDCSD16""625LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF927K1CUNVxJ96_","ASM1SDCSD16""625LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF927K1CUNVxJ120_","ASM1SDCSD16""625LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF927K1CUNVxJ24_","ASM1SDCSD16""800LF927K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF927K1CUNVxJ48_","ASM1SDCSD16""800LF927K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF927K1CUNVxJ96_","ASM1SDCSD16""800LF927K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF927K1CUNVxJ120_","ASM1SDCSD16""800LF927K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,2700,"2700K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF30K1CUNVxJ24_","ASM1SBWSD8""125LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF30K1CUNVxJ48_","ASM1SBWSD8""125LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF30K1CUNVxJ96_","ASM1SBWSD8""125LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF30K1CUNVxJ120_","ASM1SBWSD8""125LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF30K1CUNVxJ24_","ASM1SBWSD8""250LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF30K1CUNVxJ48_","ASM1SBWSD8""250LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF30K1CUNVxJ96_","ASM1SBWSD8""250LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF30K1CUNVxJ120_","ASM1SBWSD8""250LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF30K1CUNVxJ24_","ASM1SBWSD8""375LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF30K1CUNVxJ48_","ASM1SBWSD8""375LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF30K1CUNVxJ96_","ASM1SBWSD8""375LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF30K1CUNVxJ120_","ASM1SBWSD8""375LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF30K1CUNVxJ24_","ASM1SBWSD8""500LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF30K1CUNVxJ48_","ASM1SBWSD8""500LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF30K1CUNVxJ96_","ASM1SBWSD8""500LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF30K1CUNVxJ120_","ASM1SBWSD8""500LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF30K1CUNVxJ24_","ASM1SBWSD8""625LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF30K1CUNVxJ48_","ASM1SBWSD8""625LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF30K1CUNVxJ96_","ASM1SBWSD8""625LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF30K1CUNVxJ120_","ASM1SBWSD8""625LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF30K1CUNVxJ24_","ASM1SBWSD8""800LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF30K1CUNVxJ48_","ASM1SBWSD8""800LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF30K1CUNVxJ96_","ASM1SBWSD8""800LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF30K1CUNVxJ120_","ASM1SBWSD8""800LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF30K1CUNVxJ24_","ASM1SBWSD12""125LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF30K1CUNVxJ48_","ASM1SBWSD12""125LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF30K1CUNVxJ96_","ASM1SBWSD12""125LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF30K1CUNVxJ120_","ASM1SBWSD12""125LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF30K1CUNVxJ24_","ASM1SBWSD12""250LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF30K1CUNVxJ48_","ASM1SBWSD12""250LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF30K1CUNVxJ96_","ASM1SBWSD12""250LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF30K1CUNVxJ120_","ASM1SBWSD12""250LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF30K1CUNVxJ24_","ASM1SBWSD12""375LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF30K1CUNVxJ48_","ASM1SBWSD12""375LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF30K1CUNVxJ96_","ASM1SBWSD12""375LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF30K1CUNVxJ120_","ASM1SBWSD12""375LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF30K1CUNVxJ24_","ASM1SBWSD12""500LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF30K1CUNVxJ48_","ASM1SBWSD12""500LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF30K1CUNVxJ96_","ASM1SBWSD12""500LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF30K1CUNVxJ120_","ASM1SBWSD12""500LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF30K1CUNVxJ24_","ASM1SBWSD12""625LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF30K1CUNVxJ48_","ASM1SBWSD12""625LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF30K1CUNVxJ96_","ASM1SBWSD12""625LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF30K1CUNVxJ120_","ASM1SBWSD12""625LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF30K1CUNVxJ24_","ASM1SBWSD12""800LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF30K1CUNVxJ48_","ASM1SBWSD12""800LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF30K1CUNVxJ96_","ASM1SBWSD12""800LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF30K1CUNVxJ120_","ASM1SBWSD12""800LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF30K1CUNVxJ24_","ASM1SBWSD16""125LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF30K1CUNVxJ48_","ASM1SBWSD16""125LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF30K1CUNVxJ96_","ASM1SBWSD16""125LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF30K1CUNVxJ120_","ASM1SBWSD16""125LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF30K1CUNVxJ24_","ASM1SBWSD16""250LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF30K1CUNVxJ48_","ASM1SBWSD16""250LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF30K1CUNVxJ96_","ASM1SBWSD16""250LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF30K1CUNVxJ120_","ASM1SBWSD16""250LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF30K1CUNVxJ24_","ASM1SBWSD16""375LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF30K1CUNVxJ48_","ASM1SBWSD16""375LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF30K1CUNVxJ96_","ASM1SBWSD16""375LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF30K1CUNVxJ120_","ASM1SBWSD16""375LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF30K1CUNVxJ24_","ASM1SBWSD16""500LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF30K1CUNVxJ48_","ASM1SBWSD16""500LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF30K1CUNVxJ96_","ASM1SBWSD16""500LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF30K1CUNVxJ120_","ASM1SBWSD16""500LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF30K1CUNVxJ24_","ASM1SBWSD16""625LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF30K1CUNVxJ48_","ASM1SBWSD16""625LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF30K1CUNVxJ96_","ASM1SBWSD16""625LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF30K1CUNVxJ120_","ASM1SBWSD16""625LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF30K1CUNVxJ24_","ASM1SBWSD16""800LF30K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF30K1CUNVxJ48_","ASM1SBWSD16""800LF30K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF30K1CUNVxJ96_","ASM1SBWSD16""800LF30K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF30K1CUNVxJ120_","ASM1SBWSD16""800LF30K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF30K1CUNVxJ24_","ASM1SDCSD8""125LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF30K1CUNVxJ48_","ASM1SDCSD8""125LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF30K1CUNVxJ96_","ASM1SDCSD8""125LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF30K1CUNVxJ120_","ASM1SDCSD8""125LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF30K1CUNVxJ24_","ASM1SDCSD8""250LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF30K1CUNVxJ48_","ASM1SDCSD8""250LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF30K1CUNVxJ96_","ASM1SDCSD8""250LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF30K1CUNVxJ120_","ASM1SDCSD8""250LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF30K1CUNVxJ24_","ASM1SDCSD8""375LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF30K1CUNVxJ48_","ASM1SDCSD8""375LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF30K1CUNVxJ96_","ASM1SDCSD8""375LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF30K1CUNVxJ120_","ASM1SDCSD8""375LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF30K1CUNVxJ24_","ASM1SDCSD8""500LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF30K1CUNVxJ48_","ASM1SDCSD8""500LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF30K1CUNVxJ96_","ASM1SDCSD8""500LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF30K1CUNVxJ120_","ASM1SDCSD8""500LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF30K1CUNVxJ24_","ASM1SDCSD8""625LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF30K1CUNVxJ48_","ASM1SDCSD8""625LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF30K1CUNVxJ96_","ASM1SDCSD8""625LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF30K1CUNVxJ120_","ASM1SDCSD8""625LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF30K1CUNVxJ24_","ASM1SDCSD8""800LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF30K1CUNVxJ48_","ASM1SDCSD8""800LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF30K1CUNVxJ96_","ASM1SDCSD8""800LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF30K1CUNVxJ120_","ASM1SDCSD8""800LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF30K1CUNVxJ24_","ASM1SDCSD12""125LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF30K1CUNVxJ48_","ASM1SDCSD12""125LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF30K1CUNVxJ96_","ASM1SDCSD12""125LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF30K1CUNVxJ120_","ASM1SDCSD12""125LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF30K1CUNVxJ24_","ASM1SDCSD12""250LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF30K1CUNVxJ48_","ASM1SDCSD12""250LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF30K1CUNVxJ96_","ASM1SDCSD12""250LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF30K1CUNVxJ120_","ASM1SDCSD12""250LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF30K1CUNVxJ24_","ASM1SDCSD12""375LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF30K1CUNVxJ48_","ASM1SDCSD12""375LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF30K1CUNVxJ96_","ASM1SDCSD12""375LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF30K1CUNVxJ120_","ASM1SDCSD12""375LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF30K1CUNVxJ24_","ASM1SDCSD12""500LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF30K1CUNVxJ48_","ASM1SDCSD12""500LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF30K1CUNVxJ96_","ASM1SDCSD12""500LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF30K1CUNVxJ120_","ASM1SDCSD12""500LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF30K1CUNVxJ24_","ASM1SDCSD12""625LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF30K1CUNVxJ48_","ASM1SDCSD12""625LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF30K1CUNVxJ96_","ASM1SDCSD12""625LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF30K1CUNVxJ120_","ASM1SDCSD12""625LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF30K1CUNVxJ24_","ASM1SDCSD12""800LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF30K1CUNVxJ48_","ASM1SDCSD12""800LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF30K1CUNVxJ96_","ASM1SDCSD12""800LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF30K1CUNVxJ120_","ASM1SDCSD12""800LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF30K1CUNVxJ24_","ASM1SDCSD16""125LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF30K1CUNVxJ48_","ASM1SDCSD16""125LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF30K1CUNVxJ96_","ASM1SDCSD16""125LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF30K1CUNVxJ120_","ASM1SDCSD16""125LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF30K1CUNVxJ24_","ASM1SDCSD16""250LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF30K1CUNVxJ48_","ASM1SDCSD16""250LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF30K1CUNVxJ96_","ASM1SDCSD16""250LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF30K1CUNVxJ120_","ASM1SDCSD16""250LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF30K1CUNVxJ24_","ASM1SDCSD16""375LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF30K1CUNVxJ48_","ASM1SDCSD16""375LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF30K1CUNVxJ96_","ASM1SDCSD16""375LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF30K1CUNVxJ120_","ASM1SDCSD16""375LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF30K1CUNVxJ24_","ASM1SDCSD16""500LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF30K1CUNVxJ48_","ASM1SDCSD16""500LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF30K1CUNVxJ96_","ASM1SDCSD16""500LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF30K1CUNVxJ120_","ASM1SDCSD16""500LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF30K1CUNVxJ24_","ASM1SDCSD16""625LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF30K1CUNVxJ48_","ASM1SDCSD16""625LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF30K1CUNVxJ96_","ASM1SDCSD16""625LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF30K1CUNVxJ120_","ASM1SDCSD16""625LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF30K1CUNVxJ24_","ASM1SDCSD16""800LF30K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF30K1CUNVxJ48_","ASM1SDCSD16""800LF30K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF30K1CUNVxJ96_","ASM1SDCSD16""800LF30K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF30K1CUNVxJ120_","ASM1SDCSD16""800LF30K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF930K1CUNVxJ24_","ASM1SBWSD8""125LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF930K1CUNVxJ48_","ASM1SBWSD8""125LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF930K1CUNVxJ96_","ASM1SBWSD8""125LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF930K1CUNVxJ120_","ASM1SBWSD8""125LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF930K1CUNVxJ24_","ASM1SBWSD8""250LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF930K1CUNVxJ48_","ASM1SBWSD8""250LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF930K1CUNVxJ96_","ASM1SBWSD8""250LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF930K1CUNVxJ120_","ASM1SBWSD8""250LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF930K1CUNVxJ24_","ASM1SBWSD8""375LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF930K1CUNVxJ48_","ASM1SBWSD8""375LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF930K1CUNVxJ96_","ASM1SBWSD8""375LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF930K1CUNVxJ120_","ASM1SBWSD8""375LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF930K1CUNVxJ24_","ASM1SBWSD8""500LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF930K1CUNVxJ48_","ASM1SBWSD8""500LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF930K1CUNVxJ96_","ASM1SBWSD8""500LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF930K1CUNVxJ120_","ASM1SBWSD8""500LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF930K1CUNVxJ24_","ASM1SBWSD8""625LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF930K1CUNVxJ48_","ASM1SBWSD8""625LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF930K1CUNVxJ96_","ASM1SBWSD8""625LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF930K1CUNVxJ120_","ASM1SBWSD8""625LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF930K1CUNVxJ24_","ASM1SBWSD8""800LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF930K1CUNVxJ48_","ASM1SBWSD8""800LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF930K1CUNVxJ96_","ASM1SBWSD8""800LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF930K1CUNVxJ120_","ASM1SBWSD8""800LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF930K1CUNVxJ24_","ASM1SBWSD12""125LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF930K1CUNVxJ48_","ASM1SBWSD12""125LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF930K1CUNVxJ96_","ASM1SBWSD12""125LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF930K1CUNVxJ120_","ASM1SBWSD12""125LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF930K1CUNVxJ24_","ASM1SBWSD12""250LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF930K1CUNVxJ48_","ASM1SBWSD12""250LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF930K1CUNVxJ96_","ASM1SBWSD12""250LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF930K1CUNVxJ120_","ASM1SBWSD12""250LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF930K1CUNVxJ24_","ASM1SBWSD12""375LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF930K1CUNVxJ48_","ASM1SBWSD12""375LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF930K1CUNVxJ96_","ASM1SBWSD12""375LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF930K1CUNVxJ120_","ASM1SBWSD12""375LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF930K1CUNVxJ24_","ASM1SBWSD12""500LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF930K1CUNVxJ48_","ASM1SBWSD12""500LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF930K1CUNVxJ96_","ASM1SBWSD12""500LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF930K1CUNVxJ120_","ASM1SBWSD12""500LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF930K1CUNVxJ24_","ASM1SBWSD12""625LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF930K1CUNVxJ48_","ASM1SBWSD12""625LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF930K1CUNVxJ96_","ASM1SBWSD12""625LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF930K1CUNVxJ120_","ASM1SBWSD12""625LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF930K1CUNVxJ24_","ASM1SBWSD12""800LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF930K1CUNVxJ48_","ASM1SBWSD12""800LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF930K1CUNVxJ96_","ASM1SBWSD12""800LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF930K1CUNVxJ120_","ASM1SBWSD12""800LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF930K1CUNVxJ24_","ASM1SBWSD16""125LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF930K1CUNVxJ48_","ASM1SBWSD16""125LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF930K1CUNVxJ96_","ASM1SBWSD16""125LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF930K1CUNVxJ120_","ASM1SBWSD16""125LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF930K1CUNVxJ24_","ASM1SBWSD16""250LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF930K1CUNVxJ48_","ASM1SBWSD16""250LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF930K1CUNVxJ96_","ASM1SBWSD16""250LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF930K1CUNVxJ120_","ASM1SBWSD16""250LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF930K1CUNVxJ24_","ASM1SBWSD16""375LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF930K1CUNVxJ48_","ASM1SBWSD16""375LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF930K1CUNVxJ96_","ASM1SBWSD16""375LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF930K1CUNVxJ120_","ASM1SBWSD16""375LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF930K1CUNVxJ24_","ASM1SBWSD16""500LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF930K1CUNVxJ48_","ASM1SBWSD16""500LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF930K1CUNVxJ96_","ASM1SBWSD16""500LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF930K1CUNVxJ120_","ASM1SBWSD16""500LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF930K1CUNVxJ24_","ASM1SBWSD16""625LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF930K1CUNVxJ48_","ASM1SBWSD16""625LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF930K1CUNVxJ96_","ASM1SBWSD16""625LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF930K1CUNVxJ120_","ASM1SBWSD16""625LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF930K1CUNVxJ24_","ASM1SBWSD16""800LF930K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF930K1CUNVxJ48_","ASM1SBWSD16""800LF930K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF930K1CUNVxJ96_","ASM1SBWSD16""800LF930K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF930K1CUNVxJ120_","ASM1SBWSD16""800LF930K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF930K1CUNVxJ24_","ASM1SDCSD8""125LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF930K1CUNVxJ48_","ASM1SDCSD8""125LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF930K1CUNVxJ96_","ASM1SDCSD8""125LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF930K1CUNVxJ120_","ASM1SDCSD8""125LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF930K1CUNVxJ24_","ASM1SDCSD8""250LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF930K1CUNVxJ48_","ASM1SDCSD8""250LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF930K1CUNVxJ96_","ASM1SDCSD8""250LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF930K1CUNVxJ120_","ASM1SDCSD8""250LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF930K1CUNVxJ24_","ASM1SDCSD8""375LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF930K1CUNVxJ48_","ASM1SDCSD8""375LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF930K1CUNVxJ96_","ASM1SDCSD8""375LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF930K1CUNVxJ120_","ASM1SDCSD8""375LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF930K1CUNVxJ24_","ASM1SDCSD8""500LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF930K1CUNVxJ48_","ASM1SDCSD8""500LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF930K1CUNVxJ96_","ASM1SDCSD8""500LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF930K1CUNVxJ120_","ASM1SDCSD8""500LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF930K1CUNVxJ24_","ASM1SDCSD8""625LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF930K1CUNVxJ48_","ASM1SDCSD8""625LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF930K1CUNVxJ96_","ASM1SDCSD8""625LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF930K1CUNVxJ120_","ASM1SDCSD8""625LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF930K1CUNVxJ24_","ASM1SDCSD8""800LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF930K1CUNVxJ48_","ASM1SDCSD8""800LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF930K1CUNVxJ96_","ASM1SDCSD8""800LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF930K1CUNVxJ120_","ASM1SDCSD8""800LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF930K1CUNVxJ24_","ASM1SDCSD12""125LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF930K1CUNVxJ48_","ASM1SDCSD12""125LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF930K1CUNVxJ96_","ASM1SDCSD12""125LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF930K1CUNVxJ120_","ASM1SDCSD12""125LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF930K1CUNVxJ24_","ASM1SDCSD12""250LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF930K1CUNVxJ48_","ASM1SDCSD12""250LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF930K1CUNVxJ96_","ASM1SDCSD12""250LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF930K1CUNVxJ120_","ASM1SDCSD12""250LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF930K1CUNVxJ24_","ASM1SDCSD12""375LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF930K1CUNVxJ48_","ASM1SDCSD12""375LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF930K1CUNVxJ96_","ASM1SDCSD12""375LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF930K1CUNVxJ120_","ASM1SDCSD12""375LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF930K1CUNVxJ24_","ASM1SDCSD12""500LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF930K1CUNVxJ48_","ASM1SDCSD12""500LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF930K1CUNVxJ96_","ASM1SDCSD12""500LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF930K1CUNVxJ120_","ASM1SDCSD12""500LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF930K1CUNVxJ24_","ASM1SDCSD12""625LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF930K1CUNVxJ48_","ASM1SDCSD12""625LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF930K1CUNVxJ96_","ASM1SDCSD12""625LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF930K1CUNVxJ120_","ASM1SDCSD12""625LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF930K1CUNVxJ24_","ASM1SDCSD12""800LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF930K1CUNVxJ48_","ASM1SDCSD12""800LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF930K1CUNVxJ96_","ASM1SDCSD12""800LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF930K1CUNVxJ120_","ASM1SDCSD12""800LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF930K1CUNVxJ24_","ASM1SDCSD16""125LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF930K1CUNVxJ48_","ASM1SDCSD16""125LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF930K1CUNVxJ96_","ASM1SDCSD16""125LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF930K1CUNVxJ120_","ASM1SDCSD16""125LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF930K1CUNVxJ24_","ASM1SDCSD16""250LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF930K1CUNVxJ48_","ASM1SDCSD16""250LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF930K1CUNVxJ96_","ASM1SDCSD16""250LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF930K1CUNVxJ120_","ASM1SDCSD16""250LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF930K1CUNVxJ24_","ASM1SDCSD16""375LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF930K1CUNVxJ48_","ASM1SDCSD16""375LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF930K1CUNVxJ96_","ASM1SDCSD16""375LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF930K1CUNVxJ120_","ASM1SDCSD16""375LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF930K1CUNVxJ24_","ASM1SDCSD16""500LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF930K1CUNVxJ48_","ASM1SDCSD16""500LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF930K1CUNVxJ96_","ASM1SDCSD16""500LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF930K1CUNVxJ120_","ASM1SDCSD16""500LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF930K1CUNVxJ24_","ASM1SDCSD16""625LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF930K1CUNVxJ48_","ASM1SDCSD16""625LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF930K1CUNVxJ96_","ASM1SDCSD16""625LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF930K1CUNVxJ120_","ASM1SDCSD16""625LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF930K1CUNVxJ24_","ASM1SDCSD16""800LF930K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF930K1CUNVxJ48_","ASM1SDCSD16""800LF930K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF930K1CUNVxJ96_","ASM1SDCSD16""800LF930K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF930K1CUNVxJ120_","ASM1SDCSD16""800LF930K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3000,"3000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF35K1CUNVxJ24_","ASM1SBWSD8""125LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF35K1CUNVxJ48_","ASM1SBWSD8""125LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF35K1CUNVxJ96_","ASM1SBWSD8""125LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF35K1CUNVxJ120_","ASM1SBWSD8""125LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF35K1CUNVxJ24_","ASM1SBWSD8""250LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF35K1CUNVxJ48_","ASM1SBWSD8""250LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF35K1CUNVxJ96_","ASM1SBWSD8""250LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF35K1CUNVxJ120_","ASM1SBWSD8""250LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF35K1CUNVxJ24_","ASM1SBWSD8""375LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF35K1CUNVxJ48_","ASM1SBWSD8""375LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF35K1CUNVxJ96_","ASM1SBWSD8""375LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF35K1CUNVxJ120_","ASM1SBWSD8""375LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF35K1CUNVxJ24_","ASM1SBWSD8""500LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF35K1CUNVxJ48_","ASM1SBWSD8""500LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF35K1CUNVxJ96_","ASM1SBWSD8""500LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF35K1CUNVxJ120_","ASM1SBWSD8""500LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF35K1CUNVxJ24_","ASM1SBWSD8""625LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF35K1CUNVxJ48_","ASM1SBWSD8""625LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF35K1CUNVxJ96_","ASM1SBWSD8""625LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF35K1CUNVxJ120_","ASM1SBWSD8""625LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF35K1CUNVxJ24_","ASM1SBWSD8""800LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF35K1CUNVxJ48_","ASM1SBWSD8""800LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF35K1CUNVxJ96_","ASM1SBWSD8""800LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF35K1CUNVxJ120_","ASM1SBWSD8""800LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF35K1CUNVxJ24_","ASM1SBWSD12""125LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF35K1CUNVxJ48_","ASM1SBWSD12""125LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF35K1CUNVxJ96_","ASM1SBWSD12""125LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF35K1CUNVxJ120_","ASM1SBWSD12""125LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF35K1CUNVxJ24_","ASM1SBWSD12""250LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF35K1CUNVxJ48_","ASM1SBWSD12""250LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF35K1CUNVxJ96_","ASM1SBWSD12""250LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF35K1CUNVxJ120_","ASM1SBWSD12""250LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF35K1CUNVxJ24_","ASM1SBWSD12""375LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF35K1CUNVxJ48_","ASM1SBWSD12""375LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF35K1CUNVxJ96_","ASM1SBWSD12""375LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF35K1CUNVxJ120_","ASM1SBWSD12""375LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF35K1CUNVxJ24_","ASM1SBWSD12""500LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF35K1CUNVxJ48_","ASM1SBWSD12""500LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF35K1CUNVxJ96_","ASM1SBWSD12""500LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF35K1CUNVxJ120_","ASM1SBWSD12""500LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF35K1CUNVxJ24_","ASM1SBWSD12""625LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF35K1CUNVxJ48_","ASM1SBWSD12""625LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF35K1CUNVxJ96_","ASM1SBWSD12""625LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF35K1CUNVxJ120_","ASM1SBWSD12""625LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF35K1CUNVxJ24_","ASM1SBWSD12""800LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF35K1CUNVxJ48_","ASM1SBWSD12""800LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF35K1CUNVxJ96_","ASM1SBWSD12""800LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF35K1CUNVxJ120_","ASM1SBWSD12""800LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF35K1CUNVxJ24_","ASM1SBWSD16""125LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF35K1CUNVxJ48_","ASM1SBWSD16""125LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF35K1CUNVxJ96_","ASM1SBWSD16""125LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF35K1CUNVxJ120_","ASM1SBWSD16""125LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF35K1CUNVxJ24_","ASM1SBWSD16""250LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF35K1CUNVxJ48_","ASM1SBWSD16""250LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF35K1CUNVxJ96_","ASM1SBWSD16""250LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF35K1CUNVxJ120_","ASM1SBWSD16""250LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF35K1CUNVxJ24_","ASM1SBWSD16""375LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF35K1CUNVxJ48_","ASM1SBWSD16""375LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF35K1CUNVxJ96_","ASM1SBWSD16""375LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF35K1CUNVxJ120_","ASM1SBWSD16""375LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF35K1CUNVxJ24_","ASM1SBWSD16""500LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF35K1CUNVxJ48_","ASM1SBWSD16""500LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF35K1CUNVxJ96_","ASM1SBWSD16""500LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF35K1CUNVxJ120_","ASM1SBWSD16""500LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF35K1CUNVxJ24_","ASM1SBWSD16""625LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF35K1CUNVxJ48_","ASM1SBWSD16""625LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF35K1CUNVxJ96_","ASM1SBWSD16""625LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF35K1CUNVxJ120_","ASM1SBWSD16""625LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF35K1CUNVxJ24_","ASM1SBWSD16""800LF35K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF35K1CUNVxJ48_","ASM1SBWSD16""800LF35K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF35K1CUNVxJ96_","ASM1SBWSD16""800LF35K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF35K1CUNVxJ120_","ASM1SBWSD16""800LF35K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF35K1CUNVxJ24_","ASM1SDCSD8""125LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF35K1CUNVxJ48_","ASM1SDCSD8""125LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF35K1CUNVxJ96_","ASM1SDCSD8""125LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF35K1CUNVxJ120_","ASM1SDCSD8""125LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF35K1CUNVxJ24_","ASM1SDCSD8""250LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF35K1CUNVxJ48_","ASM1SDCSD8""250LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF35K1CUNVxJ96_","ASM1SDCSD8""250LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF35K1CUNVxJ120_","ASM1SDCSD8""250LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF35K1CUNVxJ24_","ASM1SDCSD8""375LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF35K1CUNVxJ48_","ASM1SDCSD8""375LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF35K1CUNVxJ96_","ASM1SDCSD8""375LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF35K1CUNVxJ120_","ASM1SDCSD8""375LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF35K1CUNVxJ24_","ASM1SDCSD8""500LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF35K1CUNVxJ48_","ASM1SDCSD8""500LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF35K1CUNVxJ96_","ASM1SDCSD8""500LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF35K1CUNVxJ120_","ASM1SDCSD8""500LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF35K1CUNVxJ24_","ASM1SDCSD8""625LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF35K1CUNVxJ48_","ASM1SDCSD8""625LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF35K1CUNVxJ96_","ASM1SDCSD8""625LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF35K1CUNVxJ120_","ASM1SDCSD8""625LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF35K1CUNVxJ24_","ASM1SDCSD8""800LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF35K1CUNVxJ48_","ASM1SDCSD8""800LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF35K1CUNVxJ96_","ASM1SDCSD8""800LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF35K1CUNVxJ120_","ASM1SDCSD8""800LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF35K1CUNVxJ24_","ASM1SDCSD12""125LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF35K1CUNVxJ48_","ASM1SDCSD12""125LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF35K1CUNVxJ96_","ASM1SDCSD12""125LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF35K1CUNVxJ120_","ASM1SDCSD12""125LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF35K1CUNVxJ24_","ASM1SDCSD12""250LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF35K1CUNVxJ48_","ASM1SDCSD12""250LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF35K1CUNVxJ96_","ASM1SDCSD12""250LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF35K1CUNVxJ120_","ASM1SDCSD12""250LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF35K1CUNVxJ24_","ASM1SDCSD12""375LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF35K1CUNVxJ48_","ASM1SDCSD12""375LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF35K1CUNVxJ96_","ASM1SDCSD12""375LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF35K1CUNVxJ120_","ASM1SDCSD12""375LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF35K1CUNVxJ24_","ASM1SDCSD12""500LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF35K1CUNVxJ48_","ASM1SDCSD12""500LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF35K1CUNVxJ96_","ASM1SDCSD12""500LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF35K1CUNVxJ120_","ASM1SDCSD12""500LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF35K1CUNVxJ24_","ASM1SDCSD12""625LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF35K1CUNVxJ48_","ASM1SDCSD12""625LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF35K1CUNVxJ96_","ASM1SDCSD12""625LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF35K1CUNVxJ120_","ASM1SDCSD12""625LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF35K1CUNVxJ24_","ASM1SDCSD12""800LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF35K1CUNVxJ48_","ASM1SDCSD12""800LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF35K1CUNVxJ96_","ASM1SDCSD12""800LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF35K1CUNVxJ120_","ASM1SDCSD12""800LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF35K1CUNVxJ24_","ASM1SDCSD16""125LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF35K1CUNVxJ48_","ASM1SDCSD16""125LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF35K1CUNVxJ96_","ASM1SDCSD16""125LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF35K1CUNVxJ120_","ASM1SDCSD16""125LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF35K1CUNVxJ24_","ASM1SDCSD16""250LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF35K1CUNVxJ48_","ASM1SDCSD16""250LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF35K1CUNVxJ96_","ASM1SDCSD16""250LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF35K1CUNVxJ120_","ASM1SDCSD16""250LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF35K1CUNVxJ24_","ASM1SDCSD16""375LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF35K1CUNVxJ48_","ASM1SDCSD16""375LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF35K1CUNVxJ96_","ASM1SDCSD16""375LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF35K1CUNVxJ120_","ASM1SDCSD16""375LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF35K1CUNVxJ24_","ASM1SDCSD16""500LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF35K1CUNVxJ48_","ASM1SDCSD16""500LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF35K1CUNVxJ96_","ASM1SDCSD16""500LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF35K1CUNVxJ120_","ASM1SDCSD16""500LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF35K1CUNVxJ24_","ASM1SDCSD16""625LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF35K1CUNVxJ48_","ASM1SDCSD16""625LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF35K1CUNVxJ96_","ASM1SDCSD16""625LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF35K1CUNVxJ120_","ASM1SDCSD16""625LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF35K1CUNVxJ24_","ASM1SDCSD16""800LF35K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF35K1CUNVxJ48_","ASM1SDCSD16""800LF35K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF35K1CUNVxJ96_","ASM1SDCSD16""800LF35K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF35K1CUNVxJ120_","ASM1SDCSD16""800LF35K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF935K1CUNVxJ24_","ASM1SBWSD8""125LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF935K1CUNVxJ48_","ASM1SBWSD8""125LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF935K1CUNVxJ96_","ASM1SBWSD8""125LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF935K1CUNVxJ120_","ASM1SBWSD8""125LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF935K1CUNVxJ24_","ASM1SBWSD8""250LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF935K1CUNVxJ48_","ASM1SBWSD8""250LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF935K1CUNVxJ96_","ASM1SBWSD8""250LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF935K1CUNVxJ120_","ASM1SBWSD8""250LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF935K1CUNVxJ24_","ASM1SBWSD8""375LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF935K1CUNVxJ48_","ASM1SBWSD8""375LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF935K1CUNVxJ96_","ASM1SBWSD8""375LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF935K1CUNVxJ120_","ASM1SBWSD8""375LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF935K1CUNVxJ24_","ASM1SBWSD8""500LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF935K1CUNVxJ48_","ASM1SBWSD8""500LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF935K1CUNVxJ96_","ASM1SBWSD8""500LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF935K1CUNVxJ120_","ASM1SBWSD8""500LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF935K1CUNVxJ24_","ASM1SBWSD8""625LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF935K1CUNVxJ48_","ASM1SBWSD8""625LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF935K1CUNVxJ96_","ASM1SBWSD8""625LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF935K1CUNVxJ120_","ASM1SBWSD8""625LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF935K1CUNVxJ24_","ASM1SBWSD8""800LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF935K1CUNVxJ48_","ASM1SBWSD8""800LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF935K1CUNVxJ96_","ASM1SBWSD8""800LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF935K1CUNVxJ120_","ASM1SBWSD8""800LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF935K1CUNVxJ24_","ASM1SBWSD12""125LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF935K1CUNVxJ48_","ASM1SBWSD12""125LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF935K1CUNVxJ96_","ASM1SBWSD12""125LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF935K1CUNVxJ120_","ASM1SBWSD12""125LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF935K1CUNVxJ24_","ASM1SBWSD12""250LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF935K1CUNVxJ48_","ASM1SBWSD12""250LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF935K1CUNVxJ96_","ASM1SBWSD12""250LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF935K1CUNVxJ120_","ASM1SBWSD12""250LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF935K1CUNVxJ24_","ASM1SBWSD12""375LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF935K1CUNVxJ48_","ASM1SBWSD12""375LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF935K1CUNVxJ96_","ASM1SBWSD12""375LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF935K1CUNVxJ120_","ASM1SBWSD12""375LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF935K1CUNVxJ24_","ASM1SBWSD12""500LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF935K1CUNVxJ48_","ASM1SBWSD12""500LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF935K1CUNVxJ96_","ASM1SBWSD12""500LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF935K1CUNVxJ120_","ASM1SBWSD12""500LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF935K1CUNVxJ24_","ASM1SBWSD12""625LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF935K1CUNVxJ48_","ASM1SBWSD12""625LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF935K1CUNVxJ96_","ASM1SBWSD12""625LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF935K1CUNVxJ120_","ASM1SBWSD12""625LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF935K1CUNVxJ24_","ASM1SBWSD12""800LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF935K1CUNVxJ48_","ASM1SBWSD12""800LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF935K1CUNVxJ96_","ASM1SBWSD12""800LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF935K1CUNVxJ120_","ASM1SBWSD12""800LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF935K1CUNVxJ24_","ASM1SBWSD16""125LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF935K1CUNVxJ48_","ASM1SBWSD16""125LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF935K1CUNVxJ96_","ASM1SBWSD16""125LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF935K1CUNVxJ120_","ASM1SBWSD16""125LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF935K1CUNVxJ24_","ASM1SBWSD16""250LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF935K1CUNVxJ48_","ASM1SBWSD16""250LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF935K1CUNVxJ96_","ASM1SBWSD16""250LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF935K1CUNVxJ120_","ASM1SBWSD16""250LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF935K1CUNVxJ24_","ASM1SBWSD16""375LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF935K1CUNVxJ48_","ASM1SBWSD16""375LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF935K1CUNVxJ96_","ASM1SBWSD16""375LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF935K1CUNVxJ120_","ASM1SBWSD16""375LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF935K1CUNVxJ24_","ASM1SBWSD16""500LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF935K1CUNVxJ48_","ASM1SBWSD16""500LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF935K1CUNVxJ96_","ASM1SBWSD16""500LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF935K1CUNVxJ120_","ASM1SBWSD16""500LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF935K1CUNVxJ24_","ASM1SBWSD16""625LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF935K1CUNVxJ48_","ASM1SBWSD16""625LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF935K1CUNVxJ96_","ASM1SBWSD16""625LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF935K1CUNVxJ120_","ASM1SBWSD16""625LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF935K1CUNVxJ24_","ASM1SBWSD16""800LF935K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF935K1CUNVxJ48_","ASM1SBWSD16""800LF935K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF935K1CUNVxJ96_","ASM1SBWSD16""800LF935K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF935K1CUNVxJ120_","ASM1SBWSD16""800LF935K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF935K1CUNVxJ24_","ASM1SDCSD8""125LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF935K1CUNVxJ48_","ASM1SDCSD8""125LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF935K1CUNVxJ96_","ASM1SDCSD8""125LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF935K1CUNVxJ120_","ASM1SDCSD8""125LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF935K1CUNVxJ24_","ASM1SDCSD8""250LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF935K1CUNVxJ48_","ASM1SDCSD8""250LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF935K1CUNVxJ96_","ASM1SDCSD8""250LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF935K1CUNVxJ120_","ASM1SDCSD8""250LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF935K1CUNVxJ24_","ASM1SDCSD8""375LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF935K1CUNVxJ48_","ASM1SDCSD8""375LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF935K1CUNVxJ96_","ASM1SDCSD8""375LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF935K1CUNVxJ120_","ASM1SDCSD8""375LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF935K1CUNVxJ24_","ASM1SDCSD8""500LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF935K1CUNVxJ48_","ASM1SDCSD8""500LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF935K1CUNVxJ96_","ASM1SDCSD8""500LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF935K1CUNVxJ120_","ASM1SDCSD8""500LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF935K1CUNVxJ24_","ASM1SDCSD8""625LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF935K1CUNVxJ48_","ASM1SDCSD8""625LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF935K1CUNVxJ96_","ASM1SDCSD8""625LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF935K1CUNVxJ120_","ASM1SDCSD8""625LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF935K1CUNVxJ24_","ASM1SDCSD8""800LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF935K1CUNVxJ48_","ASM1SDCSD8""800LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF935K1CUNVxJ96_","ASM1SDCSD8""800LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF935K1CUNVxJ120_","ASM1SDCSD8""800LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF935K1CUNVxJ24_","ASM1SDCSD12""125LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF935K1CUNVxJ48_","ASM1SDCSD12""125LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF935K1CUNVxJ96_","ASM1SDCSD12""125LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF935K1CUNVxJ120_","ASM1SDCSD12""125LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF935K1CUNVxJ24_","ASM1SDCSD12""250LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF935K1CUNVxJ48_","ASM1SDCSD12""250LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF935K1CUNVxJ96_","ASM1SDCSD12""250LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF935K1CUNVxJ120_","ASM1SDCSD12""250LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF935K1CUNVxJ24_","ASM1SDCSD12""375LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF935K1CUNVxJ48_","ASM1SDCSD12""375LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF935K1CUNVxJ96_","ASM1SDCSD12""375LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF935K1CUNVxJ120_","ASM1SDCSD12""375LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF935K1CUNVxJ24_","ASM1SDCSD12""500LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF935K1CUNVxJ48_","ASM1SDCSD12""500LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF935K1CUNVxJ96_","ASM1SDCSD12""500LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF935K1CUNVxJ120_","ASM1SDCSD12""500LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF935K1CUNVxJ24_","ASM1SDCSD12""625LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF935K1CUNVxJ48_","ASM1SDCSD12""625LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF935K1CUNVxJ96_","ASM1SDCSD12""625LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF935K1CUNVxJ120_","ASM1SDCSD12""625LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF935K1CUNVxJ24_","ASM1SDCSD12""800LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF935K1CUNVxJ48_","ASM1SDCSD12""800LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF935K1CUNVxJ96_","ASM1SDCSD12""800LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF935K1CUNVxJ120_","ASM1SDCSD12""800LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF935K1CUNVxJ24_","ASM1SDCSD16""125LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF935K1CUNVxJ48_","ASM1SDCSD16""125LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF935K1CUNVxJ96_","ASM1SDCSD16""125LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF935K1CUNVxJ120_","ASM1SDCSD16""125LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF935K1CUNVxJ24_","ASM1SDCSD16""250LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF935K1CUNVxJ48_","ASM1SDCSD16""250LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF935K1CUNVxJ96_","ASM1SDCSD16""250LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF935K1CUNVxJ120_","ASM1SDCSD16""250LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF935K1CUNVxJ24_","ASM1SDCSD16""375LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF935K1CUNVxJ48_","ASM1SDCSD16""375LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF935K1CUNVxJ96_","ASM1SDCSD16""375LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF935K1CUNVxJ120_","ASM1SDCSD16""375LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF935K1CUNVxJ24_","ASM1SDCSD16""500LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF935K1CUNVxJ48_","ASM1SDCSD16""500LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF935K1CUNVxJ96_","ASM1SDCSD16""500LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF935K1CUNVxJ120_","ASM1SDCSD16""500LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF935K1CUNVxJ24_","ASM1SDCSD16""625LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF935K1CUNVxJ48_","ASM1SDCSD16""625LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF935K1CUNVxJ96_","ASM1SDCSD16""625LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF935K1CUNVxJ120_","ASM1SDCSD16""625LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF935K1CUNVxJ24_","ASM1SDCSD16""800LF935K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF935K1CUNVxJ48_","ASM1SDCSD16""800LF935K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF935K1CUNVxJ96_","ASM1SDCSD16""800LF935K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF935K1CUNVxJ120_","ASM1SDCSD16""800LF935K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,3500,"3500K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF40K1CUNVxJ24_","ASM1SBWSD8""125LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF40K1CUNVxJ48_","ASM1SBWSD8""125LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF40K1CUNVxJ96_","ASM1SBWSD8""125LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF40K1CUNVxJ120_","ASM1SBWSD8""125LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF40K1CUNVxJ24_","ASM1SBWSD8""250LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF40K1CUNVxJ48_","ASM1SBWSD8""250LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF40K1CUNVxJ96_","ASM1SBWSD8""250LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF40K1CUNVxJ120_","ASM1SBWSD8""250LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF40K1CUNVxJ24_","ASM1SBWSD8""375LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF40K1CUNVxJ48_","ASM1SBWSD8""375LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF40K1CUNVxJ96_","ASM1SBWSD8""375LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF40K1CUNVxJ120_","ASM1SBWSD8""375LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF40K1CUNVxJ24_","ASM1SBWSD8""500LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF40K1CUNVxJ48_","ASM1SBWSD8""500LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF40K1CUNVxJ96_","ASM1SBWSD8""500LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF40K1CUNVxJ120_","ASM1SBWSD8""500LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF40K1CUNVxJ24_","ASM1SBWSD8""625LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF40K1CUNVxJ48_","ASM1SBWSD8""625LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF40K1CUNVxJ96_","ASM1SBWSD8""625LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF40K1CUNVxJ120_","ASM1SBWSD8""625LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF40K1CUNVxJ24_","ASM1SBWSD8""800LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF40K1CUNVxJ48_","ASM1SBWSD8""800LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF40K1CUNVxJ96_","ASM1SBWSD8""800LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF40K1CUNVxJ120_","ASM1SBWSD8""800LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF40K1CUNVxJ24_","ASM1SBWSD12""125LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF40K1CUNVxJ48_","ASM1SBWSD12""125LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF40K1CUNVxJ96_","ASM1SBWSD12""125LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF40K1CUNVxJ120_","ASM1SBWSD12""125LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF40K1CUNVxJ24_","ASM1SBWSD12""250LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF40K1CUNVxJ48_","ASM1SBWSD12""250LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF40K1CUNVxJ96_","ASM1SBWSD12""250LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF40K1CUNVxJ120_","ASM1SBWSD12""250LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF40K1CUNVxJ24_","ASM1SBWSD12""375LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF40K1CUNVxJ48_","ASM1SBWSD12""375LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF40K1CUNVxJ96_","ASM1SBWSD12""375LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF40K1CUNVxJ120_","ASM1SBWSD12""375LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF40K1CUNVxJ24_","ASM1SBWSD12""500LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF40K1CUNVxJ48_","ASM1SBWSD12""500LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF40K1CUNVxJ96_","ASM1SBWSD12""500LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF40K1CUNVxJ120_","ASM1SBWSD12""500LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF40K1CUNVxJ24_","ASM1SBWSD12""625LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF40K1CUNVxJ48_","ASM1SBWSD12""625LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF40K1CUNVxJ96_","ASM1SBWSD12""625LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF40K1CUNVxJ120_","ASM1SBWSD12""625LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF40K1CUNVxJ24_","ASM1SBWSD12""800LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF40K1CUNVxJ48_","ASM1SBWSD12""800LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF40K1CUNVxJ96_","ASM1SBWSD12""800LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF40K1CUNVxJ120_","ASM1SBWSD12""800LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF40K1CUNVxJ24_","ASM1SBWSD16""125LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF40K1CUNVxJ48_","ASM1SBWSD16""125LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF40K1CUNVxJ96_","ASM1SBWSD16""125LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF40K1CUNVxJ120_","ASM1SBWSD16""125LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF40K1CUNVxJ24_","ASM1SBWSD16""250LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF40K1CUNVxJ48_","ASM1SBWSD16""250LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF40K1CUNVxJ96_","ASM1SBWSD16""250LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF40K1CUNVxJ120_","ASM1SBWSD16""250LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF40K1CUNVxJ24_","ASM1SBWSD16""375LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF40K1CUNVxJ48_","ASM1SBWSD16""375LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF40K1CUNVxJ96_","ASM1SBWSD16""375LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF40K1CUNVxJ120_","ASM1SBWSD16""375LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF40K1CUNVxJ24_","ASM1SBWSD16""500LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF40K1CUNVxJ48_","ASM1SBWSD16""500LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF40K1CUNVxJ96_","ASM1SBWSD16""500LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF40K1CUNVxJ120_","ASM1SBWSD16""500LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF40K1CUNVxJ24_","ASM1SBWSD16""625LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF40K1CUNVxJ48_","ASM1SBWSD16""625LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF40K1CUNVxJ96_","ASM1SBWSD16""625LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF40K1CUNVxJ120_","ASM1SBWSD16""625LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF40K1CUNVxJ24_","ASM1SBWSD16""800LF40K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF40K1CUNVxJ48_","ASM1SBWSD16""800LF40K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF40K1CUNVxJ96_","ASM1SBWSD16""800LF40K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF40K1CUNVxJ120_","ASM1SBWSD16""800LF40K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF40K1CUNVxJ24_","ASM1SDCSD8""125LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF40K1CUNVxJ48_","ASM1SDCSD8""125LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF40K1CUNVxJ96_","ASM1SDCSD8""125LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF40K1CUNVxJ120_","ASM1SDCSD8""125LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF40K1CUNVxJ24_","ASM1SDCSD8""250LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF40K1CUNVxJ48_","ASM1SDCSD8""250LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF40K1CUNVxJ96_","ASM1SDCSD8""250LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF40K1CUNVxJ120_","ASM1SDCSD8""250LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF40K1CUNVxJ24_","ASM1SDCSD8""375LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF40K1CUNVxJ48_","ASM1SDCSD8""375LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF40K1CUNVxJ96_","ASM1SDCSD8""375LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF40K1CUNVxJ120_","ASM1SDCSD8""375LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF40K1CUNVxJ24_","ASM1SDCSD8""500LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF40K1CUNVxJ48_","ASM1SDCSD8""500LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF40K1CUNVxJ96_","ASM1SDCSD8""500LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF40K1CUNVxJ120_","ASM1SDCSD8""500LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF40K1CUNVxJ24_","ASM1SDCSD8""625LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF40K1CUNVxJ48_","ASM1SDCSD8""625LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF40K1CUNVxJ96_","ASM1SDCSD8""625LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF40K1CUNVxJ120_","ASM1SDCSD8""625LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF40K1CUNVxJ24_","ASM1SDCSD8""800LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF40K1CUNVxJ48_","ASM1SDCSD8""800LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF40K1CUNVxJ96_","ASM1SDCSD8""800LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF40K1CUNVxJ120_","ASM1SDCSD8""800LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF40K1CUNVxJ24_","ASM1SDCSD12""125LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF40K1CUNVxJ48_","ASM1SDCSD12""125LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF40K1CUNVxJ96_","ASM1SDCSD12""125LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF40K1CUNVxJ120_","ASM1SDCSD12""125LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF40K1CUNVxJ24_","ASM1SDCSD12""250LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF40K1CUNVxJ48_","ASM1SDCSD12""250LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF40K1CUNVxJ96_","ASM1SDCSD12""250LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF40K1CUNVxJ120_","ASM1SDCSD12""250LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF40K1CUNVxJ24_","ASM1SDCSD12""375LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF40K1CUNVxJ48_","ASM1SDCSD12""375LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF40K1CUNVxJ96_","ASM1SDCSD12""375LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF40K1CUNVxJ120_","ASM1SDCSD12""375LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF40K1CUNVxJ24_","ASM1SDCSD12""500LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF40K1CUNVxJ48_","ASM1SDCSD12""500LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF40K1CUNVxJ96_","ASM1SDCSD12""500LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF40K1CUNVxJ120_","ASM1SDCSD12""500LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF40K1CUNVxJ24_","ASM1SDCSD12""625LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF40K1CUNVxJ48_","ASM1SDCSD12""625LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF40K1CUNVxJ96_","ASM1SDCSD12""625LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF40K1CUNVxJ120_","ASM1SDCSD12""625LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF40K1CUNVxJ24_","ASM1SDCSD12""800LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF40K1CUNVxJ48_","ASM1SDCSD12""800LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF40K1CUNVxJ96_","ASM1SDCSD12""800LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF40K1CUNVxJ120_","ASM1SDCSD12""800LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF40K1CUNVxJ24_","ASM1SDCSD16""125LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF40K1CUNVxJ48_","ASM1SDCSD16""125LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF40K1CUNVxJ96_","ASM1SDCSD16""125LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF40K1CUNVxJ120_","ASM1SDCSD16""125LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF40K1CUNVxJ24_","ASM1SDCSD16""250LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF40K1CUNVxJ48_","ASM1SDCSD16""250LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF40K1CUNVxJ96_","ASM1SDCSD16""250LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF40K1CUNVxJ120_","ASM1SDCSD16""250LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF40K1CUNVxJ24_","ASM1SDCSD16""375LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF40K1CUNVxJ48_","ASM1SDCSD16""375LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF40K1CUNVxJ96_","ASM1SDCSD16""375LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF40K1CUNVxJ120_","ASM1SDCSD16""375LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF40K1CUNVxJ24_","ASM1SDCSD16""500LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF40K1CUNVxJ48_","ASM1SDCSD16""500LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF40K1CUNVxJ96_","ASM1SDCSD16""500LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF40K1CUNVxJ120_","ASM1SDCSD16""500LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF40K1CUNVxJ24_","ASM1SDCSD16""625LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF40K1CUNVxJ48_","ASM1SDCSD16""625LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF40K1CUNVxJ96_","ASM1SDCSD16""625LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF40K1CUNVxJ120_","ASM1SDCSD16""625LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF40K1CUNVxJ24_","ASM1SDCSD16""800LF40K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF40K1CUNVxJ48_","ASM1SDCSD16""800LF40K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF40K1CUNVxJ96_","ASM1SDCSD16""800LF40K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF40K1CUNVxJ120_","ASM1SDCSD16""800LF40K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 80+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF940K1CUNVxJ24_","ASM1SBWSD8""125LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF940K1CUNVxJ48_","ASM1SBWSD8""125LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF940K1CUNVxJ96_","ASM1SBWSD8""125LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""125LF940K1CUNVxJ120_","ASM1SBWSD8""125LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF940K1CUNVxJ24_","ASM1SBWSD8""250LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF940K1CUNVxJ48_","ASM1SBWSD8""250LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF940K1CUNVxJ96_","ASM1SBWSD8""250LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""250LF940K1CUNVxJ120_","ASM1SBWSD8""250LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF940K1CUNVxJ24_","ASM1SBWSD8""375LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF940K1CUNVxJ48_","ASM1SBWSD8""375LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF940K1CUNVxJ96_","ASM1SBWSD8""375LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""375LF940K1CUNVxJ120_","ASM1SBWSD8""375LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF940K1CUNVxJ24_","ASM1SBWSD8""500LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF940K1CUNVxJ48_","ASM1SBWSD8""500LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF940K1CUNVxJ96_","ASM1SBWSD8""500LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""500LF940K1CUNVxJ120_","ASM1SBWSD8""500LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF940K1CUNVxJ24_","ASM1SBWSD8""625LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF940K1CUNVxJ48_","ASM1SBWSD8""625LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF940K1CUNVxJ96_","ASM1SBWSD8""625LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""625LF940K1CUNVxJ120_","ASM1SBWSD8""625LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF940K1CUNVxJ24_","ASM1SBWSD8""800LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF940K1CUNVxJ48_","ASM1SBWSD8""800LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF940K1CUNVxJ96_","ASM1SBWSD8""800LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD8""800LF940K1CUNVxJ120_","ASM1SBWSD8""800LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF940K1CUNVxJ24_","ASM1SBWSD12""125LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF940K1CUNVxJ48_","ASM1SBWSD12""125LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF940K1CUNVxJ96_","ASM1SBWSD12""125LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""125LF940K1CUNVxJ120_","ASM1SBWSD12""125LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF940K1CUNVxJ24_","ASM1SBWSD12""250LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF940K1CUNVxJ48_","ASM1SBWSD12""250LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF940K1CUNVxJ96_","ASM1SBWSD12""250LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""250LF940K1CUNVxJ120_","ASM1SBWSD12""250LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF940K1CUNVxJ24_","ASM1SBWSD12""375LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF940K1CUNVxJ48_","ASM1SBWSD12""375LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF940K1CUNVxJ96_","ASM1SBWSD12""375LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""375LF940K1CUNVxJ120_","ASM1SBWSD12""375LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF940K1CUNVxJ24_","ASM1SBWSD12""500LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF940K1CUNVxJ48_","ASM1SBWSD12""500LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF940K1CUNVxJ96_","ASM1SBWSD12""500LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""500LF940K1CUNVxJ120_","ASM1SBWSD12""500LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF940K1CUNVxJ24_","ASM1SBWSD12""625LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF940K1CUNVxJ48_","ASM1SBWSD12""625LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF940K1CUNVxJ96_","ASM1SBWSD12""625LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""625LF940K1CUNVxJ120_","ASM1SBWSD12""625LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF940K1CUNVxJ24_","ASM1SBWSD12""800LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF940K1CUNVxJ48_","ASM1SBWSD12""800LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF940K1CUNVxJ96_","ASM1SBWSD12""800LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD12""800LF940K1CUNVxJ120_","ASM1SBWSD12""800LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF940K1CUNVxJ24_","ASM1SBWSD16""125LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF940K1CUNVxJ48_","ASM1SBWSD16""125LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF940K1CUNVxJ96_","ASM1SBWSD16""125LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""125LF940K1CUNVxJ120_","ASM1SBWSD16""125LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-DCSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF940K1CUNVxJ24_","ASM1SBWSD16""250LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF940K1CUNVxJ48_","ASM1SBWSD16""250LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF940K1CUNVxJ96_","ASM1SBWSD16""250LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""250LF940K1CUNVxJ120_","ASM1SBWSD16""250LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-DCSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF940K1CUNVxJ24_","ASM1SBWSD16""375LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF940K1CUNVxJ48_","ASM1SBWSD16""375LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF940K1CUNVxJ96_","ASM1SBWSD16""375LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""375LF940K1CUNVxJ120_","ASM1SBWSD16""375LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-DCSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF940K1CUNVxJ24_","ASM1SBWSD16""500LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF940K1CUNVxJ48_","ASM1SBWSD16""500LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF940K1CUNVxJ96_","ASM1SBWSD16""500LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""500LF940K1CUNVxJ120_","ASM1SBWSD16""500LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-DCSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF940K1CUNVxJ24_","ASM1SBWSD16""625LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF940K1CUNVxJ48_","ASM1SBWSD16""625LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF940K1CUNVxJ96_","ASM1SBWSD16""625LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""625LF940K1CUNVxJ120_","ASM1SBWSD16""625LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-DCSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF940K1CUNVxJ24_","ASM1SBWSD16""800LF940K1CUNVxJ24_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF940K1CUNVxJ48_","ASM1SBWSD16""800LF940K1CUNVxJ48_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF940K1CUNVxJ96_","ASM1SBWSD16""800LF940K1CUNVxJ96_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SBWSD16""800LF940K1CUNVxJ120_","ASM1SBWSD16""800LF940K1CUNVxJ120_",Batwing Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-DCSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF940K1CUNVxJ24_","ASM1SDCSD8""125LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF940K1CUNVxJ48_","ASM1SDCSD8""125LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF940K1CUNVxJ96_","ASM1SDCSD8""125LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""125LF940K1CUNVxJ120_","ASM1SDCSD8""125LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF940K1CUNVxJ24_","ASM1SDCSD8""250LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF940K1CUNVxJ48_","ASM1SDCSD8""250LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF940K1CUNVxJ96_","ASM1SDCSD8""250LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""250LF940K1CUNVxJ120_","ASM1SDCSD8""250LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF940K1CUNVxJ24_","ASM1SDCSD8""375LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF940K1CUNVxJ48_","ASM1SDCSD8""375LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF940K1CUNVxJ96_","ASM1SDCSD8""375LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""375LF940K1CUNVxJ120_","ASM1SDCSD8""375LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF940K1CUNVxJ24_","ASM1SDCSD8""500LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF940K1CUNVxJ48_","ASM1SDCSD8""500LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF940K1CUNVxJ96_","ASM1SDCSD8""500LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""500LF940K1CUNVxJ120_","ASM1SDCSD8""500LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF940K1CUNVxJ24_","ASM1SDCSD8""625LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF940K1CUNVxJ48_","ASM1SDCSD8""625LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF940K1CUNVxJ96_","ASM1SDCSD8""625LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""625LF940K1CUNVxJ120_","ASM1SDCSD8""625LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF940K1CUNVxJ24_","ASM1SDCSD8""800LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF940K1CUNVxJ48_","ASM1SDCSD8""800LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF940K1CUNVxJ96_","ASM1SDCSD8""800LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD8""800LF940K1CUNVxJ120_","ASM1SDCSD8""800LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,8,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF940K1CUNVxJ24_","ASM1SDCSD12""125LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF940K1CUNVxJ48_","ASM1SDCSD12""125LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF940K1CUNVxJ96_","ASM1SDCSD12""125LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""125LF940K1CUNVxJ120_","ASM1SDCSD12""125LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF940K1CUNVxJ24_","ASM1SDCSD12""250LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF940K1CUNVxJ48_","ASM1SDCSD12""250LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF940K1CUNVxJ96_","ASM1SDCSD12""250LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""250LF940K1CUNVxJ120_","ASM1SDCSD12""250LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF940K1CUNVxJ24_","ASM1SDCSD12""375LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF940K1CUNVxJ48_","ASM1SDCSD12""375LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF940K1CUNVxJ96_","ASM1SDCSD12""375LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""375LF940K1CUNVxJ120_","ASM1SDCSD12""375LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF940K1CUNVxJ24_","ASM1SDCSD12""500LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF940K1CUNVxJ48_","ASM1SDCSD12""500LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF940K1CUNVxJ96_","ASM1SDCSD12""500LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""500LF940K1CUNVxJ120_","ASM1SDCSD12""500LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF940K1CUNVxJ24_","ASM1SDCSD12""625LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF940K1CUNVxJ48_","ASM1SDCSD12""625LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF940K1CUNVxJ96_","ASM1SDCSD12""625LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""625LF940K1CUNVxJ120_","ASM1SDCSD12""625LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF940K1CUNVxJ24_","ASM1SDCSD12""800LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF940K1CUNVxJ48_","ASM1SDCSD12""800LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF940K1CUNVxJ96_","ASM1SDCSD12""800LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD12""800LF940K1CUNVxJ120_","ASM1SDCSD12""800LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,12,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF940K1CUNVxJ24_","ASM1SDCSD16""125LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",125,120,17.85714286,24,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF940K1CUNVxJ48_","ASM1SDCSD16""125LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",125,120,17.85714286,48,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF940K1CUNVxJ96_","ASM1SDCSD16""125LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",125,120,17.85714286,96,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""125LF940K1CUNVxJ120_","ASM1SDCSD16""125LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,"Indirect Distribution 125 Lumens per foot 4' minimum, Consult factory for Lutron and DALI",4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",125,120,17.85714286,120,7,7 Watts per foot,ASM1S-BWSD-125LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF940K1CUNVxJ24_","ASM1SDCSD16""250LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",250,120,31.25,24,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF940K1CUNVxJ48_","ASM1SDCSD16""250LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",250,120,31.25,48,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF940K1CUNVxJ96_","ASM1SDCSD16""250LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",250,120,31.25,96,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""250LF940K1CUNVxJ120_","ASM1SDCSD16""250LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 250 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",250,120,31.25,120,8,8 Watts per foot,ASM1S-BWSD-250LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF940K1CUNVxJ24_","ASM1SDCSD16""375LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",375,120,31.25,24,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF940K1CUNVxJ48_","ASM1SDCSD16""375LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",375,120,31.25,48,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF940K1CUNVxJ96_","ASM1SDCSD16""375LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",375,120,31.25,96,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""375LF940K1CUNVxJ120_","ASM1SDCSD16""375LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 375 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",375,120,31.25,120,12,12 Watts per foot,ASM1S-BWSD-375LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF940K1CUNVxJ24_","ASM1SDCSD16""500LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",500,120,33.33333333,24,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF940K1CUNVxJ48_","ASM1SDCSD16""500LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",500,120,33.33333333,48,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF940K1CUNVxJ96_","ASM1SDCSD16""500LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",500,120,33.33333333,96,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""500LF940K1CUNVxJ120_","ASM1SDCSD16""500LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 500 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",500,120,33.33333333,120,15,15 Watts per foot,ASM1S-BWSD-500LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF940K1CUNVxJ24_","ASM1SDCSD16""625LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",625,120,34.72222222,24,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF940K1CUNVxJ48_","ASM1SDCSD16""625LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",625,120,34.72222222,48,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF940K1CUNVxJ96_","ASM1SDCSD16""625LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",625,120,34.72222222,96,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""625LF940K1CUNVxJ120_","ASM1SDCSD16""625LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 625 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",625,120,34.72222222,120,18,18 Watts per foot,ASM1S-BWSD-625LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF940K1CUNVxJ24_","ASM1SDCSD16""800LF940K1CUNVxJ24_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"24"" Cable Suspension",800,120,33.33333333,24,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF940K1CUNVxJ48_","ASM1SDCSD16""800LF940K1CUNVxJ48_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"48"" Cable Suspension",800,120,33.33333333,48,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF940K1CUNVxJ96_","ASM1SDCSD16""800LF940K1CUNVxJ96_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"96"" Cable Suspension",800,120,33.33333333,96,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
"ASM1SDCSD16""800LF940K1CUNVxJ120_","ASM1SDCSD16""800LF940K1CUNVxJ120_",Dust Cover Top/Solid Bottom,16,Indirect Distribution 800 Lumens per foot,4000,"4000K, 90+ CRI",Single Circuit,120/277 UNV Volt,Please Contact Manufacturer for Driver Information,"120"" Cable Suspension",800,120,33.33333333,120,24,24 Watts per foot,ASM1S-BWSD-800LF-35K-1C-UNV-4.ies,N/A
