,Model##OTHER##,Shielding Type##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Color Temperature Note##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Driver##Other##,Circuit##OTHER##,Mounting##Other##,Cable Suspension##Length##Inches,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Photometric Web File##OTHER##,Driver Comment##OTHER##,Voltage Comment##OTHER##,Lumen Output Comment##OTHER##,Constraints##OTHER##
ASM1TIP4BW8750L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW8750L30K1CUNVLD1J24TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW8750L30K1CUNVLD1J48TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW8750L30K1CUNVLD1J96TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW8750L30K1CUNVLD1J120TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW8750L930K1CUNVLD1J24TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW8750L930K1CUNVLD1J48TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW8750L930K1CUNVLD1J96TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW8750L930K1CUNVLD1J120TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW8750L35K1CUNVLD1J24TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW8750L35K1CUNVLD1J48TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW8750L35K1CUNVLD1J96TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW8750L35K1CUNVLD1J120TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW8750L935K1CUNVLD1J24TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW8750L935K1CUNVLD1J48TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW8750L935K1CUNVLD1J96TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW8750L935K1CUNVLD1J120TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW8750L40K1CUNVLD1J24TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW8750L40K1CUNVLD1J48TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW8750L40K1CUNVLD1J96TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW8750L40K1CUNVLD1J120TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW8750L940K1CUNVLD1J24TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW8750L940K1CUNVLD1J48TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW8750L940K1CUNVLD1J96TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW8750L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW8750L940K1CUNVLD1J120TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4BW12750L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW12750L30K1CUNVLD1J24TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW12750L30K1CUNVLD1J48TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW12750L30K1CUNVLD1J96TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW12750L30K1CUNVLD1J120TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW12750L930K1CUNVLD1J24TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW12750L930K1CUNVLD1J48TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW12750L930K1CUNVLD1J96TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW12750L930K1CUNVLD1J120TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW12750L35K1CUNVLD1J24TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW12750L35K1CUNVLD1J48TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW12750L35K1CUNVLD1J96TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW12750L35K1CUNVLD1J120TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW12750L935K1CUNVLD1J24TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW12750L935K1CUNVLD1J48TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW12750L935K1CUNVLD1J96TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW12750L935K1CUNVLD1J120TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW12750L40K1CUNVLD1J24TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW12750L40K1CUNVLD1J48TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW12750L40K1CUNVLD1J96TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW12750L40K1CUNVLD1J120TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW12750L940K1CUNVLD1J24TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW12750L940K1CUNVLD1J48TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW12750L940K1CUNVLD1J96TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW12750L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW12750L940K1CUNVLD1J120TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4BW16750L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW16750L30K1CUNVLD1J24TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW16750L30K1CUNVLD1J48TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW16750L30K1CUNVLD1J96TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW16750L30K1CUNVLD1J120TSBKCD,Batwing Optic,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW16750L930K1CUNVLD1J24TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW16750L930K1CUNVLD1J48TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW16750L930K1CUNVLD1J96TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW16750L930K1CUNVLD1J120TSBKCD,Batwing Optic,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW16750L35K1CUNVLD1J24TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW16750L35K1CUNVLD1J48TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW16750L35K1CUNVLD1J96TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW16750L35K1CUNVLD1J120TSBKCD,Batwing Optic,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW16750L935K1CUNVLD1J24TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW16750L935K1CUNVLD1J48TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW16750L935K1CUNVLD1J96TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW16750L935K1CUNVLD1J120TSBKCD,Batwing Optic,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW16750L40K1CUNVLD1J24TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW16750L40K1CUNVLD1J48TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW16750L40K1CUNVLD1J96TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW16750L40K1CUNVLD1J120TSBKCD,Batwing Optic,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW16750L940K1CUNVLD1J24TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW16750L940K1CUNVLD1J48TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW16750L940K1CUNVLD1J96TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4BW16750L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW16750L940K1CUNVLD1J120TSBKCD,Batwing Optic,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-BW-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC8750L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC8750L30K1CUNVLD1J24TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC8750L30K1CUNVLD1J48TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC8750L30K1CUNVLD1J96TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC8750L30K1CUNVLD1J120TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC8750L930K1CUNVLD1J24TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC8750L930K1CUNVLD1J48TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC8750L930K1CUNVLD1J96TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC8750L930K1CUNVLD1J120TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC8750L35K1CUNVLD1J24TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC8750L35K1CUNVLD1J48TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC8750L35K1CUNVLD1J96TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC8750L35K1CUNVLD1J120TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC8750L935K1CUNVLD1J24TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC8750L935K1CUNVLD1J48TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC8750L935K1CUNVLD1J96TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC8750L935K1CUNVLD1J120TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC8750L40K1CUNVLD1J24TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC8750L40K1CUNVLD1J48TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC8750L40K1CUNVLD1J96TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC8750L40K1CUNVLD1J120TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC8750L940K1CUNVLD1J24TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC8750L940K1CUNVLD1J48TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC8750L940K1CUNVLD1J96TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC8750L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC8750L940K1CUNVLD1J120TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,48
ASM1TIP4DC12750L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC12750L30K1CUNVLD1J24TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC12750L30K1CUNVLD1J48TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC12750L30K1CUNVLD1J96TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC12750L30K1CUNVLD1J120TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC12750L930K1CUNVLD1J24TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC12750L930K1CUNVLD1J48TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC12750L930K1CUNVLD1J96TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC12750L930K1CUNVLD1J120TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC12750L35K1CUNVLD1J24TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC12750L35K1CUNVLD1J48TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC12750L35K1CUNVLD1J96TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC12750L35K1CUNVLD1J120TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC12750L935K1CUNVLD1J24TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC12750L935K1CUNVLD1J48TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC12750L935K1CUNVLD1J96TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC12750L935K1CUNVLD1J120TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC12750L40K1CUNVLD1J24TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC12750L40K1CUNVLD1J48TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC12750L40K1CUNVLD1J96TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC12750L40K1CUNVLD1J120TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC12750L940K1CUNVLD1J24TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC12750L940K1CUNVLD1J48TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC12750L940K1CUNVLD1J96TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC12750L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC12750L940K1CUNVLD1J120TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,412
ASM1TIP4DC16750L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC16750L30K1CUNVLD1J24TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC16750L30K1CUNVLD1J48TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC16750L30K1CUNVLD1J96TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC16750L30K1CUNVLD1J120TSBKCD,Dust Cover,750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC16750L930K1CUNVLD1J24TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC16750L930K1CUNVLD1J48TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC16750L930K1CUNVLD1J96TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC16750L930K1CUNVLD1J120TSBKCD,Dust Cover,750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC16750L35K1CUNVLD1J24TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC16750L35K1CUNVLD1J48TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC16750L35K1CUNVLD1J96TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC16750L35K1CUNVLD1J120TSBKCD,Dust Cover,750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC16750L935K1CUNVLD1J24TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC16750L935K1CUNVLD1J48TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC16750L935K1CUNVLD1J96TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC16750L935K1CUNVLD1J120TSBKCD,Dust Cover,750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC16750L40K1CUNVLD1J24TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC16750L40K1CUNVLD1J48TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC16750L40K1CUNVLD1J96TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC16750L40K1CUNVLD1J120TSBKCD,Dust Cover,750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC16750L940K1CUNVLD1J24TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC16750L940K1CUNVLD1J48TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC16750L940K1CUNVLD1J96TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP4DC16750L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC16750L940K1CUNVLD1J120TSBKCD,Dust Cover,750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,6.6,6.6 Watts,ASM1TIP-4-DC-750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 750 Lumens,416
ASM1TIP6BW81125L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW81125L30K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW81125L30K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW81125L30K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW81125L30K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW81125L930K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW81125L930K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW81125L930K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW81125L930K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW81125L35K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW81125L35K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW81125L35K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW81125L35K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW81125L935K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW81125L935K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW81125L935K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW81125L935K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW81125L40K1CUNVLD1J24TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW81125L40K1CUNVLD1J48TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW81125L40K1CUNVLD1J96TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW81125L40K1CUNVLD1J120TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW81125L940K1CUNVLD1J24TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW81125L940K1CUNVLD1J48TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW81125L940K1CUNVLD1J96TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW81125L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW81125L940K1CUNVLD1J120TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6BW121125L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW121125L30K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW121125L30K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW121125L30K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW121125L30K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW121125L930K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW121125L930K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW121125L930K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW121125L930K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW121125L35K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW121125L35K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW121125L35K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW121125L35K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW121125L935K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW121125L935K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW121125L935K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW121125L935K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW121125L40K1CUNVLD1J24TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW121125L40K1CUNVLD1J48TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW121125L40K1CUNVLD1J96TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW121125L40K1CUNVLD1J120TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW121125L940K1CUNVLD1J24TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW121125L940K1CUNVLD1J48TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW121125L940K1CUNVLD1J96TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW121125L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW121125L940K1CUNVLD1J120TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6BW161125L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW161125L30K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW161125L30K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW161125L30K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW161125L30K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW161125L930K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW161125L930K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW161125L930K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW161125L930K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW161125L35K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW161125L35K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW161125L35K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW161125L35K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW161125L935K1CUNVLD1J24TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW161125L935K1CUNVLD1J48TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW161125L935K1CUNVLD1J96TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW161125L935K1CUNVLD1J120TSBKCD,Batwing Optic,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW161125L40K1CUNVLD1J24TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW161125L40K1CUNVLD1J48TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW161125L40K1CUNVLD1J96TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW161125L40K1CUNVLD1J120TSBKCD,Batwing Optic,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW161125L940K1CUNVLD1J24TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW161125L940K1CUNVLD1J48TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW161125L940K1CUNVLD1J96TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6BW161125L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW161125L940K1CUNVLD1J120TSBKCD,Batwing Optic,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-BW-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC81125L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC81125L30K1CUNVLD1J24TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC81125L30K1CUNVLD1J48TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC81125L30K1CUNVLD1J96TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC81125L30K1CUNVLD1J120TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC81125L930K1CUNVLD1J24TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC81125L930K1CUNVLD1J48TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC81125L930K1CUNVLD1J96TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC81125L930K1CUNVLD1J120TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC81125L35K1CUNVLD1J24TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC81125L35K1CUNVLD1J48TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC81125L35K1CUNVLD1J96TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC81125L35K1CUNVLD1J120TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC81125L935K1CUNVLD1J24TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC81125L935K1CUNVLD1J48TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC81125L935K1CUNVLD1J96TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC81125L935K1CUNVLD1J120TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC81125L40K1CUNVLD1J24TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC81125L40K1CUNVLD1J48TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC81125L40K1CUNVLD1J96TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC81125L40K1CUNVLD1J120TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC81125L940K1CUNVLD1J24TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC81125L940K1CUNVLD1J48TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC81125L940K1CUNVLD1J96TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC81125L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC81125L940K1CUNVLD1J120TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,68
ASM1TIP6DC121125L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC121125L30K1CUNVLD1J24TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC121125L30K1CUNVLD1J48TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC121125L30K1CUNVLD1J96TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC121125L30K1CUNVLD1J120TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC121125L930K1CUNVLD1J24TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC121125L930K1CUNVLD1J48TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC121125L930K1CUNVLD1J96TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC121125L930K1CUNVLD1J120TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC121125L35K1CUNVLD1J24TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC121125L35K1CUNVLD1J48TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC121125L35K1CUNVLD1J96TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC121125L35K1CUNVLD1J120TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC121125L935K1CUNVLD1J24TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC121125L935K1CUNVLD1J48TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC121125L935K1CUNVLD1J96TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC121125L935K1CUNVLD1J120TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC121125L40K1CUNVLD1J24TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC121125L40K1CUNVLD1J48TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC121125L40K1CUNVLD1J96TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC121125L40K1CUNVLD1J120TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC121125L940K1CUNVLD1J24TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC121125L940K1CUNVLD1J48TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC121125L940K1CUNVLD1J96TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC121125L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC121125L940K1CUNVLD1J120TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,612
ASM1TIP6DC161125L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC161125L30K1CUNVLD1J24TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC161125L30K1CUNVLD1J48TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC161125L30K1CUNVLD1J96TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC161125L30K1CUNVLD1J120TSBKCD,Dust Cover,1125,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC161125L930K1CUNVLD1J24TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC161125L930K1CUNVLD1J48TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC161125L930K1CUNVLD1J96TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC161125L930K1CUNVLD1J120TSBKCD,Dust Cover,1125,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC161125L35K1CUNVLD1J24TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC161125L35K1CUNVLD1J48TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC161125L35K1CUNVLD1J96TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC161125L35K1CUNVLD1J120TSBKCD,Dust Cover,1125,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC161125L935K1CUNVLD1J24TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC161125L935K1CUNVLD1J48TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC161125L935K1CUNVLD1J96TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC161125L935K1CUNVLD1J120TSBKCD,Dust Cover,1125,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC161125L40K1CUNVLD1J24TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC161125L40K1CUNVLD1J48TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC161125L40K1CUNVLD1J96TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC161125L40K1CUNVLD1J120TSBKCD,Dust Cover,1125,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC161125L940K1CUNVLD1J24TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC161125L940K1CUNVLD1J48TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC161125L940K1CUNVLD1J96TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP6DC161125L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC161125L940K1CUNVLD1J120TSBKCD,Dust Cover,1125,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,8.5,8.5 Watts,ASM1TIP-6-DC-1125L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1125 Lumens,616
ASM1TIP4BW81500L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW81500L30K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW81500L30K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW81500L30K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW81500L30K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW81500L930K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW81500L930K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW81500L930K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW81500L930K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW81500L35K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW81500L35K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW81500L35K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW81500L35K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW81500L935K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW81500L935K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW81500L935K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW81500L935K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW81500L40K1CUNVLD1J24TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW81500L40K1CUNVLD1J48TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW81500L40K1CUNVLD1J96TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW81500L40K1CUNVLD1J120TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW81500L940K1CUNVLD1J24TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW81500L940K1CUNVLD1J48TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW81500L940K1CUNVLD1J96TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW81500L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW81500L940K1CUNVLD1J120TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4BW121500L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW121500L30K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW121500L30K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW121500L30K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW121500L30K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW121500L930K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW121500L930K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW121500L930K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW121500L930K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW121500L35K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW121500L35K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW121500L35K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW121500L35K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW121500L935K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW121500L935K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW121500L935K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW121500L935K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW121500L40K1CUNVLD1J24TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW121500L40K1CUNVLD1J48TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW121500L40K1CUNVLD1J96TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW121500L40K1CUNVLD1J120TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW121500L940K1CUNVLD1J24TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW121500L940K1CUNVLD1J48TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW121500L940K1CUNVLD1J96TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW121500L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW121500L940K1CUNVLD1J120TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4BW161500L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW161500L30K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW161500L30K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW161500L30K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW161500L30K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW161500L930K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW161500L930K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW161500L930K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW161500L930K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW161500L35K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW161500L35K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW161500L35K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW161500L35K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW161500L935K1CUNVLD1J24TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW161500L935K1CUNVLD1J48TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW161500L935K1CUNVLD1J96TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW161500L935K1CUNVLD1J120TSBKCD,Batwing Optic,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW161500L40K1CUNVLD1J24TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW161500L40K1CUNVLD1J48TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW161500L40K1CUNVLD1J96TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW161500L40K1CUNVLD1J120TSBKCD,Batwing Optic,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW161500L940K1CUNVLD1J24TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW161500L940K1CUNVLD1J48TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW161500L940K1CUNVLD1J96TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4BW161500L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW161500L940K1CUNVLD1J120TSBKCD,Batwing Optic,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-BW-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC81500L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC81500L30K1CUNVLD1J24TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC81500L30K1CUNVLD1J48TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC81500L30K1CUNVLD1J96TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC81500L30K1CUNVLD1J120TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC81500L930K1CUNVLD1J24TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC81500L930K1CUNVLD1J48TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC81500L930K1CUNVLD1J96TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC81500L930K1CUNVLD1J120TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC81500L35K1CUNVLD1J24TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC81500L35K1CUNVLD1J48TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC81500L35K1CUNVLD1J96TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC81500L35K1CUNVLD1J120TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC81500L935K1CUNVLD1J24TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC81500L935K1CUNVLD1J48TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC81500L935K1CUNVLD1J96TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC81500L935K1CUNVLD1J120TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC81500L40K1CUNVLD1J24TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC81500L40K1CUNVLD1J48TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC81500L40K1CUNVLD1J96TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC81500L40K1CUNVLD1J120TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC81500L940K1CUNVLD1J24TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC81500L940K1CUNVLD1J48TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC81500L940K1CUNVLD1J96TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC81500L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC81500L940K1CUNVLD1J120TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,48
ASM1TIP4DC121500L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC121500L30K1CUNVLD1J24TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC121500L30K1CUNVLD1J48TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC121500L30K1CUNVLD1J96TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC121500L30K1CUNVLD1J120TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC121500L930K1CUNVLD1J24TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC121500L930K1CUNVLD1J48TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC121500L930K1CUNVLD1J96TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC121500L930K1CUNVLD1J120TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC121500L35K1CUNVLD1J24TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC121500L35K1CUNVLD1J48TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC121500L35K1CUNVLD1J96TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC121500L35K1CUNVLD1J120TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC121500L935K1CUNVLD1J24TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC121500L935K1CUNVLD1J48TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC121500L935K1CUNVLD1J96TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC121500L935K1CUNVLD1J120TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC121500L40K1CUNVLD1J24TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC121500L40K1CUNVLD1J48TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC121500L40K1CUNVLD1J96TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC121500L40K1CUNVLD1J120TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC121500L940K1CUNVLD1J24TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC121500L940K1CUNVLD1J48TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC121500L940K1CUNVLD1J96TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC121500L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC121500L940K1CUNVLD1J120TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,412
ASM1TIP4DC161500L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC161500L30K1CUNVLD1J24TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC161500L30K1CUNVLD1J48TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC161500L30K1CUNVLD1J96TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC161500L30K1CUNVLD1J120TSBKCD,Dust Cover,1500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC161500L930K1CUNVLD1J24TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC161500L930K1CUNVLD1J48TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC161500L930K1CUNVLD1J96TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC161500L930K1CUNVLD1J120TSBKCD,Dust Cover,1500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC161500L35K1CUNVLD1J24TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC161500L35K1CUNVLD1J48TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC161500L35K1CUNVLD1J96TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC161500L35K1CUNVLD1J120TSBKCD,Dust Cover,1500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC161500L935K1CUNVLD1J24TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC161500L935K1CUNVLD1J48TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC161500L935K1CUNVLD1J96TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC161500L935K1CUNVLD1J120TSBKCD,Dust Cover,1500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC161500L40K1CUNVLD1J24TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC161500L40K1CUNVLD1J48TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC161500L40K1CUNVLD1J96TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC161500L40K1CUNVLD1J120TSBKCD,Dust Cover,1500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC161500L940K1CUNVLD1J24TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC161500L940K1CUNVLD1J48TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC161500L940K1CUNVLD1J96TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP4DC161500L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC161500L940K1CUNVLD1J120TSBKCD,Dust Cover,1500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,11.1,11.1 Watts,ASM1TIP-4-DC-1500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 1500 Lumens,416
ASM1TIP6BW82250L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW82250L30K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW82250L30K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW82250L30K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW82250L30K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW82250L930K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW82250L930K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW82250L930K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW82250L930K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW82250L35K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW82250L35K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW82250L35K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW82250L35K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW82250L935K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW82250L935K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW82250L935K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW82250L935K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW82250L40K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW82250L40K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW82250L40K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW82250L40K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW82250L940K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW82250L940K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW82250L940K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW82250L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW82250L940K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6BW122250L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW122250L30K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW122250L30K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW122250L30K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW122250L30K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW122250L930K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW122250L930K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW122250L930K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW122250L930K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW122250L35K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW122250L35K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW122250L35K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW122250L35K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW122250L935K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW122250L935K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW122250L935K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW122250L935K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW122250L40K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW122250L40K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW122250L40K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW122250L40K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW122250L940K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW122250L940K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW122250L940K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW122250L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW122250L940K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6BW162250L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW162250L30K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW162250L30K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW162250L30K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW162250L30K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW162250L930K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW162250L930K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW162250L930K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW162250L930K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW162250L35K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW162250L35K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW162250L35K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW162250L35K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW162250L935K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW162250L935K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW162250L935K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW162250L935K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW162250L40K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW162250L40K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW162250L40K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW162250L40K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW162250L940K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW162250L940K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW162250L940K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6BW162250L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW162250L940K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC82250L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC82250L30K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC82250L30K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC82250L30K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC82250L30K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC82250L930K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC82250L930K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC82250L930K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC82250L930K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC82250L35K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC82250L35K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC82250L35K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC82250L35K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC82250L935K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC82250L935K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC82250L935K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC82250L935K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC82250L40K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC82250L40K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC82250L40K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC82250L40K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC82250L940K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC82250L940K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC82250L940K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC82250L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC82250L940K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,68
ASM1TIP6DC122250L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC122250L30K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC122250L30K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC122250L30K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC122250L30K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC122250L930K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC122250L930K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC122250L930K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC122250L930K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC122250L35K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC122250L35K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC122250L35K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC122250L35K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC122250L935K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC122250L935K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC122250L935K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC122250L935K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC122250L40K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC122250L40K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC122250L40K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC122250L40K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC122250L940K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC122250L940K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC122250L940K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC122250L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC122250L940K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,612
ASM1TIP6DC162250L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC162250L30K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC162250L30K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC162250L30K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC162250L30K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC162250L930K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC162250L930K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC162250L930K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC162250L930K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC162250L35K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC162250L35K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC162250L35K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC162250L35K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC162250L935K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC162250L935K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC162250L935K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC162250L935K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC162250L40K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC162250L40K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC162250L40K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC162250L40K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC162250L940K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC162250L940K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC162250L940K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP6DC162250L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC162250L940K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,15.2,15.2 Watts,ASM1TIP-6-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,616
ASM1TIP4BW82250L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW82250L30K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW82250L30K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW82250L30K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW82250L30K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW82250L930K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW82250L930K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW82250L930K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW82250L930K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW82250L35K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW82250L35K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW82250L35K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW82250L35K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW82250L935K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW82250L935K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW82250L935K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW82250L935K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW82250L40K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW82250L40K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW82250L40K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW82250L40K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW82250L940K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW82250L940K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW82250L940K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW82250L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW82250L940K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4BW122250L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW122250L30K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW122250L30K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW122250L30K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW122250L30K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW122250L930K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW122250L930K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW122250L930K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW122250L930K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW122250L35K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW122250L35K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW122250L35K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW122250L35K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW122250L935K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW122250L935K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW122250L935K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW122250L935K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW122250L40K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW122250L40K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW122250L40K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW122250L40K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW122250L940K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW122250L940K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW122250L940K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW122250L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW122250L940K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4BW162250L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW162250L30K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW162250L30K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW162250L30K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW162250L30K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW162250L930K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW162250L930K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW162250L930K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW162250L930K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW162250L35K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW162250L35K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW162250L35K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW162250L35K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW162250L935K1CUNVLD1J24TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW162250L935K1CUNVLD1J48TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW162250L935K1CUNVLD1J96TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW162250L935K1CUNVLD1J120TSBKCD,Batwing Optic,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW162250L40K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW162250L40K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW162250L40K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW162250L40K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW162250L940K1CUNVLD1J24TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW162250L940K1CUNVLD1J48TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW162250L940K1CUNVLD1J96TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW162250L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW162250L940K1CUNVLD1J120TSBKCD,Batwing Optic,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-BW-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC82250L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC82250L30K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC82250L30K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC82250L30K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC82250L30K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC82250L930K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC82250L930K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC82250L930K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC82250L930K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC82250L35K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC82250L35K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC82250L35K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC82250L35K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC82250L935K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC82250L935K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC82250L935K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC82250L935K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC82250L40K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC82250L40K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC82250L40K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC82250L40K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC82250L940K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC82250L940K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC82250L940K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC82250L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC82250L940K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,48
ASM1TIP4DC122250L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC122250L30K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC122250L30K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC122250L30K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC122250L30K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC122250L930K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC122250L930K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC122250L930K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC122250L930K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC122250L35K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC122250L35K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC122250L35K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC122250L35K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC122250L935K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC122250L935K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC122250L935K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC122250L935K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC122250L40K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC122250L40K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC122250L40K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC122250L40K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC122250L940K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC122250L940K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC122250L940K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC122250L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC122250L940K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,412
ASM1TIP4DC162250L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC162250L30K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC162250L30K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC162250L30K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC162250L30K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC162250L930K1CUNVLD1J24TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC162250L930K1CUNVLD1J48TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC162250L930K1CUNVLD1J96TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC162250L930K1CUNVLD1J120TSBKCD,Dust Cover,2250,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC162250L35K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC162250L35K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC162250L35K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC162250L35K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC162250L935K1CUNVLD1J24TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC162250L935K1CUNVLD1J48TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC162250L935K1CUNVLD1J96TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC162250L935K1CUNVLD1J120TSBKCD,Dust Cover,2250,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC162250L40K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC162250L40K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC162250L40K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC162250L40K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC162250L940K1CUNVLD1J24TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC162250L940K1CUNVLD1J48TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC162250L940K1CUNVLD1J96TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4DC162250L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC162250L940K1CUNVLD1J120TSBKCD,Dust Cover,2250,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,16.2,16.2 Watts,ASM1TIP-4-DC-2250L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 2250 Lumens,416
ASM1TIP4BW83000L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW83000L30K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW83000L30K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW83000L30K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW83000L30K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW83000L930K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW83000L930K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW83000L930K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW83000L930K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW83000L35K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW83000L35K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW83000L35K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW83000L35K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW83000L935K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW83000L935K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW83000L935K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW83000L935K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW83000L40K1CUNVLD1J24TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW83000L40K1CUNVLD1J48TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW83000L40K1CUNVLD1J96TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW83000L40K1CUNVLD1J120TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW83000L940K1CUNVLD1J24TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW83000L940K1CUNVLD1J48TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW83000L940K1CUNVLD1J96TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW83000L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW83000L940K1CUNVLD1J120TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4BW123000L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW123000L30K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW123000L30K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW123000L30K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW123000L30K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW123000L930K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW123000L930K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW123000L930K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW123000L930K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW123000L35K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW123000L35K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW123000L35K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW123000L35K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW123000L935K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW123000L935K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW123000L935K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW123000L935K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW123000L40K1CUNVLD1J24TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW123000L40K1CUNVLD1J48TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW123000L40K1CUNVLD1J96TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW123000L40K1CUNVLD1J120TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW123000L940K1CUNVLD1J24TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW123000L940K1CUNVLD1J48TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW123000L940K1CUNVLD1J96TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW123000L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW123000L940K1CUNVLD1J120TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4BW163000L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW163000L30K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW163000L30K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW163000L30K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW163000L30K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW163000L930K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW163000L930K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW163000L930K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW163000L930K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW163000L35K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW163000L35K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW163000L35K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW163000L35K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW163000L935K1CUNVLD1J24TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW163000L935K1CUNVLD1J48TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW163000L935K1CUNVLD1J96TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW163000L935K1CUNVLD1J120TSBKCD,Batwing Optic,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW163000L40K1CUNVLD1J24TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW163000L40K1CUNVLD1J48TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW163000L40K1CUNVLD1J96TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW163000L40K1CUNVLD1J120TSBKCD,Batwing Optic,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW163000L940K1CUNVLD1J24TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW163000L940K1CUNVLD1J48TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW163000L940K1CUNVLD1J96TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4BW163000L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW163000L940K1CUNVLD1J120TSBKCD,Batwing Optic,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-BW-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC83000L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC83000L30K1CUNVLD1J24TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC83000L30K1CUNVLD1J48TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC83000L30K1CUNVLD1J96TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC83000L30K1CUNVLD1J120TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC83000L930K1CUNVLD1J24TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC83000L930K1CUNVLD1J48TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC83000L930K1CUNVLD1J96TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC83000L930K1CUNVLD1J120TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC83000L35K1CUNVLD1J24TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC83000L35K1CUNVLD1J48TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC83000L35K1CUNVLD1J96TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC83000L35K1CUNVLD1J120TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC83000L935K1CUNVLD1J24TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC83000L935K1CUNVLD1J48TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC83000L935K1CUNVLD1J96TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC83000L935K1CUNVLD1J120TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC83000L40K1CUNVLD1J24TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC83000L40K1CUNVLD1J48TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC83000L40K1CUNVLD1J96TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC83000L40K1CUNVLD1J120TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC83000L940K1CUNVLD1J24TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC83000L940K1CUNVLD1J48TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC83000L940K1CUNVLD1J96TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC83000L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC83000L940K1CUNVLD1J120TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,48
ASM1TIP4DC123000L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC123000L30K1CUNVLD1J24TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC123000L30K1CUNVLD1J48TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC123000L30K1CUNVLD1J96TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC123000L30K1CUNVLD1J120TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC123000L930K1CUNVLD1J24TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC123000L930K1CUNVLD1J48TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC123000L930K1CUNVLD1J96TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC123000L930K1CUNVLD1J120TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC123000L35K1CUNVLD1J24TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC123000L35K1CUNVLD1J48TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC123000L35K1CUNVLD1J96TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC123000L35K1CUNVLD1J120TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC123000L935K1CUNVLD1J24TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC123000L935K1CUNVLD1J48TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC123000L935K1CUNVLD1J96TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC123000L935K1CUNVLD1J120TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC123000L40K1CUNVLD1J24TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC123000L40K1CUNVLD1J48TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC123000L40K1CUNVLD1J96TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC123000L40K1CUNVLD1J120TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC123000L940K1CUNVLD1J24TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC123000L940K1CUNVLD1J48TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC123000L940K1CUNVLD1J96TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC123000L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC123000L940K1CUNVLD1J120TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,412
ASM1TIP4DC163000L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC163000L30K1CUNVLD1J24TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC163000L30K1CUNVLD1J48TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC163000L30K1CUNVLD1J96TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC163000L30K1CUNVLD1J120TSBKCD,Dust Cover,3000,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC163000L930K1CUNVLD1J24TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC163000L930K1CUNVLD1J48TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC163000L930K1CUNVLD1J96TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC163000L930K1CUNVLD1J120TSBKCD,Dust Cover,3000,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC163000L35K1CUNVLD1J24TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC163000L35K1CUNVLD1J48TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC163000L35K1CUNVLD1J96TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC163000L35K1CUNVLD1J120TSBKCD,Dust Cover,3000,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC163000L935K1CUNVLD1J24TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC163000L935K1CUNVLD1J48TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC163000L935K1CUNVLD1J96TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC163000L935K1CUNVLD1J120TSBKCD,Dust Cover,3000,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC163000L40K1CUNVLD1J24TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC163000L40K1CUNVLD1J48TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC163000L40K1CUNVLD1J96TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC163000L40K1CUNVLD1J120TSBKCD,Dust Cover,3000,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC163000L940K1CUNVLD1J24TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC163000L940K1CUNVLD1J48TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC163000L940K1CUNVLD1J96TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP4DC163000L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC163000L940K1CUNVLD1J120TSBKCD,Dust Cover,3000,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,21,21 Watts,ASM1TIP-4-DC-3000L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3000 Lumens,416
ASM1TIP6BW83375L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW83375L30K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW83375L30K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW83375L30K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW83375L30K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW83375L930K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW83375L930K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW83375L930K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW83375L930K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW83375L35K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW83375L35K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW83375L35K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW83375L35K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW83375L935K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW83375L935K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW83375L935K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW83375L935K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW83375L40K1CUNVLD1J24TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW83375L40K1CUNVLD1J48TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW83375L40K1CUNVLD1J96TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW83375L40K1CUNVLD1J120TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW83375L940K1CUNVLD1J24TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW83375L940K1CUNVLD1J48TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW83375L940K1CUNVLD1J96TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW83375L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW83375L940K1CUNVLD1J120TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6BW123375L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW123375L30K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW123375L30K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW123375L30K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW123375L30K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW123375L930K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW123375L930K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW123375L930K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW123375L930K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW123375L35K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW123375L35K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW123375L35K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW123375L35K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW123375L935K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW123375L935K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW123375L935K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW123375L935K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW123375L40K1CUNVLD1J24TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW123375L40K1CUNVLD1J48TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW123375L40K1CUNVLD1J96TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW123375L40K1CUNVLD1J120TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW123375L940K1CUNVLD1J24TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW123375L940K1CUNVLD1J48TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW123375L940K1CUNVLD1J96TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW123375L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW123375L940K1CUNVLD1J120TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6BW163375L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW163375L30K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW163375L30K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW163375L30K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW163375L30K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW163375L930K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW163375L930K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW163375L930K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW163375L930K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW163375L35K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW163375L35K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW163375L35K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW163375L35K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW163375L935K1CUNVLD1J24TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW163375L935K1CUNVLD1J48TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW163375L935K1CUNVLD1J96TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW163375L935K1CUNVLD1J120TSBKCD,Batwing Optic,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW163375L40K1CUNVLD1J24TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW163375L40K1CUNVLD1J48TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW163375L40K1CUNVLD1J96TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW163375L40K1CUNVLD1J120TSBKCD,Batwing Optic,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW163375L940K1CUNVLD1J24TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW163375L940K1CUNVLD1J48TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW163375L940K1CUNVLD1J96TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6BW163375L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW163375L940K1CUNVLD1J120TSBKCD,Batwing Optic,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-BW-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC83375L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC83375L30K1CUNVLD1J24TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC83375L30K1CUNVLD1J48TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC83375L30K1CUNVLD1J96TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC83375L30K1CUNVLD1J120TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC83375L930K1CUNVLD1J24TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC83375L930K1CUNVLD1J48TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC83375L930K1CUNVLD1J96TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC83375L930K1CUNVLD1J120TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC83375L35K1CUNVLD1J24TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC83375L35K1CUNVLD1J48TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC83375L35K1CUNVLD1J96TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC83375L35K1CUNVLD1J120TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC83375L935K1CUNVLD1J24TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC83375L935K1CUNVLD1J48TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC83375L935K1CUNVLD1J96TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC83375L935K1CUNVLD1J120TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC83375L40K1CUNVLD1J24TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC83375L40K1CUNVLD1J48TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC83375L40K1CUNVLD1J96TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC83375L40K1CUNVLD1J120TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC83375L940K1CUNVLD1J24TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC83375L940K1CUNVLD1J48TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC83375L940K1CUNVLD1J96TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC83375L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC83375L940K1CUNVLD1J120TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,68
ASM1TIP6DC123375L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC123375L30K1CUNVLD1J24TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC123375L30K1CUNVLD1J48TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC123375L30K1CUNVLD1J96TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC123375L30K1CUNVLD1J120TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC123375L930K1CUNVLD1J24TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC123375L930K1CUNVLD1J48TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC123375L930K1CUNVLD1J96TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC123375L930K1CUNVLD1J120TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC123375L35K1CUNVLD1J24TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC123375L35K1CUNVLD1J48TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC123375L35K1CUNVLD1J96TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC123375L35K1CUNVLD1J120TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC123375L935K1CUNVLD1J24TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC123375L935K1CUNVLD1J48TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC123375L935K1CUNVLD1J96TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC123375L935K1CUNVLD1J120TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC123375L40K1CUNVLD1J24TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC123375L40K1CUNVLD1J48TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC123375L40K1CUNVLD1J96TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC123375L40K1CUNVLD1J120TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC123375L940K1CUNVLD1J24TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC123375L940K1CUNVLD1J48TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC123375L940K1CUNVLD1J96TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC123375L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC123375L940K1CUNVLD1J120TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,612
ASM1TIP6DC163375L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC163375L30K1CUNVLD1J24TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC163375L30K1CUNVLD1J48TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC163375L30K1CUNVLD1J96TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC163375L30K1CUNVLD1J120TSBKCD,Dust Cover,3375,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC163375L930K1CUNVLD1J24TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC163375L930K1CUNVLD1J48TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC163375L930K1CUNVLD1J96TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC163375L930K1CUNVLD1J120TSBKCD,Dust Cover,3375,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC163375L35K1CUNVLD1J24TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC163375L35K1CUNVLD1J48TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC163375L35K1CUNVLD1J96TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC163375L35K1CUNVLD1J120TSBKCD,Dust Cover,3375,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC163375L935K1CUNVLD1J24TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC163375L935K1CUNVLD1J48TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC163375L935K1CUNVLD1J96TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC163375L935K1CUNVLD1J120TSBKCD,Dust Cover,3375,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC163375L40K1CUNVLD1J24TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC163375L40K1CUNVLD1J48TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC163375L40K1CUNVLD1J96TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC163375L40K1CUNVLD1J120TSBKCD,Dust Cover,3375,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC163375L940K1CUNVLD1J24TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC163375L940K1CUNVLD1J48TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC163375L940K1CUNVLD1J96TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP6DC163375L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC163375L940K1CUNVLD1J120TSBKCD,Dust Cover,3375,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,22.4,22.4 Watts,ASM1TIP-6-DC-3375L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3375 Lumens,616
ASM1TIP4BW83750L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW83750L30K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW83750L30K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW83750L30K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW83750L30K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW83750L930K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW83750L930K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW83750L930K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW83750L930K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW83750L35K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW83750L35K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW83750L35K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW83750L35K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW83750L935K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW83750L935K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW83750L935K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW83750L935K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW83750L40K1CUNVLD1J24TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW83750L40K1CUNVLD1J48TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW83750L40K1CUNVLD1J96TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW83750L40K1CUNVLD1J120TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW83750L940K1CUNVLD1J24TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW83750L940K1CUNVLD1J48TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW83750L940K1CUNVLD1J96TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW83750L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW83750L940K1CUNVLD1J120TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4BW123750L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW123750L30K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW123750L30K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW123750L30K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW123750L30K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW123750L930K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW123750L930K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW123750L930K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW123750L930K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW123750L35K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW123750L35K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW123750L35K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW123750L35K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW123750L935K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW123750L935K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW123750L935K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW123750L935K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW123750L40K1CUNVLD1J24TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW123750L40K1CUNVLD1J48TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW123750L40K1CUNVLD1J96TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW123750L40K1CUNVLD1J120TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW123750L940K1CUNVLD1J24TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW123750L940K1CUNVLD1J48TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW123750L940K1CUNVLD1J96TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW123750L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW123750L940K1CUNVLD1J120TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4BW163750L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW163750L30K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW163750L30K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW163750L30K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW163750L30K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW163750L930K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW163750L930K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW163750L930K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW163750L930K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW163750L35K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW163750L35K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW163750L35K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW163750L35K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW163750L935K1CUNVLD1J24TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW163750L935K1CUNVLD1J48TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW163750L935K1CUNVLD1J96TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW163750L935K1CUNVLD1J120TSBKCD,Batwing Optic,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW163750L40K1CUNVLD1J24TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW163750L40K1CUNVLD1J48TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW163750L40K1CUNVLD1J96TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW163750L40K1CUNVLD1J120TSBKCD,Batwing Optic,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW163750L940K1CUNVLD1J24TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW163750L940K1CUNVLD1J48TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW163750L940K1CUNVLD1J96TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4BW163750L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW163750L940K1CUNVLD1J120TSBKCD,Batwing Optic,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-BW-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC83750L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC83750L30K1CUNVLD1J24TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC83750L30K1CUNVLD1J48TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC83750L30K1CUNVLD1J96TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC83750L30K1CUNVLD1J120TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC83750L930K1CUNVLD1J24TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC83750L930K1CUNVLD1J48TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC83750L930K1CUNVLD1J96TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC83750L930K1CUNVLD1J120TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC83750L35K1CUNVLD1J24TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC83750L35K1CUNVLD1J48TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC83750L35K1CUNVLD1J96TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC83750L35K1CUNVLD1J120TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC83750L935K1CUNVLD1J24TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC83750L935K1CUNVLD1J48TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC83750L935K1CUNVLD1J96TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC83750L935K1CUNVLD1J120TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC83750L40K1CUNVLD1J24TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC83750L40K1CUNVLD1J48TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC83750L40K1CUNVLD1J96TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC83750L40K1CUNVLD1J120TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC83750L940K1CUNVLD1J24TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC83750L940K1CUNVLD1J48TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC83750L940K1CUNVLD1J96TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC83750L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC83750L940K1CUNVLD1J120TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,48
ASM1TIP4DC123750L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC123750L30K1CUNVLD1J24TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC123750L30K1CUNVLD1J48TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC123750L30K1CUNVLD1J96TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC123750L30K1CUNVLD1J120TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC123750L930K1CUNVLD1J24TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC123750L930K1CUNVLD1J48TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC123750L930K1CUNVLD1J96TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC123750L930K1CUNVLD1J120TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC123750L35K1CUNVLD1J24TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC123750L35K1CUNVLD1J48TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC123750L35K1CUNVLD1J96TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC123750L35K1CUNVLD1J120TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC123750L935K1CUNVLD1J24TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC123750L935K1CUNVLD1J48TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC123750L935K1CUNVLD1J96TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC123750L935K1CUNVLD1J120TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC123750L40K1CUNVLD1J24TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC123750L40K1CUNVLD1J48TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC123750L40K1CUNVLD1J96TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC123750L40K1CUNVLD1J120TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC123750L940K1CUNVLD1J24TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC123750L940K1CUNVLD1J48TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC123750L940K1CUNVLD1J96TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC123750L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC123750L940K1CUNVLD1J120TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,412
ASM1TIP4DC163750L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC163750L30K1CUNVLD1J24TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC163750L30K1CUNVLD1J48TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC163750L30K1CUNVLD1J96TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC163750L30K1CUNVLD1J120TSBKCD,Dust Cover,3750,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC163750L930K1CUNVLD1J24TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC163750L930K1CUNVLD1J48TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC163750L930K1CUNVLD1J96TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC163750L930K1CUNVLD1J120TSBKCD,Dust Cover,3750,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC163750L35K1CUNVLD1J24TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC163750L35K1CUNVLD1J48TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC163750L35K1CUNVLD1J96TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC163750L35K1CUNVLD1J120TSBKCD,Dust Cover,3750,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC163750L935K1CUNVLD1J24TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC163750L935K1CUNVLD1J48TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC163750L935K1CUNVLD1J96TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC163750L935K1CUNVLD1J120TSBKCD,Dust Cover,3750,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC163750L40K1CUNVLD1J24TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC163750L40K1CUNVLD1J48TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC163750L40K1CUNVLD1J96TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC163750L40K1CUNVLD1J120TSBKCD,Dust Cover,3750,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC163750L940K1CUNVLD1J24TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC163750L940K1CUNVLD1J48TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC163750L940K1CUNVLD1J96TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP4DC163750L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC163750L940K1CUNVLD1J120TSBKCD,Dust Cover,3750,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,27,27 Watts,ASM1TIP-4-DC-3750L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 3750 Lumens,416
ASM1TIP6BW84500L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW84500L30K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW84500L30K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW84500L30K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW84500L30K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW84500L930K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW84500L930K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW84500L930K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW84500L930K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW84500L35K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW84500L35K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW84500L35K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW84500L35K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW84500L935K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW84500L935K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW84500L935K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW84500L935K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW84500L40K1CUNVLD1J24TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW84500L40K1CUNVLD1J48TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW84500L40K1CUNVLD1J96TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW84500L40K1CUNVLD1J120TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW84500L940K1CUNVLD1J24TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW84500L940K1CUNVLD1J48TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW84500L940K1CUNVLD1J96TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW84500L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW84500L940K1CUNVLD1J120TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6BW124500L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW124500L30K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW124500L30K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW124500L30K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW124500L30K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW124500L930K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW124500L930K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW124500L930K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW124500L930K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW124500L35K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW124500L35K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW124500L35K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW124500L35K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW124500L935K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW124500L935K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW124500L935K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW124500L935K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW124500L40K1CUNVLD1J24TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW124500L40K1CUNVLD1J48TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW124500L40K1CUNVLD1J96TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW124500L40K1CUNVLD1J120TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW124500L940K1CUNVLD1J24TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW124500L940K1CUNVLD1J48TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW124500L940K1CUNVLD1J96TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW124500L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW124500L940K1CUNVLD1J120TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6BW164500L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW164500L30K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW164500L30K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW164500L30K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW164500L30K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW164500L930K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW164500L930K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW164500L930K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW164500L930K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW164500L35K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW164500L35K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW164500L35K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW164500L35K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW164500L935K1CUNVLD1J24TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW164500L935K1CUNVLD1J48TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW164500L935K1CUNVLD1J96TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW164500L935K1CUNVLD1J120TSBKCD,Batwing Optic,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW164500L40K1CUNVLD1J24TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW164500L40K1CUNVLD1J48TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW164500L40K1CUNVLD1J96TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW164500L40K1CUNVLD1J120TSBKCD,Batwing Optic,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW164500L940K1CUNVLD1J24TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW164500L940K1CUNVLD1J48TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW164500L940K1CUNVLD1J96TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6BW164500L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW164500L940K1CUNVLD1J120TSBKCD,Batwing Optic,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-BW-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC84500L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC84500L30K1CUNVLD1J24TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC84500L30K1CUNVLD1J48TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC84500L30K1CUNVLD1J96TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC84500L30K1CUNVLD1J120TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC84500L930K1CUNVLD1J24TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC84500L930K1CUNVLD1J48TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC84500L930K1CUNVLD1J96TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC84500L930K1CUNVLD1J120TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC84500L35K1CUNVLD1J24TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC84500L35K1CUNVLD1J48TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC84500L35K1CUNVLD1J96TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC84500L35K1CUNVLD1J120TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC84500L935K1CUNVLD1J24TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC84500L935K1CUNVLD1J48TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC84500L935K1CUNVLD1J96TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC84500L935K1CUNVLD1J120TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC84500L40K1CUNVLD1J24TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC84500L40K1CUNVLD1J48TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC84500L40K1CUNVLD1J96TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC84500L40K1CUNVLD1J120TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC84500L940K1CUNVLD1J24TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC84500L940K1CUNVLD1J48TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC84500L940K1CUNVLD1J96TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC84500L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC84500L940K1CUNVLD1J120TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,68
ASM1TIP6DC124500L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC124500L30K1CUNVLD1J24TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC124500L30K1CUNVLD1J48TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC124500L30K1CUNVLD1J96TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC124500L30K1CUNVLD1J120TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC124500L930K1CUNVLD1J24TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC124500L930K1CUNVLD1J48TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC124500L930K1CUNVLD1J96TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC124500L930K1CUNVLD1J120TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC124500L35K1CUNVLD1J24TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC124500L35K1CUNVLD1J48TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC124500L35K1CUNVLD1J96TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC124500L35K1CUNVLD1J120TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC124500L935K1CUNVLD1J24TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC124500L935K1CUNVLD1J48TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC124500L935K1CUNVLD1J96TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC124500L935K1CUNVLD1J120TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC124500L40K1CUNVLD1J24TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC124500L40K1CUNVLD1J48TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC124500L40K1CUNVLD1J96TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC124500L40K1CUNVLD1J120TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC124500L940K1CUNVLD1J24TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC124500L940K1CUNVLD1J48TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC124500L940K1CUNVLD1J96TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC124500L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC124500L940K1CUNVLD1J120TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,612
ASM1TIP6DC164500L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC164500L30K1CUNVLD1J24TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC164500L30K1CUNVLD1J48TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC164500L30K1CUNVLD1J96TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC164500L30K1CUNVLD1J120TSBKCD,Dust Cover,4500,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC164500L930K1CUNVLD1J24TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC164500L930K1CUNVLD1J48TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC164500L930K1CUNVLD1J96TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC164500L930K1CUNVLD1J120TSBKCD,Dust Cover,4500,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC164500L35K1CUNVLD1J24TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC164500L35K1CUNVLD1J48TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC164500L35K1CUNVLD1J96TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC164500L35K1CUNVLD1J120TSBKCD,Dust Cover,4500,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC164500L935K1CUNVLD1J24TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC164500L935K1CUNVLD1J48TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC164500L935K1CUNVLD1J96TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC164500L935K1CUNVLD1J120TSBKCD,Dust Cover,4500,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC164500L40K1CUNVLD1J24TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC164500L40K1CUNVLD1J48TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC164500L40K1CUNVLD1J96TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC164500L40K1CUNVLD1J120TSBKCD,Dust Cover,4500,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC164500L940K1CUNVLD1J24TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC164500L940K1CUNVLD1J48TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC164500L940K1CUNVLD1J96TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP6DC164500L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC164500L940K1CUNVLD1J120TSBKCD,Dust Cover,4500,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,30.1,30.1 Watts,ASM1TIP-6-DC-4500L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4500 Lumens,616
ASM1TIP4BW84800L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW84800L30K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW84800L30K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW84800L30K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW84800L30K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW84800L930K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW84800L930K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW84800L930K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW84800L930K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW84800L35K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW84800L35K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW84800L35K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW84800L35K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW84800L935K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW84800L935K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW84800L935K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW84800L935K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW84800L40K1CUNVLD1J24TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW84800L40K1CUNVLD1J48TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW84800L40K1CUNVLD1J96TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW84800L40K1CUNVLD1J120TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW84800L940K1CUNVLD1J24TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW84800L940K1CUNVLD1J48TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW84800L940K1CUNVLD1J96TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW84800L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW84800L940K1CUNVLD1J120TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4BW124800L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW124800L30K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW124800L30K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW124800L30K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW124800L30K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW124800L930K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW124800L930K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW124800L930K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW124800L930K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW124800L35K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW124800L35K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW124800L35K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW124800L35K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW124800L935K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW124800L935K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW124800L935K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW124800L935K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW124800L40K1CUNVLD1J24TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW124800L40K1CUNVLD1J48TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW124800L40K1CUNVLD1J96TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW124800L40K1CUNVLD1J120TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW124800L940K1CUNVLD1J24TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW124800L940K1CUNVLD1J48TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW124800L940K1CUNVLD1J96TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW124800L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW124800L940K1CUNVLD1J120TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4BW164800L30K1CUNVLD1J24TSBKCD,ASM1TIP4BW164800L30K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L30K1CUNVLD1J48TSBKCD,ASM1TIP4BW164800L30K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L30K1CUNVLD1J96TSBKCD,ASM1TIP4BW164800L30K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L30K1CUNVLD1J120TSBKCD,ASM1TIP4BW164800L30K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L930K1CUNVLD1J24TSBKCD,ASM1TIP4BW164800L930K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L930K1CUNVLD1J48TSBKCD,ASM1TIP4BW164800L930K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L930K1CUNVLD1J96TSBKCD,ASM1TIP4BW164800L930K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L930K1CUNVLD1J120TSBKCD,ASM1TIP4BW164800L930K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L35K1CUNVLD1J24TSBKCD,ASM1TIP4BW164800L35K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L35K1CUNVLD1J48TSBKCD,ASM1TIP4BW164800L35K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L35K1CUNVLD1J96TSBKCD,ASM1TIP4BW164800L35K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L35K1CUNVLD1J120TSBKCD,ASM1TIP4BW164800L35K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L935K1CUNVLD1J24TSBKCD,ASM1TIP4BW164800L935K1CUNVLD1J24TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L935K1CUNVLD1J48TSBKCD,ASM1TIP4BW164800L935K1CUNVLD1J48TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L935K1CUNVLD1J96TSBKCD,ASM1TIP4BW164800L935K1CUNVLD1J96TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L935K1CUNVLD1J120TSBKCD,ASM1TIP4BW164800L935K1CUNVLD1J120TSBKCD,Batwing Optic,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L40K1CUNVLD1J24TSBKCD,ASM1TIP4BW164800L40K1CUNVLD1J24TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L40K1CUNVLD1J48TSBKCD,ASM1TIP4BW164800L40K1CUNVLD1J48TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L40K1CUNVLD1J96TSBKCD,ASM1TIP4BW164800L40K1CUNVLD1J96TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L40K1CUNVLD1J120TSBKCD,ASM1TIP4BW164800L40K1CUNVLD1J120TSBKCD,Batwing Optic,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L940K1CUNVLD1J24TSBKCD,ASM1TIP4BW164800L940K1CUNVLD1J24TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L940K1CUNVLD1J48TSBKCD,ASM1TIP4BW164800L940K1CUNVLD1J48TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L940K1CUNVLD1J96TSBKCD,ASM1TIP4BW164800L940K1CUNVLD1J96TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4BW164800L940K1CUNVLD1J120TSBKCD,ASM1TIP4BW164800L940K1CUNVLD1J120TSBKCD,Batwing Optic,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-BW-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC84800L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC84800L30K1CUNVLD1J24TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC84800L30K1CUNVLD1J48TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC84800L30K1CUNVLD1J96TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC84800L30K1CUNVLD1J120TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC84800L930K1CUNVLD1J24TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC84800L930K1CUNVLD1J48TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC84800L930K1CUNVLD1J96TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC84800L930K1CUNVLD1J120TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC84800L35K1CUNVLD1J24TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC84800L35K1CUNVLD1J48TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC84800L35K1CUNVLD1J96TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC84800L35K1CUNVLD1J120TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC84800L935K1CUNVLD1J24TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC84800L935K1CUNVLD1J48TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC84800L935K1CUNVLD1J96TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC84800L935K1CUNVLD1J120TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC84800L40K1CUNVLD1J24TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC84800L40K1CUNVLD1J48TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC84800L40K1CUNVLD1J96TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC84800L40K1CUNVLD1J120TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC84800L940K1CUNVLD1J24TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC84800L940K1CUNVLD1J48TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC84800L940K1CUNVLD1J96TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC84800L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC84800L940K1CUNVLD1J120TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,48
ASM1TIP4DC124800L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC124800L30K1CUNVLD1J24TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC124800L30K1CUNVLD1J48TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC124800L30K1CUNVLD1J96TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC124800L30K1CUNVLD1J120TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC124800L930K1CUNVLD1J24TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC124800L930K1CUNVLD1J48TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC124800L930K1CUNVLD1J96TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC124800L930K1CUNVLD1J120TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC124800L35K1CUNVLD1J24TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC124800L35K1CUNVLD1J48TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC124800L35K1CUNVLD1J96TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC124800L35K1CUNVLD1J120TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC124800L935K1CUNVLD1J24TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC124800L935K1CUNVLD1J48TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC124800L935K1CUNVLD1J96TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC124800L935K1CUNVLD1J120TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC124800L40K1CUNVLD1J24TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC124800L40K1CUNVLD1J48TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC124800L40K1CUNVLD1J96TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC124800L40K1CUNVLD1J120TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC124800L940K1CUNVLD1J24TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC124800L940K1CUNVLD1J48TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC124800L940K1CUNVLD1J96TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC124800L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC124800L940K1CUNVLD1J120TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,412
ASM1TIP4DC164800L30K1CUNVLD1J24TSBKCD,ASM1TIP4DC164800L30K1CUNVLD1J24TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L30K1CUNVLD1J48TSBKCD,ASM1TIP4DC164800L30K1CUNVLD1J48TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L30K1CUNVLD1J96TSBKCD,ASM1TIP4DC164800L30K1CUNVLD1J96TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L30K1CUNVLD1J120TSBKCD,ASM1TIP4DC164800L30K1CUNVLD1J120TSBKCD,Dust Cover,4800,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L930K1CUNVLD1J24TSBKCD,ASM1TIP4DC164800L930K1CUNVLD1J24TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L930K1CUNVLD1J48TSBKCD,ASM1TIP4DC164800L930K1CUNVLD1J48TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L930K1CUNVLD1J96TSBKCD,ASM1TIP4DC164800L930K1CUNVLD1J96TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L930K1CUNVLD1J120TSBKCD,ASM1TIP4DC164800L930K1CUNVLD1J120TSBKCD,Dust Cover,4800,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L35K1CUNVLD1J24TSBKCD,ASM1TIP4DC164800L35K1CUNVLD1J24TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L35K1CUNVLD1J48TSBKCD,ASM1TIP4DC164800L35K1CUNVLD1J48TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L35K1CUNVLD1J96TSBKCD,ASM1TIP4DC164800L35K1CUNVLD1J96TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L35K1CUNVLD1J120TSBKCD,ASM1TIP4DC164800L35K1CUNVLD1J120TSBKCD,Dust Cover,4800,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L935K1CUNVLD1J24TSBKCD,ASM1TIP4DC164800L935K1CUNVLD1J24TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L935K1CUNVLD1J48TSBKCD,ASM1TIP4DC164800L935K1CUNVLD1J48TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L935K1CUNVLD1J96TSBKCD,ASM1TIP4DC164800L935K1CUNVLD1J96TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L935K1CUNVLD1J120TSBKCD,ASM1TIP4DC164800L935K1CUNVLD1J120TSBKCD,Dust Cover,4800,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L40K1CUNVLD1J24TSBKCD,ASM1TIP4DC164800L40K1CUNVLD1J24TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L40K1CUNVLD1J48TSBKCD,ASM1TIP4DC164800L40K1CUNVLD1J48TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L40K1CUNVLD1J96TSBKCD,ASM1TIP4DC164800L40K1CUNVLD1J96TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L40K1CUNVLD1J120TSBKCD,ASM1TIP4DC164800L40K1CUNVLD1J120TSBKCD,Dust Cover,4800,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L940K1CUNVLD1J24TSBKCD,ASM1TIP4DC164800L940K1CUNVLD1J24TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L940K1CUNVLD1J48TSBKCD,ASM1TIP4DC164800L940K1CUNVLD1J48TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L940K1CUNVLD1J96TSBKCD,ASM1TIP4DC164800L940K1CUNVLD1J96TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP4DC164800L940K1CUNVLD1J120TSBKCD,ASM1TIP4DC164800L940K1CUNVLD1J120TSBKCD,Dust Cover,4800,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,35.1,35.1 Watts,ASM1TIP-4-DC-4800L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 4800 Lumens,416
ASM1TIP6BW85625L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW85625L30K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW85625L30K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW85625L30K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW85625L30K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW85625L930K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW85625L930K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW85625L930K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW85625L930K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW85625L35K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW85625L35K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW85625L35K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW85625L35K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW85625L935K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW85625L935K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW85625L935K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW85625L935K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW85625L40K1CUNVLD1J24TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW85625L40K1CUNVLD1J48TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW85625L40K1CUNVLD1J96TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW85625L40K1CUNVLD1J120TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW85625L940K1CUNVLD1J24TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW85625L940K1CUNVLD1J48TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW85625L940K1CUNVLD1J96TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW85625L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW85625L940K1CUNVLD1J120TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6BW125625L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW125625L30K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW125625L30K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW125625L30K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW125625L30K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW125625L930K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW125625L930K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW125625L930K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW125625L930K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW125625L35K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW125625L35K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW125625L35K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW125625L35K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW125625L935K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW125625L935K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW125625L935K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW125625L935K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW125625L40K1CUNVLD1J24TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW125625L40K1CUNVLD1J48TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW125625L40K1CUNVLD1J96TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW125625L40K1CUNVLD1J120TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW125625L940K1CUNVLD1J24TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW125625L940K1CUNVLD1J48TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW125625L940K1CUNVLD1J96TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW125625L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW125625L940K1CUNVLD1J120TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6BW165625L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW165625L30K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW165625L30K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW165625L30K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW165625L30K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW165625L930K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW165625L930K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW165625L930K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW165625L930K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW165625L35K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW165625L35K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW165625L35K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW165625L35K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW165625L935K1CUNVLD1J24TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW165625L935K1CUNVLD1J48TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW165625L935K1CUNVLD1J96TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW165625L935K1CUNVLD1J120TSBKCD,Batwing Optic,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW165625L40K1CUNVLD1J24TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW165625L40K1CUNVLD1J48TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW165625L40K1CUNVLD1J96TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW165625L40K1CUNVLD1J120TSBKCD,Batwing Optic,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW165625L940K1CUNVLD1J24TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW165625L940K1CUNVLD1J48TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW165625L940K1CUNVLD1J96TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW165625L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW165625L940K1CUNVLD1J120TSBKCD,Batwing Optic,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-BW-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC85625L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC85625L30K1CUNVLD1J24TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC85625L30K1CUNVLD1J48TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC85625L30K1CUNVLD1J96TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC85625L30K1CUNVLD1J120TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC85625L930K1CUNVLD1J24TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC85625L930K1CUNVLD1J48TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC85625L930K1CUNVLD1J96TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC85625L930K1CUNVLD1J120TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC85625L35K1CUNVLD1J24TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC85625L35K1CUNVLD1J48TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC85625L35K1CUNVLD1J96TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC85625L35K1CUNVLD1J120TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC85625L935K1CUNVLD1J24TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC85625L935K1CUNVLD1J48TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC85625L935K1CUNVLD1J96TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC85625L935K1CUNVLD1J120TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC85625L40K1CUNVLD1J24TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC85625L40K1CUNVLD1J48TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC85625L40K1CUNVLD1J96TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC85625L40K1CUNVLD1J120TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC85625L940K1CUNVLD1J24TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC85625L940K1CUNVLD1J48TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC85625L940K1CUNVLD1J96TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC85625L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC85625L940K1CUNVLD1J120TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,68
ASM1TIP6DC125625L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC125625L30K1CUNVLD1J24TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC125625L30K1CUNVLD1J48TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC125625L30K1CUNVLD1J96TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC125625L30K1CUNVLD1J120TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC125625L930K1CUNVLD1J24TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC125625L930K1CUNVLD1J48TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC125625L930K1CUNVLD1J96TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC125625L930K1CUNVLD1J120TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC125625L35K1CUNVLD1J24TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC125625L35K1CUNVLD1J48TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC125625L35K1CUNVLD1J96TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC125625L35K1CUNVLD1J120TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC125625L935K1CUNVLD1J24TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC125625L935K1CUNVLD1J48TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC125625L935K1CUNVLD1J96TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC125625L935K1CUNVLD1J120TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC125625L40K1CUNVLD1J24TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC125625L40K1CUNVLD1J48TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC125625L40K1CUNVLD1J96TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC125625L40K1CUNVLD1J120TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC125625L940K1CUNVLD1J24TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC125625L940K1CUNVLD1J48TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC125625L940K1CUNVLD1J96TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC125625L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC125625L940K1CUNVLD1J120TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,612
ASM1TIP6DC165625L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC165625L30K1CUNVLD1J24TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC165625L30K1CUNVLD1J48TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC165625L30K1CUNVLD1J96TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC165625L30K1CUNVLD1J120TSBKCD,Dust Cover,5625,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC165625L930K1CUNVLD1J24TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC165625L930K1CUNVLD1J48TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC165625L930K1CUNVLD1J96TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC165625L930K1CUNVLD1J120TSBKCD,Dust Cover,5625,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC165625L35K1CUNVLD1J24TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC165625L35K1CUNVLD1J48TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC165625L35K1CUNVLD1J96TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC165625L35K1CUNVLD1J120TSBKCD,Dust Cover,5625,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC165625L935K1CUNVLD1J24TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC165625L935K1CUNVLD1J48TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC165625L935K1CUNVLD1J96TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC165625L935K1CUNVLD1J120TSBKCD,Dust Cover,5625,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC165625L40K1CUNVLD1J24TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC165625L40K1CUNVLD1J48TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC165625L40K1CUNVLD1J96TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC165625L40K1CUNVLD1J120TSBKCD,Dust Cover,5625,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC165625L940K1CUNVLD1J24TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC165625L940K1CUNVLD1J48TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC165625L940K1CUNVLD1J96TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6DC165625L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC165625L940K1CUNVLD1J120TSBKCD,Dust Cover,5625,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,37.5,37.5 Watts,ASM1TIP-6-DC-5625L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 5625 Lumens,616
ASM1TIP6BW87200L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW87200L30K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW87200L30K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW87200L30K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW87200L30K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW87200L930K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW87200L930K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW87200L930K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW87200L930K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW87200L35K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW87200L35K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW87200L35K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW87200L35K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW87200L935K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW87200L935K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW87200L935K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW87200L935K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW87200L40K1CUNVLD1J24TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW87200L40K1CUNVLD1J48TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW87200L40K1CUNVLD1J96TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW87200L40K1CUNVLD1J120TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW87200L940K1CUNVLD1J24TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW87200L940K1CUNVLD1J48TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW87200L940K1CUNVLD1J96TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW87200L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW87200L940K1CUNVLD1J120TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6BW127200L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW127200L30K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW127200L30K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW127200L30K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW127200L30K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW127200L930K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW127200L930K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW127200L930K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW127200L930K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW127200L35K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW127200L35K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW127200L35K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW127200L35K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW127200L935K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW127200L935K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW127200L935K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW127200L935K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW127200L40K1CUNVLD1J24TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW127200L40K1CUNVLD1J48TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW127200L40K1CUNVLD1J96TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW127200L40K1CUNVLD1J120TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW127200L940K1CUNVLD1J24TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW127200L940K1CUNVLD1J48TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW127200L940K1CUNVLD1J96TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW127200L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW127200L940K1CUNVLD1J120TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6BW167200L30K1CUNVLD1J24TSBKCD,ASM1TIP6BW167200L30K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L30K1CUNVLD1J48TSBKCD,ASM1TIP6BW167200L30K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L30K1CUNVLD1J96TSBKCD,ASM1TIP6BW167200L30K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L30K1CUNVLD1J120TSBKCD,ASM1TIP6BW167200L30K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L930K1CUNVLD1J24TSBKCD,ASM1TIP6BW167200L930K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L930K1CUNVLD1J48TSBKCD,ASM1TIP6BW167200L930K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L930K1CUNVLD1J96TSBKCD,ASM1TIP6BW167200L930K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L930K1CUNVLD1J120TSBKCD,ASM1TIP6BW167200L930K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L35K1CUNVLD1J24TSBKCD,ASM1TIP6BW167200L35K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L35K1CUNVLD1J48TSBKCD,ASM1TIP6BW167200L35K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L35K1CUNVLD1J96TSBKCD,ASM1TIP6BW167200L35K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L35K1CUNVLD1J120TSBKCD,ASM1TIP6BW167200L35K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L935K1CUNVLD1J24TSBKCD,ASM1TIP6BW167200L935K1CUNVLD1J24TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L935K1CUNVLD1J48TSBKCD,ASM1TIP6BW167200L935K1CUNVLD1J48TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L935K1CUNVLD1J96TSBKCD,ASM1TIP6BW167200L935K1CUNVLD1J96TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L935K1CUNVLD1J120TSBKCD,ASM1TIP6BW167200L935K1CUNVLD1J120TSBKCD,Batwing Optic,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L40K1CUNVLD1J24TSBKCD,ASM1TIP6BW167200L40K1CUNVLD1J24TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L40K1CUNVLD1J48TSBKCD,ASM1TIP6BW167200L40K1CUNVLD1J48TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L40K1CUNVLD1J96TSBKCD,ASM1TIP6BW167200L40K1CUNVLD1J96TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L40K1CUNVLD1J120TSBKCD,ASM1TIP6BW167200L40K1CUNVLD1J120TSBKCD,Batwing Optic,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L940K1CUNVLD1J24TSBKCD,ASM1TIP6BW167200L940K1CUNVLD1J24TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L940K1CUNVLD1J48TSBKCD,ASM1TIP6BW167200L940K1CUNVLD1J48TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L940K1CUNVLD1J96TSBKCD,ASM1TIP6BW167200L940K1CUNVLD1J96TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6BW167200L940K1CUNVLD1J120TSBKCD,ASM1TIP6BW167200L940K1CUNVLD1J120TSBKCD,Batwing Optic,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-BW-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC87200L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC87200L30K1CUNVLD1J24TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC87200L30K1CUNVLD1J48TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC87200L30K1CUNVLD1J96TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC87200L30K1CUNVLD1J120TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC87200L930K1CUNVLD1J24TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC87200L930K1CUNVLD1J48TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC87200L930K1CUNVLD1J96TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC87200L930K1CUNVLD1J120TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC87200L35K1CUNVLD1J24TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC87200L35K1CUNVLD1J48TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC87200L35K1CUNVLD1J96TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC87200L35K1CUNVLD1J120TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC87200L935K1CUNVLD1J24TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC87200L935K1CUNVLD1J48TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC87200L935K1CUNVLD1J96TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC87200L935K1CUNVLD1J120TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC87200L40K1CUNVLD1J24TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC87200L40K1CUNVLD1J48TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC87200L40K1CUNVLD1J96TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC87200L40K1CUNVLD1J120TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC87200L940K1CUNVLD1J24TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC87200L940K1CUNVLD1J48TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC87200L940K1CUNVLD1J96TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC87200L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC87200L940K1CUNVLD1J120TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,68
ASM1TIP6DC127200L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC127200L30K1CUNVLD1J24TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC127200L30K1CUNVLD1J48TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC127200L30K1CUNVLD1J96TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC127200L30K1CUNVLD1J120TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC127200L930K1CUNVLD1J24TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC127200L930K1CUNVLD1J48TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC127200L930K1CUNVLD1J96TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC127200L930K1CUNVLD1J120TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC127200L35K1CUNVLD1J24TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC127200L35K1CUNVLD1J48TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC127200L35K1CUNVLD1J96TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC127200L35K1CUNVLD1J120TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC127200L935K1CUNVLD1J24TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC127200L935K1CUNVLD1J48TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC127200L935K1CUNVLD1J96TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC127200L935K1CUNVLD1J120TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC127200L40K1CUNVLD1J24TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC127200L40K1CUNVLD1J48TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC127200L40K1CUNVLD1J96TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC127200L40K1CUNVLD1J120TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC127200L940K1CUNVLD1J24TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC127200L940K1CUNVLD1J48TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC127200L940K1CUNVLD1J96TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC127200L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC127200L940K1CUNVLD1J120TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,612
ASM1TIP6DC167200L30K1CUNVLD1J24TSBKCD,ASM1TIP6DC167200L30K1CUNVLD1J24TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L30K1CUNVLD1J48TSBKCD,ASM1TIP6DC167200L30K1CUNVLD1J48TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L30K1CUNVLD1J96TSBKCD,ASM1TIP6DC167200L30K1CUNVLD1J96TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L30K1CUNVLD1J120TSBKCD,ASM1TIP6DC167200L30K1CUNVLD1J120TSBKCD,Dust Cover,7200,3000,"3000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L930K1CUNVLD1J24TSBKCD,ASM1TIP6DC167200L930K1CUNVLD1J24TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L930K1CUNVLD1J48TSBKCD,ASM1TIP6DC167200L930K1CUNVLD1J48TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L930K1CUNVLD1J96TSBKCD,ASM1TIP6DC167200L930K1CUNVLD1J96TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L930K1CUNVLD1J120TSBKCD,ASM1TIP6DC167200L930K1CUNVLD1J120TSBKCD,Dust Cover,7200,3000,"3000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L35K1CUNVLD1J24TSBKCD,ASM1TIP6DC167200L35K1CUNVLD1J24TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L35K1CUNVLD1J48TSBKCD,ASM1TIP6DC167200L35K1CUNVLD1J48TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L35K1CUNVLD1J96TSBKCD,ASM1TIP6DC167200L35K1CUNVLD1J96TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L35K1CUNVLD1J120TSBKCD,ASM1TIP6DC167200L35K1CUNVLD1J120TSBKCD,Dust Cover,7200,3500,"3500K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L935K1CUNVLD1J24TSBKCD,ASM1TIP6DC167200L935K1CUNVLD1J24TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L935K1CUNVLD1J48TSBKCD,ASM1TIP6DC167200L935K1CUNVLD1J48TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L935K1CUNVLD1J96TSBKCD,ASM1TIP6DC167200L935K1CUNVLD1J96TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L935K1CUNVLD1J120TSBKCD,ASM1TIP6DC167200L935K1CUNVLD1J120TSBKCD,Dust Cover,7200,3500,"3500K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L40K1CUNVLD1J24TSBKCD,ASM1TIP6DC167200L40K1CUNVLD1J24TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L40K1CUNVLD1J48TSBKCD,ASM1TIP6DC167200L40K1CUNVLD1J48TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L40K1CUNVLD1J96TSBKCD,ASM1TIP6DC167200L40K1CUNVLD1J96TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L40K1CUNVLD1J120TSBKCD,ASM1TIP6DC167200L40K1CUNVLD1J120TSBKCD,Dust Cover,7200,4000,"4000K, 80+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L940K1CUNVLD1J24TSBKCD,ASM1TIP6DC167200L940K1CUNVLD1J24TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"24"" Cable Suspension",24,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L940K1CUNVLD1J48TSBKCD,ASM1TIP6DC167200L940K1CUNVLD1J48TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"48"" Cable Suspension",48,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L940K1CUNVLD1J96TSBKCD,ASM1TIP6DC167200L940K1CUNVLD1J96TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"96"" Cable Suspension",96,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
ASM1TIP6DC167200L940K1CUNVLD1J120TSBKCD,ASM1TIP6DC167200L940K1CUNVLD1J120TSBKCD,Dust Cover,7200,4000,"4000K, 90+ CRI",120,0-10V - 10% Dimming,Single Circuit,"120"" Cable Suspension",120,49.7,49.7 Watts,ASM1TIP-6-DC-7200L-35K-1C-UNV.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Indirect Distribution - 7200 Lumens,616
