,Model##OTHER##,Shielding Type##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Lumen Output##Other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Color Temperature Note##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Mounting##Other##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Photometric Web File##OTHER##,Lumen Output Comment##OTHER##,Perimeter##OTHER##,Perimeter Ceiling Trim##OTHER##,Perimeter Grid##OTHER##,Perimeter Grid Bracket##OTHER##,Perimeter ST Ceiling Trim##OTHER##,Perimeter TF Trim##OTHER##,Perimeter Wall Clip##OTHER##,Regress##LENGTH##INCHES,Perimeter Flange Width##LENGTH##INCHES
FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-G-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-XF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-125LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-AF0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-250LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-AF0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-375LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-AF0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-625LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-AF0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-750LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-AF0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-875LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-AF0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-AF0-1000LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-AF0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-AF1-125LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-125LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-125LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-AF1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-250LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-250LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-AF1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-375LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-375LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-AF1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-625LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-625LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-AF1-625LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-750LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-750LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-AF1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-875LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-875LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-AF1-875LF-35K-1C-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-AF1-1000LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-AF1-1000LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Asymmetric Room Fill",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-AF1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-G-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-XF-x-WH,Flush Lens,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-G-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-XF-x-WH,Flush Lens,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-G-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-XF-x-WH,Flush Lens,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-G-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-XF-x-WH,Flush Lens,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-G-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-XF-x-WH,Flush Lens,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-G-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,0,0.2812
FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-XF-x-WH,Flush Lens,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-G-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-XF-x-WH,Flush Lens,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,35,35 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,0,0.2812
FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-125LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,6,6 Watts,FSM2PR-FL0-125LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-250LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,9,9 Watts,FSM2PR-FL0-250LF-35K-UNV-LD1-G-WH-4.ies,3' minimum with LH1 drivers,0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-375LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,12,12 Watts,FSM2PR-FL0-375LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-625LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,20,20 Watts,FSM2PR-FL0-625LF-35K-UNV-LD1-G-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-750LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,25,25 Watts,FSM2PR-FL0-750LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-875LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,29,29 Watts,FSM2PR-FL0-875LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-27K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-30K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-35K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-40K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-927K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-930K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-935K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-LV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-ST-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-ST-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Slot Tee/Tegular,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,1,0,1,0,1,0,0.2812
FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-TF-x-WH,FSM2PR-FXH-FL0-1000LF-940K-1C-UNV-LD1-TF-x-WH,Flush Asymmetric Room Fill,1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trim Flange,33,33 Watts,FSM2PR-FL0-1000LF-35K-UNV-LD1-G-WH-4.ies,"4' minimum with LU5, LH1, D11",0,1,1,0,0,1,0,0,0.5
FSM2PR-FXH-FL1-125LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-125LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-125LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-250LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-250LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-375LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-375LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-625LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-625LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-FL1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-750LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-750LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-FL1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-875LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-875LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-FL1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL1-1000LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL1-1000LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-FL1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-FL2-125LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-125LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-125LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-125LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-125LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-125LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-250LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-250LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-250LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-250LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-250LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,9,9 Watts,FSM2PR-FL2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-375LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-375LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-375LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-375LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-375LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-FL2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-625LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-625LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-625LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-625LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-625LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-FL2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-750LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-750LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-750LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-750LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-750LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-FL2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-875LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-875LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-875LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-875LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-875LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-FL2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL2-1000LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-FL2-1000LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL2-1000LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-FL2-1000LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL2-1000LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-FL2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-FL4-125LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-125LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-125LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-125LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-125LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-125LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-FL4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-250LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-250LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-250LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-250LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-250LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-FL4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-375LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-375LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-375LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-375LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-375LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,14,14 Watts,FSM2PR-FL4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-625LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-625LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-625LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-625LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-625LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,23,23 Watts,FSM2PR-FL4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-750LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-750LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-750LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-750LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-750LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,28,28 Watts,FSM2PR-FL4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-875LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-875LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-875LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-875LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-875LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,33,33 Watts,FSM2PR-FL4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-FL4-1000LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-FL4-1000LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-FL4-1000LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-FL4-1000LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-FL4-1000LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,39,39 Watts,FSM2PR-FL4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR1-125LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-125LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-125LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR1-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-250LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-250LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,9,9 Watts,FSM2PR-GR1-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-375LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-375LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR1-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-625LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-625LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR1-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-750LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-750LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,26,26 Watts,FSM2PR-GR1-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-875LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-875LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,30,30 Watts,FSM2PR-GR1-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-27K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-27K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-30K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-30K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-35K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-35K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-40K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-40K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-927K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-927K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-930K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-930K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-935K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-935K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-940K-1C-LV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR1-1000LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR1-1000LF-940K-1C-UNV-LD1-XFF-x-WH,"1.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,35,35 Watts,FSM2PR-GR1-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,1,1.1
FSM2PR-FXH-GR2-125LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-125LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-125LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-125LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-125LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-125LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR2-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-250LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-250LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-250LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-250LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-250LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR2-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-375LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-375LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-375LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-375LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-375LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR2-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-625LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-625LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-625LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-625LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-625LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,21,21 Watts,FSM2PR-GR2-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-750LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-750LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-750LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-750LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-750LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR2-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-875LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-875LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-875LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-875LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-875LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,31,31 Watts,FSM2PR-GR2-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-27K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-27K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-27K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-27K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-27K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-27K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-30K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-30K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-30K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-30K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-30K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-30K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-35K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-35K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-35K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-35K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-35K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-35K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-40K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-40K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-40K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-40K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-40K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-40K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-927K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-927K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-927K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-927K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-927K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-927K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-930K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-930K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-930K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-930K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-930K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-930K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-935K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-935K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-935K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-935K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-935K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-935K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-940K-1C-LV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-940K-1C-LV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-940K-1C-LV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR2-1000LF-940K-1C-UNV-LD1-G-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,2.5,0.2812
FSM2PR-FXH-GR2-1000LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR2-1000LF-940K-1C-UNV-LD1-XFF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,1.1
FSM2PR-FXH-GR2-1000LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR2-1000LF-940K-1C-UNV-LD1-XF-x-WH,"2.5"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,36,36 Watts,FSM2PR-GR2-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,2.5,0.2812
FSM2PR-FXH-GR4-125LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-125LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-125LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-125LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-125LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-125LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",125,125 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,6,6 Watts,FSM2PR-GR4-125LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-250LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-250LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-250LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-250LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-250LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",250,250 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,10,10 Watts,FSM2PR-GR4-250LF-35K-UNV-WH-4.ies,3' minimum with LH1 drivers,1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-375LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-375LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-375LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-375LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-375LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",375,375 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,13,13 Watts,FSM2PR-GR4-375LF-35K-UNV-WH-4.ies,"4' minimum with LU5, LH1, D11",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-625LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-625LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-625LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-625LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-625LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",625,625 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,22,22 Watts,FSM2PR-GR4-625LF-35K-UNV-WH-4.ies,"3' minimum with LU5, LH1 drivers",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-750LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-750LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-750LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-750LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-750LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",750,750 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,27,27 Watts,FSM2PR-GR4-750LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-875LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-875LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-875LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-875LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-875LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",875,875 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,32,32 Watts,FSM2PR-GR4-875LF-35K-UNV-LD1-G-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-27K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-27K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-27K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-27K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-27K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-27K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-27K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-27K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-27K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-27K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-27K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-27K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 80+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-30K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-30K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-30K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-30K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-30K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-30K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-30K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-30K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-30K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-30K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-30K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-30K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 80+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-35K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-35K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-35K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-35K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-35K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-35K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-35K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-35K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-35K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-35K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-35K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-35K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 80+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-40K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-40K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-40K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-40K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-40K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-40K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-40K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-40K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-40K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-40K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-40K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-40K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 80+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-927K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-927K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-927K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-927K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-927K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-927K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-927K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-927K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-927K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-927K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-927K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-927K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,2700,"2700K, 90+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-930K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-930K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-930K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-930K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-930K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-930K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-930K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-930K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-930K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-930K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-930K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-930K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3000,"3000K, 90+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-935K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-935K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-935K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-935K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-935K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-935K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-935K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-935K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-935K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-935K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-935K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-935K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,3500,"3500K, 90+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-940K-1C-LV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-940K-1C-LV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-940K-1C-LV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-940K-1C-LV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-940K-1C-LV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-940K-1C-LV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",12,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-940K-1C-UNV-LD1-G-x-WH,FSM2PR-FXH-GR4-1000LF-940K-1C-UNV-LD1-G-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Grid,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",0,0,1,1,0,0,0,4,0.2812
FSM2PR-FXH-GR4-1000LF-940K-1C-UNV-LD1-XFF-x-WH,FSM2PR-FXH-GR4-1000LF-940K-1C-UNV-LD1-XFF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Mud-in Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,1.1
FSM2PR-FXH-GR4-1000LF-940K-1C-UNV-LD1-XF-x-WH,FSM2PR-FXH-GR4-1000LF-940K-1C-UNV-LD1-XF-x-WH,"4.0"" Regress Grazer",1000,1000 Lumens per foot,4000,"4000K, 90+ CRI",120,Trimless Drywall,37,37 Watts,FSM2PR-GR4-1000LF-35K-UNV-WH-4.ies,"LD1,L11 and D11 only, 4' minimum",1,0,0,0,0,0,0,4,0.2812
