,Model##OTHER##,Shielding Type##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Color Temperature Note##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Voltage Comment##OTHER##,Driver##Other##,Driver Comment##OTHER##,Circuit##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Lumen Output Comment##OTHER##,Photometric Web File##OTHER##,Cable Suspension##Length##Inches,Mounting##Other##
FSM1IS-DC-250LF-27K-1C-UNV-xC24,FSM1IS-DC-250LF-27K-1C-UNV-xC24,Dust Cover,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-27K-1C-UNV-xC48,FSM1IS-DC-250LF-27K-1C-UNV-xC48,Dust Cover,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-27K-1C-UNV-xC96,FSM1IS-DC-250LF-27K-1C-UNV-xC96,Dust Cover,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-27K-1C-347-xC24,FSM1IS-DC-250LF-27K-1C-347-xC24,Dust Cover,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-27K-1C-347-xC48,FSM1IS-DC-250LF-27K-1C-347-xC48,Dust Cover,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-27K-1C-347-xC96,FSM1IS-DC-250LF-27K-1C-347-xC96,Dust Cover,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-927K-1C-UNV-xC24,FSM1IS-DC-250LF-927K-1C-UNV-xC24,Dust Cover,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-927K-1C-UNV-xC48,FSM1IS-DC-250LF-927K-1C-UNV-xC48,Dust Cover,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-927K-1C-UNV-xC96,FSM1IS-DC-250LF-927K-1C-UNV-xC96,Dust Cover,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-927K-1C-347-xC24,FSM1IS-DC-250LF-927K-1C-347-xC24,Dust Cover,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-927K-1C-347-xC48,FSM1IS-DC-250LF-927K-1C-347-xC48,Dust Cover,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-927K-1C-347-xC96,FSM1IS-DC-250LF-927K-1C-347-xC96,Dust Cover,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-30K-1C-UNV-xC24,FSM1IS-DC-250LF-30K-1C-UNV-xC24,Dust Cover,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-30K-1C-UNV-xC48,FSM1IS-DC-250LF-30K-1C-UNV-xC48,Dust Cover,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-30K-1C-UNV-xC96,FSM1IS-DC-250LF-30K-1C-UNV-xC96,Dust Cover,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-30K-1C-347-xC24,FSM1IS-DC-250LF-30K-1C-347-xC24,Dust Cover,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-30K-1C-347-xC48,FSM1IS-DC-250LF-30K-1C-347-xC48,Dust Cover,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-30K-1C-347-xC96,FSM1IS-DC-250LF-30K-1C-347-xC96,Dust Cover,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-930K-1C-UNV-xC24,FSM1IS-DC-250LF-930K-1C-UNV-xC24,Dust Cover,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-930K-1C-UNV-xC48,FSM1IS-DC-250LF-930K-1C-UNV-xC48,Dust Cover,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-930K-1C-UNV-xC96,FSM1IS-DC-250LF-930K-1C-UNV-xC96,Dust Cover,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-930K-1C-347-xC24,FSM1IS-DC-250LF-930K-1C-347-xC24,Dust Cover,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-930K-1C-347-xC48,FSM1IS-DC-250LF-930K-1C-347-xC48,Dust Cover,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-930K-1C-347-xC96,FSM1IS-DC-250LF-930K-1C-347-xC96,Dust Cover,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-35K-1C-UNV-xC24,FSM1IS-DC-250LF-35K-1C-UNV-xC24,Dust Cover,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-35K-1C-UNV-xC48,FSM1IS-DC-250LF-35K-1C-UNV-xC48,Dust Cover,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-35K-1C-UNV-xC96,FSM1IS-DC-250LF-35K-1C-UNV-xC96,Dust Cover,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-35K-1C-347-xC24,FSM1IS-DC-250LF-35K-1C-347-xC24,Dust Cover,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-35K-1C-347-xC48,FSM1IS-DC-250LF-35K-1C-347-xC48,Dust Cover,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-35K-1C-347-xC96,FSM1IS-DC-250LF-35K-1C-347-xC96,Dust Cover,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-935K-1C-UNV-xC24,FSM1IS-DC-250LF-935K-1C-UNV-xC24,Dust Cover,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-935K-1C-UNV-xC48,FSM1IS-DC-250LF-935K-1C-UNV-xC48,Dust Cover,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-935K-1C-UNV-xC96,FSM1IS-DC-250LF-935K-1C-UNV-xC96,Dust Cover,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-935K-1C-347-xC24,FSM1IS-DC-250LF-935K-1C-347-xC24,Dust Cover,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-935K-1C-347-xC48,FSM1IS-DC-250LF-935K-1C-347-xC48,Dust Cover,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-935K-1C-347-xC96,FSM1IS-DC-250LF-935K-1C-347-xC96,Dust Cover,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-40K-1C-UNV-xC24,FSM1IS-DC-250LF-40K-1C-UNV-xC24,Dust Cover,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-40K-1C-UNV-xC48,FSM1IS-DC-250LF-40K-1C-UNV-xC48,Dust Cover,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-40K-1C-UNV-xC96,FSM1IS-DC-250LF-40K-1C-UNV-xC96,Dust Cover,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-40K-1C-347-xC24,FSM1IS-DC-250LF-40K-1C-347-xC24,Dust Cover,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-40K-1C-347-xC48,FSM1IS-DC-250LF-40K-1C-347-xC48,Dust Cover,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-40K-1C-347-xC96,FSM1IS-DC-250LF-40K-1C-347-xC96,Dust Cover,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-940K-1C-UNV-xC24,FSM1IS-DC-250LF-940K-1C-UNV-xC24,Dust Cover,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-940K-1C-UNV-xC48,FSM1IS-DC-250LF-940K-1C-UNV-xC48,Dust Cover,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-940K-1C-UNV-xC96,FSM1IS-DC-250LF-940K-1C-UNV-xC96,Dust Cover,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-250LF-940K-1C-347-xC24,FSM1IS-DC-250LF-940K-1C-347-xC24,Dust Cover,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-250LF-940K-1C-347-xC48,FSM1IS-DC-250LF-940K-1C-347-xC48,Dust Cover,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-250LF-940K-1C-347-xC96,FSM1IS-DC-250LF-940K-1C-347-xC96,Dust Cover,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,8,8W,122,250 Lumens per foot.,FSM1IS-DC-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-27K-1C-UNV-xC24,FSM1IS-DC-375LF-27K-1C-UNV-xC24,Dust Cover,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-27K-1C-UNV-xC48,FSM1IS-DC-375LF-27K-1C-UNV-xC48,Dust Cover,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-27K-1C-UNV-xC96,FSM1IS-DC-375LF-27K-1C-UNV-xC96,Dust Cover,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-27K-1C-347-xC24,FSM1IS-DC-375LF-27K-1C-347-xC24,Dust Cover,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-27K-1C-347-xC48,FSM1IS-DC-375LF-27K-1C-347-xC48,Dust Cover,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-27K-1C-347-xC96,FSM1IS-DC-375LF-27K-1C-347-xC96,Dust Cover,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-927K-1C-UNV-xC24,FSM1IS-DC-375LF-927K-1C-UNV-xC24,Dust Cover,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-927K-1C-UNV-xC48,FSM1IS-DC-375LF-927K-1C-UNV-xC48,Dust Cover,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-927K-1C-UNV-xC96,FSM1IS-DC-375LF-927K-1C-UNV-xC96,Dust Cover,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-927K-1C-347-xC24,FSM1IS-DC-375LF-927K-1C-347-xC24,Dust Cover,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-927K-1C-347-xC48,FSM1IS-DC-375LF-927K-1C-347-xC48,Dust Cover,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-927K-1C-347-xC96,FSM1IS-DC-375LF-927K-1C-347-xC96,Dust Cover,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-30K-1C-UNV-xC24,FSM1IS-DC-375LF-30K-1C-UNV-xC24,Dust Cover,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-30K-1C-UNV-xC48,FSM1IS-DC-375LF-30K-1C-UNV-xC48,Dust Cover,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-30K-1C-UNV-xC96,FSM1IS-DC-375LF-30K-1C-UNV-xC96,Dust Cover,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-30K-1C-347-xC24,FSM1IS-DC-375LF-30K-1C-347-xC24,Dust Cover,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-30K-1C-347-xC48,FSM1IS-DC-375LF-30K-1C-347-xC48,Dust Cover,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-30K-1C-347-xC96,FSM1IS-DC-375LF-30K-1C-347-xC96,Dust Cover,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-930K-1C-UNV-xC24,FSM1IS-DC-375LF-930K-1C-UNV-xC24,Dust Cover,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-930K-1C-UNV-xC48,FSM1IS-DC-375LF-930K-1C-UNV-xC48,Dust Cover,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-930K-1C-UNV-xC96,FSM1IS-DC-375LF-930K-1C-UNV-xC96,Dust Cover,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-930K-1C-347-xC24,FSM1IS-DC-375LF-930K-1C-347-xC24,Dust Cover,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-930K-1C-347-xC48,FSM1IS-DC-375LF-930K-1C-347-xC48,Dust Cover,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-930K-1C-347-xC96,FSM1IS-DC-375LF-930K-1C-347-xC96,Dust Cover,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-35K-1C-UNV-xC24,FSM1IS-DC-375LF-35K-1C-UNV-xC24,Dust Cover,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-35K-1C-UNV-xC48,FSM1IS-DC-375LF-35K-1C-UNV-xC48,Dust Cover,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-35K-1C-UNV-xC96,FSM1IS-DC-375LF-35K-1C-UNV-xC96,Dust Cover,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-35K-1C-347-xC24,FSM1IS-DC-375LF-35K-1C-347-xC24,Dust Cover,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-35K-1C-347-xC48,FSM1IS-DC-375LF-35K-1C-347-xC48,Dust Cover,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-35K-1C-347-xC96,FSM1IS-DC-375LF-35K-1C-347-xC96,Dust Cover,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-935K-1C-UNV-xC24,FSM1IS-DC-375LF-935K-1C-UNV-xC24,Dust Cover,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-935K-1C-UNV-xC48,FSM1IS-DC-375LF-935K-1C-UNV-xC48,Dust Cover,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-935K-1C-UNV-xC96,FSM1IS-DC-375LF-935K-1C-UNV-xC96,Dust Cover,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-935K-1C-347-xC24,FSM1IS-DC-375LF-935K-1C-347-xC24,Dust Cover,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-935K-1C-347-xC48,FSM1IS-DC-375LF-935K-1C-347-xC48,Dust Cover,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-935K-1C-347-xC96,FSM1IS-DC-375LF-935K-1C-347-xC96,Dust Cover,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-40K-1C-UNV-xC24,FSM1IS-DC-375LF-40K-1C-UNV-xC24,Dust Cover,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-40K-1C-UNV-xC48,FSM1IS-DC-375LF-40K-1C-UNV-xC48,Dust Cover,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-40K-1C-UNV-xC96,FSM1IS-DC-375LF-40K-1C-UNV-xC96,Dust Cover,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-40K-1C-347-xC24,FSM1IS-DC-375LF-40K-1C-347-xC24,Dust Cover,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-40K-1C-347-xC48,FSM1IS-DC-375LF-40K-1C-347-xC48,Dust Cover,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-40K-1C-347-xC96,FSM1IS-DC-375LF-40K-1C-347-xC96,Dust Cover,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-940K-1C-UNV-xC24,FSM1IS-DC-375LF-940K-1C-UNV-xC24,Dust Cover,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-940K-1C-UNV-xC48,FSM1IS-DC-375LF-940K-1C-UNV-xC48,Dust Cover,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-940K-1C-UNV-xC96,FSM1IS-DC-375LF-940K-1C-UNV-xC96,Dust Cover,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-375LF-940K-1C-347-xC24,FSM1IS-DC-375LF-940K-1C-347-xC24,Dust Cover,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-375LF-940K-1C-347-xC48,FSM1IS-DC-375LF-940K-1C-347-xC48,Dust Cover,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-375LF-940K-1C-347-xC96,FSM1IS-DC-375LF-940K-1C-347-xC96,Dust Cover,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,130,350 Lumens per foot.,FSM1IS-DC-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-27K-1C-UNV-xC24,FSM1IS-DC-500LF-27K-1C-UNV-xC24,Dust Cover,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-27K-1C-UNV-xC48,FSM1IS-DC-500LF-27K-1C-UNV-xC48,Dust Cover,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-27K-1C-UNV-xC96,FSM1IS-DC-500LF-27K-1C-UNV-xC96,Dust Cover,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-27K-1C-347-xC24,FSM1IS-DC-500LF-27K-1C-347-xC24,Dust Cover,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-27K-1C-347-xC48,FSM1IS-DC-500LF-27K-1C-347-xC48,Dust Cover,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-27K-1C-347-xC96,FSM1IS-DC-500LF-27K-1C-347-xC96,Dust Cover,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-927K-1C-UNV-xC24,FSM1IS-DC-500LF-927K-1C-UNV-xC24,Dust Cover,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-927K-1C-UNV-xC48,FSM1IS-DC-500LF-927K-1C-UNV-xC48,Dust Cover,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-927K-1C-UNV-xC96,FSM1IS-DC-500LF-927K-1C-UNV-xC96,Dust Cover,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-927K-1C-347-xC24,FSM1IS-DC-500LF-927K-1C-347-xC24,Dust Cover,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-927K-1C-347-xC48,FSM1IS-DC-500LF-927K-1C-347-xC48,Dust Cover,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-927K-1C-347-xC96,FSM1IS-DC-500LF-927K-1C-347-xC96,Dust Cover,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-30K-1C-UNV-xC24,FSM1IS-DC-500LF-30K-1C-UNV-xC24,Dust Cover,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-30K-1C-UNV-xC48,FSM1IS-DC-500LF-30K-1C-UNV-xC48,Dust Cover,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-30K-1C-UNV-xC96,FSM1IS-DC-500LF-30K-1C-UNV-xC96,Dust Cover,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-30K-1C-347-xC24,FSM1IS-DC-500LF-30K-1C-347-xC24,Dust Cover,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-30K-1C-347-xC48,FSM1IS-DC-500LF-30K-1C-347-xC48,Dust Cover,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-30K-1C-347-xC96,FSM1IS-DC-500LF-30K-1C-347-xC96,Dust Cover,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-930K-1C-UNV-xC24,FSM1IS-DC-500LF-930K-1C-UNV-xC24,Dust Cover,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-930K-1C-UNV-xC48,FSM1IS-DC-500LF-930K-1C-UNV-xC48,Dust Cover,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-930K-1C-UNV-xC96,FSM1IS-DC-500LF-930K-1C-UNV-xC96,Dust Cover,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-930K-1C-347-xC24,FSM1IS-DC-500LF-930K-1C-347-xC24,Dust Cover,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-930K-1C-347-xC48,FSM1IS-DC-500LF-930K-1C-347-xC48,Dust Cover,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-930K-1C-347-xC96,FSM1IS-DC-500LF-930K-1C-347-xC96,Dust Cover,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-35K-1C-UNV-xC24,FSM1IS-DC-500LF-35K-1C-UNV-xC24,Dust Cover,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-35K-1C-UNV-xC48,FSM1IS-DC-500LF-35K-1C-UNV-xC48,Dust Cover,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-35K-1C-UNV-xC96,FSM1IS-DC-500LF-35K-1C-UNV-xC96,Dust Cover,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-35K-1C-347-xC24,FSM1IS-DC-500LF-35K-1C-347-xC24,Dust Cover,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-35K-1C-347-xC48,FSM1IS-DC-500LF-35K-1C-347-xC48,Dust Cover,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-35K-1C-347-xC96,FSM1IS-DC-500LF-35K-1C-347-xC96,Dust Cover,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-935K-1C-UNV-xC24,FSM1IS-DC-500LF-935K-1C-UNV-xC24,Dust Cover,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-935K-1C-UNV-xC48,FSM1IS-DC-500LF-935K-1C-UNV-xC48,Dust Cover,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-935K-1C-UNV-xC96,FSM1IS-DC-500LF-935K-1C-UNV-xC96,Dust Cover,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-935K-1C-347-xC24,FSM1IS-DC-500LF-935K-1C-347-xC24,Dust Cover,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-935K-1C-347-xC48,FSM1IS-DC-500LF-935K-1C-347-xC48,Dust Cover,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-935K-1C-347-xC96,FSM1IS-DC-500LF-935K-1C-347-xC96,Dust Cover,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-40K-1C-UNV-xC24,FSM1IS-DC-500LF-40K-1C-UNV-xC24,Dust Cover,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-40K-1C-UNV-xC48,FSM1IS-DC-500LF-40K-1C-UNV-xC48,Dust Cover,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-40K-1C-UNV-xC96,FSM1IS-DC-500LF-40K-1C-UNV-xC96,Dust Cover,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-40K-1C-347-xC24,FSM1IS-DC-500LF-40K-1C-347-xC24,Dust Cover,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-40K-1C-347-xC48,FSM1IS-DC-500LF-40K-1C-347-xC48,Dust Cover,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-40K-1C-347-xC96,FSM1IS-DC-500LF-40K-1C-347-xC96,Dust Cover,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-940K-1C-UNV-xC24,FSM1IS-DC-500LF-940K-1C-UNV-xC24,Dust Cover,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-940K-1C-UNV-xC48,FSM1IS-DC-500LF-940K-1C-UNV-xC48,Dust Cover,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-940K-1C-UNV-xC96,FSM1IS-DC-500LF-940K-1C-UNV-xC96,Dust Cover,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-500LF-940K-1C-347-xC24,FSM1IS-DC-500LF-940K-1C-347-xC24,Dust Cover,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-500LF-940K-1C-347-xC48,FSM1IS-DC-500LF-940K-1C-347-xC48,Dust Cover,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-500LF-940K-1C-347-xC96,FSM1IS-DC-500LF-940K-1C-347-xC96,Dust Cover,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,14,14W,137,500 Lumens per foot.,FSM1IS-DC-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-27K-1C-UNV-xC24,FSM1IS-DC-625LF-27K-1C-UNV-xC24,Dust Cover,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-27K-1C-UNV-xC48,FSM1IS-DC-625LF-27K-1C-UNV-xC48,Dust Cover,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-27K-1C-UNV-xC96,FSM1IS-DC-625LF-27K-1C-UNV-xC96,Dust Cover,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-27K-1C-347-xC24,FSM1IS-DC-625LF-27K-1C-347-xC24,Dust Cover,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-27K-1C-347-xC48,FSM1IS-DC-625LF-27K-1C-347-xC48,Dust Cover,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-27K-1C-347-xC96,FSM1IS-DC-625LF-27K-1C-347-xC96,Dust Cover,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-927K-1C-UNV-xC24,FSM1IS-DC-625LF-927K-1C-UNV-xC24,Dust Cover,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-927K-1C-UNV-xC48,FSM1IS-DC-625LF-927K-1C-UNV-xC48,Dust Cover,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-927K-1C-UNV-xC96,FSM1IS-DC-625LF-927K-1C-UNV-xC96,Dust Cover,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-927K-1C-347-xC24,FSM1IS-DC-625LF-927K-1C-347-xC24,Dust Cover,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-927K-1C-347-xC48,FSM1IS-DC-625LF-927K-1C-347-xC48,Dust Cover,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-927K-1C-347-xC96,FSM1IS-DC-625LF-927K-1C-347-xC96,Dust Cover,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-30K-1C-UNV-xC24,FSM1IS-DC-625LF-30K-1C-UNV-xC24,Dust Cover,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-30K-1C-UNV-xC48,FSM1IS-DC-625LF-30K-1C-UNV-xC48,Dust Cover,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-30K-1C-UNV-xC96,FSM1IS-DC-625LF-30K-1C-UNV-xC96,Dust Cover,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-30K-1C-347-xC24,FSM1IS-DC-625LF-30K-1C-347-xC24,Dust Cover,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-30K-1C-347-xC48,FSM1IS-DC-625LF-30K-1C-347-xC48,Dust Cover,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-30K-1C-347-xC96,FSM1IS-DC-625LF-30K-1C-347-xC96,Dust Cover,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-930K-1C-UNV-xC24,FSM1IS-DC-625LF-930K-1C-UNV-xC24,Dust Cover,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-930K-1C-UNV-xC48,FSM1IS-DC-625LF-930K-1C-UNV-xC48,Dust Cover,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-930K-1C-UNV-xC96,FSM1IS-DC-625LF-930K-1C-UNV-xC96,Dust Cover,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-930K-1C-347-xC24,FSM1IS-DC-625LF-930K-1C-347-xC24,Dust Cover,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-930K-1C-347-xC48,FSM1IS-DC-625LF-930K-1C-347-xC48,Dust Cover,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-930K-1C-347-xC96,FSM1IS-DC-625LF-930K-1C-347-xC96,Dust Cover,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-35K-1C-UNV-xC24,FSM1IS-DC-625LF-35K-1C-UNV-xC24,Dust Cover,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-35K-1C-UNV-xC48,FSM1IS-DC-625LF-35K-1C-UNV-xC48,Dust Cover,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-35K-1C-UNV-xC96,FSM1IS-DC-625LF-35K-1C-UNV-xC96,Dust Cover,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-35K-1C-347-xC24,FSM1IS-DC-625LF-35K-1C-347-xC24,Dust Cover,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-35K-1C-347-xC48,FSM1IS-DC-625LF-35K-1C-347-xC48,Dust Cover,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-35K-1C-347-xC96,FSM1IS-DC-625LF-35K-1C-347-xC96,Dust Cover,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-935K-1C-UNV-xC24,FSM1IS-DC-625LF-935K-1C-UNV-xC24,Dust Cover,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-935K-1C-UNV-xC48,FSM1IS-DC-625LF-935K-1C-UNV-xC48,Dust Cover,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-935K-1C-UNV-xC96,FSM1IS-DC-625LF-935K-1C-UNV-xC96,Dust Cover,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-935K-1C-347-xC24,FSM1IS-DC-625LF-935K-1C-347-xC24,Dust Cover,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-935K-1C-347-xC48,FSM1IS-DC-625LF-935K-1C-347-xC48,Dust Cover,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-935K-1C-347-xC96,FSM1IS-DC-625LF-935K-1C-347-xC96,Dust Cover,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-40K-1C-UNV-xC24,FSM1IS-DC-625LF-40K-1C-UNV-xC24,Dust Cover,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-40K-1C-UNV-xC48,FSM1IS-DC-625LF-40K-1C-UNV-xC48,Dust Cover,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-40K-1C-UNV-xC96,FSM1IS-DC-625LF-40K-1C-UNV-xC96,Dust Cover,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-40K-1C-347-xC24,FSM1IS-DC-625LF-40K-1C-347-xC24,Dust Cover,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-40K-1C-347-xC48,FSM1IS-DC-625LF-40K-1C-347-xC48,Dust Cover,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-40K-1C-347-xC96,FSM1IS-DC-625LF-40K-1C-347-xC96,Dust Cover,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-940K-1C-UNV-xC24,FSM1IS-DC-625LF-940K-1C-UNV-xC24,Dust Cover,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-940K-1C-UNV-xC48,FSM1IS-DC-625LF-940K-1C-UNV-xC48,Dust Cover,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-940K-1C-UNV-xC96,FSM1IS-DC-625LF-940K-1C-UNV-xC96,Dust Cover,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-625LF-940K-1C-347-xC24,FSM1IS-DC-625LF-940K-1C-347-xC24,Dust Cover,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-625LF-940K-1C-347-xC48,FSM1IS-DC-625LF-940K-1C-347-xC48,Dust Cover,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-625LF-940K-1C-347-xC96,FSM1IS-DC-625LF-940K-1C-347-xC96,Dust Cover,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,18,18W,140,625 Lumens per foot.,FSM1IS-DC-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-27K-1C-UNV-xC24,FSM1IS-DC-800LF-27K-1C-UNV-xC24,Dust Cover,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-27K-1C-UNV-xC48,FSM1IS-DC-800LF-27K-1C-UNV-xC48,Dust Cover,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-27K-1C-UNV-xC96,FSM1IS-DC-800LF-27K-1C-UNV-xC96,Dust Cover,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-27K-1C-347-xC24,FSM1IS-DC-800LF-27K-1C-347-xC24,Dust Cover,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-27K-1C-347-xC48,FSM1IS-DC-800LF-27K-1C-347-xC48,Dust Cover,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-27K-1C-347-xC96,FSM1IS-DC-800LF-27K-1C-347-xC96,Dust Cover,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-927K-1C-UNV-xC24,FSM1IS-DC-800LF-927K-1C-UNV-xC24,Dust Cover,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-927K-1C-UNV-xC48,FSM1IS-DC-800LF-927K-1C-UNV-xC48,Dust Cover,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-927K-1C-UNV-xC96,FSM1IS-DC-800LF-927K-1C-UNV-xC96,Dust Cover,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-927K-1C-347-xC24,FSM1IS-DC-800LF-927K-1C-347-xC24,Dust Cover,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-927K-1C-347-xC48,FSM1IS-DC-800LF-927K-1C-347-xC48,Dust Cover,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-927K-1C-347-xC96,FSM1IS-DC-800LF-927K-1C-347-xC96,Dust Cover,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-30K-1C-UNV-xC24,FSM1IS-DC-800LF-30K-1C-UNV-xC24,Dust Cover,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-30K-1C-UNV-xC48,FSM1IS-DC-800LF-30K-1C-UNV-xC48,Dust Cover,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-30K-1C-UNV-xC96,FSM1IS-DC-800LF-30K-1C-UNV-xC96,Dust Cover,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-30K-1C-347-xC24,FSM1IS-DC-800LF-30K-1C-347-xC24,Dust Cover,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-30K-1C-347-xC48,FSM1IS-DC-800LF-30K-1C-347-xC48,Dust Cover,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-30K-1C-347-xC96,FSM1IS-DC-800LF-30K-1C-347-xC96,Dust Cover,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-930K-1C-UNV-xC24,FSM1IS-DC-800LF-930K-1C-UNV-xC24,Dust Cover,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-930K-1C-UNV-xC48,FSM1IS-DC-800LF-930K-1C-UNV-xC48,Dust Cover,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-930K-1C-UNV-xC96,FSM1IS-DC-800LF-930K-1C-UNV-xC96,Dust Cover,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-930K-1C-347-xC24,FSM1IS-DC-800LF-930K-1C-347-xC24,Dust Cover,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-930K-1C-347-xC48,FSM1IS-DC-800LF-930K-1C-347-xC48,Dust Cover,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-930K-1C-347-xC96,FSM1IS-DC-800LF-930K-1C-347-xC96,Dust Cover,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-35K-1C-UNV-xC24,FSM1IS-DC-800LF-35K-1C-UNV-xC24,Dust Cover,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-35K-1C-UNV-xC48,FSM1IS-DC-800LF-35K-1C-UNV-xC48,Dust Cover,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-35K-1C-UNV-xC96,FSM1IS-DC-800LF-35K-1C-UNV-xC96,Dust Cover,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-35K-1C-347-xC24,FSM1IS-DC-800LF-35K-1C-347-xC24,Dust Cover,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-35K-1C-347-xC48,FSM1IS-DC-800LF-35K-1C-347-xC48,Dust Cover,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-35K-1C-347-xC96,FSM1IS-DC-800LF-35K-1C-347-xC96,Dust Cover,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-935K-1C-UNV-xC24,FSM1IS-DC-800LF-935K-1C-UNV-xC24,Dust Cover,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-935K-1C-UNV-xC48,FSM1IS-DC-800LF-935K-1C-UNV-xC48,Dust Cover,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-935K-1C-UNV-xC96,FSM1IS-DC-800LF-935K-1C-UNV-xC96,Dust Cover,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-935K-1C-347-xC24,FSM1IS-DC-800LF-935K-1C-347-xC24,Dust Cover,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-935K-1C-347-xC48,FSM1IS-DC-800LF-935K-1C-347-xC48,Dust Cover,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-935K-1C-347-xC96,FSM1IS-DC-800LF-935K-1C-347-xC96,Dust Cover,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-40K-1C-UNV-xC24,FSM1IS-DC-800LF-40K-1C-UNV-xC24,Dust Cover,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-40K-1C-UNV-xC48,FSM1IS-DC-800LF-40K-1C-UNV-xC48,Dust Cover,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-40K-1C-UNV-xC96,FSM1IS-DC-800LF-40K-1C-UNV-xC96,Dust Cover,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-40K-1C-347-xC24,FSM1IS-DC-800LF-40K-1C-347-xC24,Dust Cover,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-40K-1C-347-xC48,FSM1IS-DC-800LF-40K-1C-347-xC48,Dust Cover,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-40K-1C-347-xC96,FSM1IS-DC-800LF-40K-1C-347-xC96,Dust Cover,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-940K-1C-UNV-xC24,FSM1IS-DC-800LF-940K-1C-UNV-xC24,Dust Cover,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-940K-1C-UNV-xC48,FSM1IS-DC-800LF-940K-1C-UNV-xC48,Dust Cover,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-940K-1C-UNV-xC96,FSM1IS-DC-800LF-940K-1C-UNV-xC96,Dust Cover,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-800LF-940K-1C-347-xC24,FSM1IS-DC-800LF-940K-1C-347-xC24,Dust Cover,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-800LF-940K-1C-347-xC48,FSM1IS-DC-800LF-940K-1C-347-xC48,Dust Cover,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-800LF-940K-1C-347-xC96,FSM1IS-DC-800LF-940K-1C-347-xC96,Dust Cover,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,24,24W,136,800 Lumens per foot,FSM1IS-DC-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-27K-1C-UNV-xC24,FSM1IS-DC-1000LF-27K-1C-UNV-xC24,Dust Cover,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-27K-1C-UNV-xC48,FSM1IS-DC-1000LF-27K-1C-UNV-xC48,Dust Cover,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-27K-1C-UNV-xC96,FSM1IS-DC-1000LF-27K-1C-UNV-xC96,Dust Cover,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-27K-1C-347-xC24,FSM1IS-DC-1000LF-27K-1C-347-xC24,Dust Cover,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-27K-1C-347-xC48,FSM1IS-DC-1000LF-27K-1C-347-xC48,Dust Cover,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-27K-1C-347-xC96,FSM1IS-DC-1000LF-27K-1C-347-xC96,Dust Cover,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-927K-1C-UNV-xC24,FSM1IS-DC-1000LF-927K-1C-UNV-xC24,Dust Cover,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-927K-1C-UNV-xC48,FSM1IS-DC-1000LF-927K-1C-UNV-xC48,Dust Cover,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-927K-1C-UNV-xC96,FSM1IS-DC-1000LF-927K-1C-UNV-xC96,Dust Cover,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-927K-1C-347-xC24,FSM1IS-DC-1000LF-927K-1C-347-xC24,Dust Cover,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-927K-1C-347-xC48,FSM1IS-DC-1000LF-927K-1C-347-xC48,Dust Cover,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-927K-1C-347-xC96,FSM1IS-DC-1000LF-927K-1C-347-xC96,Dust Cover,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-30K-1C-UNV-xC24,FSM1IS-DC-1000LF-30K-1C-UNV-xC24,Dust Cover,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-30K-1C-UNV-xC48,FSM1IS-DC-1000LF-30K-1C-UNV-xC48,Dust Cover,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-30K-1C-UNV-xC96,FSM1IS-DC-1000LF-30K-1C-UNV-xC96,Dust Cover,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-30K-1C-347-xC24,FSM1IS-DC-1000LF-30K-1C-347-xC24,Dust Cover,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-30K-1C-347-xC48,FSM1IS-DC-1000LF-30K-1C-347-xC48,Dust Cover,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-30K-1C-347-xC96,FSM1IS-DC-1000LF-30K-1C-347-xC96,Dust Cover,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-930K-1C-UNV-xC24,FSM1IS-DC-1000LF-930K-1C-UNV-xC24,Dust Cover,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-930K-1C-UNV-xC48,FSM1IS-DC-1000LF-930K-1C-UNV-xC48,Dust Cover,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-930K-1C-UNV-xC96,FSM1IS-DC-1000LF-930K-1C-UNV-xC96,Dust Cover,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-930K-1C-347-xC24,FSM1IS-DC-1000LF-930K-1C-347-xC24,Dust Cover,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-930K-1C-347-xC48,FSM1IS-DC-1000LF-930K-1C-347-xC48,Dust Cover,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-930K-1C-347-xC96,FSM1IS-DC-1000LF-930K-1C-347-xC96,Dust Cover,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-35K-1C-UNV-xC24,FSM1IS-DC-1000LF-35K-1C-UNV-xC24,Dust Cover,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-35K-1C-UNV-xC48,FSM1IS-DC-1000LF-35K-1C-UNV-xC48,Dust Cover,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-35K-1C-UNV-xC96,FSM1IS-DC-1000LF-35K-1C-UNV-xC96,Dust Cover,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-35K-1C-347-xC24,FSM1IS-DC-1000LF-35K-1C-347-xC24,Dust Cover,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-35K-1C-347-xC48,FSM1IS-DC-1000LF-35K-1C-347-xC48,Dust Cover,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-35K-1C-347-xC96,FSM1IS-DC-1000LF-35K-1C-347-xC96,Dust Cover,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-935K-1C-UNV-xC24,FSM1IS-DC-1000LF-935K-1C-UNV-xC24,Dust Cover,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-935K-1C-UNV-xC48,FSM1IS-DC-1000LF-935K-1C-UNV-xC48,Dust Cover,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-935K-1C-UNV-xC96,FSM1IS-DC-1000LF-935K-1C-UNV-xC96,Dust Cover,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-935K-1C-347-xC24,FSM1IS-DC-1000LF-935K-1C-347-xC24,Dust Cover,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-935K-1C-347-xC48,FSM1IS-DC-1000LF-935K-1C-347-xC48,Dust Cover,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-935K-1C-347-xC96,FSM1IS-DC-1000LF-935K-1C-347-xC96,Dust Cover,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-40K-1C-UNV-xC24,FSM1IS-DC-1000LF-40K-1C-UNV-xC24,Dust Cover,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-40K-1C-UNV-xC48,FSM1IS-DC-1000LF-40K-1C-UNV-xC48,Dust Cover,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-40K-1C-UNV-xC96,FSM1IS-DC-1000LF-40K-1C-UNV-xC96,Dust Cover,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-40K-1C-347-xC24,FSM1IS-DC-1000LF-40K-1C-347-xC24,Dust Cover,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-40K-1C-347-xC48,FSM1IS-DC-1000LF-40K-1C-347-xC48,Dust Cover,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-40K-1C-347-xC96,FSM1IS-DC-1000LF-40K-1C-347-xC96,Dust Cover,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-940K-1C-UNV-xC24,FSM1IS-DC-1000LF-940K-1C-UNV-xC24,Dust Cover,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-940K-1C-UNV-xC48,FSM1IS-DC-1000LF-940K-1C-UNV-xC48,Dust Cover,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-940K-1C-UNV-xC96,FSM1IS-DC-1000LF-940K-1C-UNV-xC96,Dust Cover,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1000LF-940K-1C-347-xC24,FSM1IS-DC-1000LF-940K-1C-347-xC24,Dust Cover,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1000LF-940K-1C-347-xC48,FSM1IS-DC-1000LF-940K-1C-347-xC48,Dust Cover,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1000LF-940K-1C-347-xC96,FSM1IS-DC-1000LF-940K-1C-347-xC96,Dust Cover,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,30,30W,136,1000 Lumens per foot. Not available with DALI.,FSM1IS-DC-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-27K-1C-UNV-xC24,FSM1IS-DC-1250LF-27K-1C-UNV-xC24,Dust Cover,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-27K-1C-UNV-xC48,FSM1IS-DC-1250LF-27K-1C-UNV-xC48,Dust Cover,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-27K-1C-UNV-xC96,FSM1IS-DC-1250LF-27K-1C-UNV-xC96,Dust Cover,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-27K-1C-347-xC24,FSM1IS-DC-1250LF-27K-1C-347-xC24,Dust Cover,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-27K-1C-347-xC48,FSM1IS-DC-1250LF-27K-1C-347-xC48,Dust Cover,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-27K-1C-347-xC96,FSM1IS-DC-1250LF-27K-1C-347-xC96,Dust Cover,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-927K-1C-UNV-xC24,FSM1IS-DC-1250LF-927K-1C-UNV-xC24,Dust Cover,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-927K-1C-UNV-xC48,FSM1IS-DC-1250LF-927K-1C-UNV-xC48,Dust Cover,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-927K-1C-UNV-xC96,FSM1IS-DC-1250LF-927K-1C-UNV-xC96,Dust Cover,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-927K-1C-347-xC24,FSM1IS-DC-1250LF-927K-1C-347-xC24,Dust Cover,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-927K-1C-347-xC48,FSM1IS-DC-1250LF-927K-1C-347-xC48,Dust Cover,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-927K-1C-347-xC96,FSM1IS-DC-1250LF-927K-1C-347-xC96,Dust Cover,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-30K-1C-UNV-xC24,FSM1IS-DC-1250LF-30K-1C-UNV-xC24,Dust Cover,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-30K-1C-UNV-xC48,FSM1IS-DC-1250LF-30K-1C-UNV-xC48,Dust Cover,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-30K-1C-UNV-xC96,FSM1IS-DC-1250LF-30K-1C-UNV-xC96,Dust Cover,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-30K-1C-347-xC24,FSM1IS-DC-1250LF-30K-1C-347-xC24,Dust Cover,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-30K-1C-347-xC48,FSM1IS-DC-1250LF-30K-1C-347-xC48,Dust Cover,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-30K-1C-347-xC96,FSM1IS-DC-1250LF-30K-1C-347-xC96,Dust Cover,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-930K-1C-UNV-xC24,FSM1IS-DC-1250LF-930K-1C-UNV-xC24,Dust Cover,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-930K-1C-UNV-xC48,FSM1IS-DC-1250LF-930K-1C-UNV-xC48,Dust Cover,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-930K-1C-UNV-xC96,FSM1IS-DC-1250LF-930K-1C-UNV-xC96,Dust Cover,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-930K-1C-347-xC24,FSM1IS-DC-1250LF-930K-1C-347-xC24,Dust Cover,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-930K-1C-347-xC48,FSM1IS-DC-1250LF-930K-1C-347-xC48,Dust Cover,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-930K-1C-347-xC96,FSM1IS-DC-1250LF-930K-1C-347-xC96,Dust Cover,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-35K-1C-UNV-xC24,FSM1IS-DC-1250LF-35K-1C-UNV-xC24,Dust Cover,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-35K-1C-UNV-xC48,FSM1IS-DC-1250LF-35K-1C-UNV-xC48,Dust Cover,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-35K-1C-UNV-xC96,FSM1IS-DC-1250LF-35K-1C-UNV-xC96,Dust Cover,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-35K-1C-347-xC24,FSM1IS-DC-1250LF-35K-1C-347-xC24,Dust Cover,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-35K-1C-347-xC48,FSM1IS-DC-1250LF-35K-1C-347-xC48,Dust Cover,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-35K-1C-347-xC96,FSM1IS-DC-1250LF-35K-1C-347-xC96,Dust Cover,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-935K-1C-UNV-xC24,FSM1IS-DC-1250LF-935K-1C-UNV-xC24,Dust Cover,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-935K-1C-UNV-xC48,FSM1IS-DC-1250LF-935K-1C-UNV-xC48,Dust Cover,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-935K-1C-UNV-xC96,FSM1IS-DC-1250LF-935K-1C-UNV-xC96,Dust Cover,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-935K-1C-347-xC24,FSM1IS-DC-1250LF-935K-1C-347-xC24,Dust Cover,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-935K-1C-347-xC48,FSM1IS-DC-1250LF-935K-1C-347-xC48,Dust Cover,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-935K-1C-347-xC96,FSM1IS-DC-1250LF-935K-1C-347-xC96,Dust Cover,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-40K-1C-UNV-xC24,FSM1IS-DC-1250LF-40K-1C-UNV-xC24,Dust Cover,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-40K-1C-UNV-xC48,FSM1IS-DC-1250LF-40K-1C-UNV-xC48,Dust Cover,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-40K-1C-UNV-xC96,FSM1IS-DC-1250LF-40K-1C-UNV-xC96,Dust Cover,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-40K-1C-347-xC24,FSM1IS-DC-1250LF-40K-1C-347-xC24,Dust Cover,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-40K-1C-347-xC48,FSM1IS-DC-1250LF-40K-1C-347-xC48,Dust Cover,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-40K-1C-347-xC96,FSM1IS-DC-1250LF-40K-1C-347-xC96,Dust Cover,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-940K-1C-UNV-xC24,FSM1IS-DC-1250LF-940K-1C-UNV-xC24,Dust Cover,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-940K-1C-UNV-xC48,FSM1IS-DC-1250LF-940K-1C-UNV-xC48,Dust Cover,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-940K-1C-UNV-xC96,FSM1IS-DC-1250LF-940K-1C-UNV-xC96,Dust Cover,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-DC-1250LF-940K-1C-347-xC24,FSM1IS-DC-1250LF-940K-1C-347-xC24,Dust Cover,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-DC-1250LF-940K-1C-347-xC48,FSM1IS-DC-1250LF-940K-1C-347-xC48,Dust Cover,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-DC-1250LF-940K-1C-347-xC96,FSM1IS-DC-1250LF-940K-1C-347-xC96,Dust Cover,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,131,1250 Lumens per foot. Not available with DALI.,FSM1IS-DC-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-27K-1C-UNV-xC24,FSM1IS-BW-250LF-27K-1C-UNV-xC24,Batwing Optic,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-27K-1C-UNV-xC48,FSM1IS-BW-250LF-27K-1C-UNV-xC48,Batwing Optic,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-27K-1C-UNV-xC96,FSM1IS-BW-250LF-27K-1C-UNV-xC96,Batwing Optic,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-27K-1C-347-xC24,FSM1IS-BW-250LF-27K-1C-347-xC24,Batwing Optic,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-27K-1C-347-xC48,FSM1IS-BW-250LF-27K-1C-347-xC48,Batwing Optic,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-27K-1C-347-xC96,FSM1IS-BW-250LF-27K-1C-347-xC96,Batwing Optic,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-927K-1C-UNV-xC24,FSM1IS-BW-250LF-927K-1C-UNV-xC24,Batwing Optic,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-927K-1C-UNV-xC48,FSM1IS-BW-250LF-927K-1C-UNV-xC48,Batwing Optic,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-927K-1C-UNV-xC96,FSM1IS-BW-250LF-927K-1C-UNV-xC96,Batwing Optic,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-927K-1C-347-xC24,FSM1IS-BW-250LF-927K-1C-347-xC24,Batwing Optic,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-927K-1C-347-xC48,FSM1IS-BW-250LF-927K-1C-347-xC48,Batwing Optic,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-927K-1C-347-xC96,FSM1IS-BW-250LF-927K-1C-347-xC96,Batwing Optic,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-30K-1C-UNV-xC24,FSM1IS-BW-250LF-30K-1C-UNV-xC24,Batwing Optic,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-30K-1C-UNV-xC48,FSM1IS-BW-250LF-30K-1C-UNV-xC48,Batwing Optic,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-30K-1C-UNV-xC96,FSM1IS-BW-250LF-30K-1C-UNV-xC96,Batwing Optic,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-30K-1C-347-xC24,FSM1IS-BW-250LF-30K-1C-347-xC24,Batwing Optic,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-30K-1C-347-xC48,FSM1IS-BW-250LF-30K-1C-347-xC48,Batwing Optic,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-30K-1C-347-xC96,FSM1IS-BW-250LF-30K-1C-347-xC96,Batwing Optic,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-930K-1C-UNV-xC24,FSM1IS-BW-250LF-930K-1C-UNV-xC24,Batwing Optic,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-930K-1C-UNV-xC48,FSM1IS-BW-250LF-930K-1C-UNV-xC48,Batwing Optic,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-930K-1C-UNV-xC96,FSM1IS-BW-250LF-930K-1C-UNV-xC96,Batwing Optic,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-930K-1C-347-xC24,FSM1IS-BW-250LF-930K-1C-347-xC24,Batwing Optic,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-930K-1C-347-xC48,FSM1IS-BW-250LF-930K-1C-347-xC48,Batwing Optic,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-930K-1C-347-xC96,FSM1IS-BW-250LF-930K-1C-347-xC96,Batwing Optic,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-35K-1C-UNV-xC24,FSM1IS-BW-250LF-35K-1C-UNV-xC24,Batwing Optic,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-35K-1C-UNV-xC48,FSM1IS-BW-250LF-35K-1C-UNV-xC48,Batwing Optic,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-35K-1C-UNV-xC96,FSM1IS-BW-250LF-35K-1C-UNV-xC96,Batwing Optic,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-35K-1C-347-xC24,FSM1IS-BW-250LF-35K-1C-347-xC24,Batwing Optic,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-35K-1C-347-xC48,FSM1IS-BW-250LF-35K-1C-347-xC48,Batwing Optic,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-35K-1C-347-xC96,FSM1IS-BW-250LF-35K-1C-347-xC96,Batwing Optic,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-935K-1C-UNV-xC24,FSM1IS-BW-250LF-935K-1C-UNV-xC24,Batwing Optic,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-935K-1C-UNV-xC48,FSM1IS-BW-250LF-935K-1C-UNV-xC48,Batwing Optic,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-935K-1C-UNV-xC96,FSM1IS-BW-250LF-935K-1C-UNV-xC96,Batwing Optic,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-935K-1C-347-xC24,FSM1IS-BW-250LF-935K-1C-347-xC24,Batwing Optic,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-935K-1C-347-xC48,FSM1IS-BW-250LF-935K-1C-347-xC48,Batwing Optic,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-935K-1C-347-xC96,FSM1IS-BW-250LF-935K-1C-347-xC96,Batwing Optic,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-40K-1C-UNV-xC24,FSM1IS-BW-250LF-40K-1C-UNV-xC24,Batwing Optic,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-40K-1C-UNV-xC48,FSM1IS-BW-250LF-40K-1C-UNV-xC48,Batwing Optic,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-40K-1C-UNV-xC96,FSM1IS-BW-250LF-40K-1C-UNV-xC96,Batwing Optic,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-40K-1C-347-xC24,FSM1IS-BW-250LF-40K-1C-347-xC24,Batwing Optic,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-40K-1C-347-xC48,FSM1IS-BW-250LF-40K-1C-347-xC48,Batwing Optic,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-40K-1C-347-xC96,FSM1IS-BW-250LF-40K-1C-347-xC96,Batwing Optic,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-940K-1C-UNV-xC24,FSM1IS-BW-250LF-940K-1C-UNV-xC24,Batwing Optic,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-940K-1C-UNV-xC48,FSM1IS-BW-250LF-940K-1C-UNV-xC48,Batwing Optic,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-940K-1C-UNV-xC96,FSM1IS-BW-250LF-940K-1C-UNV-xC96,Batwing Optic,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-250LF-940K-1C-347-xC24,FSM1IS-BW-250LF-940K-1C-347-xC24,Batwing Optic,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-250LF-940K-1C-347-xC48,FSM1IS-BW-250LF-940K-1C-347-xC48,Batwing Optic,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-250LF-940K-1C-347-xC96,FSM1IS-BW-250LF-940K-1C-347-xC96,Batwing Optic,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,119,250 Lumens per foot.,FSM1IS-BW-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-27K-1C-UNV-xC24,FSM1IS-BW-375LF-27K-1C-UNV-xC24,Batwing Optic,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-27K-1C-UNV-xC48,FSM1IS-BW-375LF-27K-1C-UNV-xC48,Batwing Optic,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-27K-1C-UNV-xC96,FSM1IS-BW-375LF-27K-1C-UNV-xC96,Batwing Optic,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-27K-1C-347-xC24,FSM1IS-BW-375LF-27K-1C-347-xC24,Batwing Optic,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-27K-1C-347-xC48,FSM1IS-BW-375LF-27K-1C-347-xC48,Batwing Optic,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-27K-1C-347-xC96,FSM1IS-BW-375LF-27K-1C-347-xC96,Batwing Optic,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-927K-1C-UNV-xC24,FSM1IS-BW-375LF-927K-1C-UNV-xC24,Batwing Optic,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-927K-1C-UNV-xC48,FSM1IS-BW-375LF-927K-1C-UNV-xC48,Batwing Optic,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-927K-1C-UNV-xC96,FSM1IS-BW-375LF-927K-1C-UNV-xC96,Batwing Optic,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-927K-1C-347-xC24,FSM1IS-BW-375LF-927K-1C-347-xC24,Batwing Optic,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-927K-1C-347-xC48,FSM1IS-BW-375LF-927K-1C-347-xC48,Batwing Optic,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-927K-1C-347-xC96,FSM1IS-BW-375LF-927K-1C-347-xC96,Batwing Optic,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-30K-1C-UNV-xC24,FSM1IS-BW-375LF-30K-1C-UNV-xC24,Batwing Optic,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-30K-1C-UNV-xC48,FSM1IS-BW-375LF-30K-1C-UNV-xC48,Batwing Optic,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-30K-1C-UNV-xC96,FSM1IS-BW-375LF-30K-1C-UNV-xC96,Batwing Optic,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-30K-1C-347-xC24,FSM1IS-BW-375LF-30K-1C-347-xC24,Batwing Optic,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-30K-1C-347-xC48,FSM1IS-BW-375LF-30K-1C-347-xC48,Batwing Optic,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-30K-1C-347-xC96,FSM1IS-BW-375LF-30K-1C-347-xC96,Batwing Optic,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-930K-1C-UNV-xC24,FSM1IS-BW-375LF-930K-1C-UNV-xC24,Batwing Optic,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-930K-1C-UNV-xC48,FSM1IS-BW-375LF-930K-1C-UNV-xC48,Batwing Optic,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-930K-1C-UNV-xC96,FSM1IS-BW-375LF-930K-1C-UNV-xC96,Batwing Optic,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-930K-1C-347-xC24,FSM1IS-BW-375LF-930K-1C-347-xC24,Batwing Optic,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-930K-1C-347-xC48,FSM1IS-BW-375LF-930K-1C-347-xC48,Batwing Optic,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-930K-1C-347-xC96,FSM1IS-BW-375LF-930K-1C-347-xC96,Batwing Optic,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-35K-1C-UNV-xC24,FSM1IS-BW-375LF-35K-1C-UNV-xC24,Batwing Optic,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-35K-1C-UNV-xC48,FSM1IS-BW-375LF-35K-1C-UNV-xC48,Batwing Optic,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-35K-1C-UNV-xC96,FSM1IS-BW-375LF-35K-1C-UNV-xC96,Batwing Optic,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-35K-1C-347-xC24,FSM1IS-BW-375LF-35K-1C-347-xC24,Batwing Optic,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-35K-1C-347-xC48,FSM1IS-BW-375LF-35K-1C-347-xC48,Batwing Optic,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-35K-1C-347-xC96,FSM1IS-BW-375LF-35K-1C-347-xC96,Batwing Optic,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-935K-1C-UNV-xC24,FSM1IS-BW-375LF-935K-1C-UNV-xC24,Batwing Optic,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-935K-1C-UNV-xC48,FSM1IS-BW-375LF-935K-1C-UNV-xC48,Batwing Optic,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-935K-1C-UNV-xC96,FSM1IS-BW-375LF-935K-1C-UNV-xC96,Batwing Optic,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-935K-1C-347-xC24,FSM1IS-BW-375LF-935K-1C-347-xC24,Batwing Optic,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-935K-1C-347-xC48,FSM1IS-BW-375LF-935K-1C-347-xC48,Batwing Optic,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-935K-1C-347-xC96,FSM1IS-BW-375LF-935K-1C-347-xC96,Batwing Optic,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-40K-1C-UNV-xC24,FSM1IS-BW-375LF-40K-1C-UNV-xC24,Batwing Optic,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-40K-1C-UNV-xC48,FSM1IS-BW-375LF-40K-1C-UNV-xC48,Batwing Optic,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-40K-1C-UNV-xC96,FSM1IS-BW-375LF-40K-1C-UNV-xC96,Batwing Optic,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-40K-1C-347-xC24,FSM1IS-BW-375LF-40K-1C-347-xC24,Batwing Optic,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-40K-1C-347-xC48,FSM1IS-BW-375LF-40K-1C-347-xC48,Batwing Optic,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-40K-1C-347-xC96,FSM1IS-BW-375LF-40K-1C-347-xC96,Batwing Optic,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-940K-1C-UNV-xC24,FSM1IS-BW-375LF-940K-1C-UNV-xC24,Batwing Optic,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-940K-1C-UNV-xC48,FSM1IS-BW-375LF-940K-1C-UNV-xC48,Batwing Optic,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-940K-1C-UNV-xC96,FSM1IS-BW-375LF-940K-1C-UNV-xC96,Batwing Optic,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-375LF-940K-1C-347-xC24,FSM1IS-BW-375LF-940K-1C-347-xC24,Batwing Optic,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-375LF-940K-1C-347-xC48,FSM1IS-BW-375LF-940K-1C-347-xC48,Batwing Optic,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-375LF-940K-1C-347-xC96,FSM1IS-BW-375LF-940K-1C-347-xC96,Batwing Optic,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,127,350 Lumens per foot.,FSM1IS-BW-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-27K-1C-UNV-xC24,FSM1IS-BW-500LF-27K-1C-UNV-xC24,Batwing Optic,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-27K-1C-UNV-xC48,FSM1IS-BW-500LF-27K-1C-UNV-xC48,Batwing Optic,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-27K-1C-UNV-xC96,FSM1IS-BW-500LF-27K-1C-UNV-xC96,Batwing Optic,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-27K-1C-347-xC24,FSM1IS-BW-500LF-27K-1C-347-xC24,Batwing Optic,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-27K-1C-347-xC48,FSM1IS-BW-500LF-27K-1C-347-xC48,Batwing Optic,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-27K-1C-347-xC96,FSM1IS-BW-500LF-27K-1C-347-xC96,Batwing Optic,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-927K-1C-UNV-xC24,FSM1IS-BW-500LF-927K-1C-UNV-xC24,Batwing Optic,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-927K-1C-UNV-xC48,FSM1IS-BW-500LF-927K-1C-UNV-xC48,Batwing Optic,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-927K-1C-UNV-xC96,FSM1IS-BW-500LF-927K-1C-UNV-xC96,Batwing Optic,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-927K-1C-347-xC24,FSM1IS-BW-500LF-927K-1C-347-xC24,Batwing Optic,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-927K-1C-347-xC48,FSM1IS-BW-500LF-927K-1C-347-xC48,Batwing Optic,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-927K-1C-347-xC96,FSM1IS-BW-500LF-927K-1C-347-xC96,Batwing Optic,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-30K-1C-UNV-xC24,FSM1IS-BW-500LF-30K-1C-UNV-xC24,Batwing Optic,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-30K-1C-UNV-xC48,FSM1IS-BW-500LF-30K-1C-UNV-xC48,Batwing Optic,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-30K-1C-UNV-xC96,FSM1IS-BW-500LF-30K-1C-UNV-xC96,Batwing Optic,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-30K-1C-347-xC24,FSM1IS-BW-500LF-30K-1C-347-xC24,Batwing Optic,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-30K-1C-347-xC48,FSM1IS-BW-500LF-30K-1C-347-xC48,Batwing Optic,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-30K-1C-347-xC96,FSM1IS-BW-500LF-30K-1C-347-xC96,Batwing Optic,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-930K-1C-UNV-xC24,FSM1IS-BW-500LF-930K-1C-UNV-xC24,Batwing Optic,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-930K-1C-UNV-xC48,FSM1IS-BW-500LF-930K-1C-UNV-xC48,Batwing Optic,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-930K-1C-UNV-xC96,FSM1IS-BW-500LF-930K-1C-UNV-xC96,Batwing Optic,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-930K-1C-347-xC24,FSM1IS-BW-500LF-930K-1C-347-xC24,Batwing Optic,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-930K-1C-347-xC48,FSM1IS-BW-500LF-930K-1C-347-xC48,Batwing Optic,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-930K-1C-347-xC96,FSM1IS-BW-500LF-930K-1C-347-xC96,Batwing Optic,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-35K-1C-UNV-xC24,FSM1IS-BW-500LF-35K-1C-UNV-xC24,Batwing Optic,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-35K-1C-UNV-xC48,FSM1IS-BW-500LF-35K-1C-UNV-xC48,Batwing Optic,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-35K-1C-UNV-xC96,FSM1IS-BW-500LF-35K-1C-UNV-xC96,Batwing Optic,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-35K-1C-347-xC24,FSM1IS-BW-500LF-35K-1C-347-xC24,Batwing Optic,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-35K-1C-347-xC48,FSM1IS-BW-500LF-35K-1C-347-xC48,Batwing Optic,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-35K-1C-347-xC96,FSM1IS-BW-500LF-35K-1C-347-xC96,Batwing Optic,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-935K-1C-UNV-xC24,FSM1IS-BW-500LF-935K-1C-UNV-xC24,Batwing Optic,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-935K-1C-UNV-xC48,FSM1IS-BW-500LF-935K-1C-UNV-xC48,Batwing Optic,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-935K-1C-UNV-xC96,FSM1IS-BW-500LF-935K-1C-UNV-xC96,Batwing Optic,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-935K-1C-347-xC24,FSM1IS-BW-500LF-935K-1C-347-xC24,Batwing Optic,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-935K-1C-347-xC48,FSM1IS-BW-500LF-935K-1C-347-xC48,Batwing Optic,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-935K-1C-347-xC96,FSM1IS-BW-500LF-935K-1C-347-xC96,Batwing Optic,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-40K-1C-UNV-xC24,FSM1IS-BW-500LF-40K-1C-UNV-xC24,Batwing Optic,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-40K-1C-UNV-xC48,FSM1IS-BW-500LF-40K-1C-UNV-xC48,Batwing Optic,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-40K-1C-UNV-xC96,FSM1IS-BW-500LF-40K-1C-UNV-xC96,Batwing Optic,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-40K-1C-347-xC24,FSM1IS-BW-500LF-40K-1C-347-xC24,Batwing Optic,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-40K-1C-347-xC48,FSM1IS-BW-500LF-40K-1C-347-xC48,Batwing Optic,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-40K-1C-347-xC96,FSM1IS-BW-500LF-40K-1C-347-xC96,Batwing Optic,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-940K-1C-UNV-xC24,FSM1IS-BW-500LF-940K-1C-UNV-xC24,Batwing Optic,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-940K-1C-UNV-xC48,FSM1IS-BW-500LF-940K-1C-UNV-xC48,Batwing Optic,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-940K-1C-UNV-xC96,FSM1IS-BW-500LF-940K-1C-UNV-xC96,Batwing Optic,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-500LF-940K-1C-347-xC24,FSM1IS-BW-500LF-940K-1C-347-xC24,Batwing Optic,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-500LF-940K-1C-347-xC48,FSM1IS-BW-500LF-940K-1C-347-xC48,Batwing Optic,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-500LF-940K-1C-347-xC96,FSM1IS-BW-500LF-940K-1C-347-xC96,Batwing Optic,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,132,500 Lumens per foot.,FSM1IS-BW-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-27K-1C-UNV-xC24,FSM1IS-BW-625LF-27K-1C-UNV-xC24,Batwing Optic,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-27K-1C-UNV-xC48,FSM1IS-BW-625LF-27K-1C-UNV-xC48,Batwing Optic,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-27K-1C-UNV-xC96,FSM1IS-BW-625LF-27K-1C-UNV-xC96,Batwing Optic,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-27K-1C-347-xC24,FSM1IS-BW-625LF-27K-1C-347-xC24,Batwing Optic,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-27K-1C-347-xC48,FSM1IS-BW-625LF-27K-1C-347-xC48,Batwing Optic,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-27K-1C-347-xC96,FSM1IS-BW-625LF-27K-1C-347-xC96,Batwing Optic,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-927K-1C-UNV-xC24,FSM1IS-BW-625LF-927K-1C-UNV-xC24,Batwing Optic,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-927K-1C-UNV-xC48,FSM1IS-BW-625LF-927K-1C-UNV-xC48,Batwing Optic,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-927K-1C-UNV-xC96,FSM1IS-BW-625LF-927K-1C-UNV-xC96,Batwing Optic,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-927K-1C-347-xC24,FSM1IS-BW-625LF-927K-1C-347-xC24,Batwing Optic,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-927K-1C-347-xC48,FSM1IS-BW-625LF-927K-1C-347-xC48,Batwing Optic,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-927K-1C-347-xC96,FSM1IS-BW-625LF-927K-1C-347-xC96,Batwing Optic,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-30K-1C-UNV-xC24,FSM1IS-BW-625LF-30K-1C-UNV-xC24,Batwing Optic,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-30K-1C-UNV-xC48,FSM1IS-BW-625LF-30K-1C-UNV-xC48,Batwing Optic,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-30K-1C-UNV-xC96,FSM1IS-BW-625LF-30K-1C-UNV-xC96,Batwing Optic,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-30K-1C-347-xC24,FSM1IS-BW-625LF-30K-1C-347-xC24,Batwing Optic,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-30K-1C-347-xC48,FSM1IS-BW-625LF-30K-1C-347-xC48,Batwing Optic,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-30K-1C-347-xC96,FSM1IS-BW-625LF-30K-1C-347-xC96,Batwing Optic,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-930K-1C-UNV-xC24,FSM1IS-BW-625LF-930K-1C-UNV-xC24,Batwing Optic,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-930K-1C-UNV-xC48,FSM1IS-BW-625LF-930K-1C-UNV-xC48,Batwing Optic,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-930K-1C-UNV-xC96,FSM1IS-BW-625LF-930K-1C-UNV-xC96,Batwing Optic,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-930K-1C-347-xC24,FSM1IS-BW-625LF-930K-1C-347-xC24,Batwing Optic,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-930K-1C-347-xC48,FSM1IS-BW-625LF-930K-1C-347-xC48,Batwing Optic,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-930K-1C-347-xC96,FSM1IS-BW-625LF-930K-1C-347-xC96,Batwing Optic,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-35K-1C-UNV-xC24,FSM1IS-BW-625LF-35K-1C-UNV-xC24,Batwing Optic,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-35K-1C-UNV-xC48,FSM1IS-BW-625LF-35K-1C-UNV-xC48,Batwing Optic,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-35K-1C-UNV-xC96,FSM1IS-BW-625LF-35K-1C-UNV-xC96,Batwing Optic,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-35K-1C-347-xC24,FSM1IS-BW-625LF-35K-1C-347-xC24,Batwing Optic,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-35K-1C-347-xC48,FSM1IS-BW-625LF-35K-1C-347-xC48,Batwing Optic,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-35K-1C-347-xC96,FSM1IS-BW-625LF-35K-1C-347-xC96,Batwing Optic,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-935K-1C-UNV-xC24,FSM1IS-BW-625LF-935K-1C-UNV-xC24,Batwing Optic,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-935K-1C-UNV-xC48,FSM1IS-BW-625LF-935K-1C-UNV-xC48,Batwing Optic,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-935K-1C-UNV-xC96,FSM1IS-BW-625LF-935K-1C-UNV-xC96,Batwing Optic,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-935K-1C-347-xC24,FSM1IS-BW-625LF-935K-1C-347-xC24,Batwing Optic,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-935K-1C-347-xC48,FSM1IS-BW-625LF-935K-1C-347-xC48,Batwing Optic,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-935K-1C-347-xC96,FSM1IS-BW-625LF-935K-1C-347-xC96,Batwing Optic,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-40K-1C-UNV-xC24,FSM1IS-BW-625LF-40K-1C-UNV-xC24,Batwing Optic,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-40K-1C-UNV-xC48,FSM1IS-BW-625LF-40K-1C-UNV-xC48,Batwing Optic,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-40K-1C-UNV-xC96,FSM1IS-BW-625LF-40K-1C-UNV-xC96,Batwing Optic,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-40K-1C-347-xC24,FSM1IS-BW-625LF-40K-1C-347-xC24,Batwing Optic,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-40K-1C-347-xC48,FSM1IS-BW-625LF-40K-1C-347-xC48,Batwing Optic,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-40K-1C-347-xC96,FSM1IS-BW-625LF-40K-1C-347-xC96,Batwing Optic,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-940K-1C-UNV-xC24,FSM1IS-BW-625LF-940K-1C-UNV-xC24,Batwing Optic,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-940K-1C-UNV-xC48,FSM1IS-BW-625LF-940K-1C-UNV-xC48,Batwing Optic,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-940K-1C-UNV-xC96,FSM1IS-BW-625LF-940K-1C-UNV-xC96,Batwing Optic,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-625LF-940K-1C-347-xC24,FSM1IS-BW-625LF-940K-1C-347-xC24,Batwing Optic,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-625LF-940K-1C-347-xC48,FSM1IS-BW-625LF-940K-1C-347-xC48,Batwing Optic,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-625LF-940K-1C-347-xC96,FSM1IS-BW-625LF-940K-1C-347-xC96,Batwing Optic,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-BW-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-27K-1C-UNV-xC24,FSM1IS-BW-800LF-27K-1C-UNV-xC24,Batwing Optic,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-27K-1C-UNV-xC48,FSM1IS-BW-800LF-27K-1C-UNV-xC48,Batwing Optic,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-27K-1C-UNV-xC96,FSM1IS-BW-800LF-27K-1C-UNV-xC96,Batwing Optic,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-27K-1C-347-xC24,FSM1IS-BW-800LF-27K-1C-347-xC24,Batwing Optic,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-27K-1C-347-xC48,FSM1IS-BW-800LF-27K-1C-347-xC48,Batwing Optic,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-27K-1C-347-xC96,FSM1IS-BW-800LF-27K-1C-347-xC96,Batwing Optic,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-927K-1C-UNV-xC24,FSM1IS-BW-800LF-927K-1C-UNV-xC24,Batwing Optic,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-927K-1C-UNV-xC48,FSM1IS-BW-800LF-927K-1C-UNV-xC48,Batwing Optic,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-927K-1C-UNV-xC96,FSM1IS-BW-800LF-927K-1C-UNV-xC96,Batwing Optic,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-927K-1C-347-xC24,FSM1IS-BW-800LF-927K-1C-347-xC24,Batwing Optic,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-927K-1C-347-xC48,FSM1IS-BW-800LF-927K-1C-347-xC48,Batwing Optic,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-927K-1C-347-xC96,FSM1IS-BW-800LF-927K-1C-347-xC96,Batwing Optic,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-30K-1C-UNV-xC24,FSM1IS-BW-800LF-30K-1C-UNV-xC24,Batwing Optic,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-30K-1C-UNV-xC48,FSM1IS-BW-800LF-30K-1C-UNV-xC48,Batwing Optic,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-30K-1C-UNV-xC96,FSM1IS-BW-800LF-30K-1C-UNV-xC96,Batwing Optic,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-30K-1C-347-xC24,FSM1IS-BW-800LF-30K-1C-347-xC24,Batwing Optic,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-30K-1C-347-xC48,FSM1IS-BW-800LF-30K-1C-347-xC48,Batwing Optic,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-30K-1C-347-xC96,FSM1IS-BW-800LF-30K-1C-347-xC96,Batwing Optic,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-930K-1C-UNV-xC24,FSM1IS-BW-800LF-930K-1C-UNV-xC24,Batwing Optic,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-930K-1C-UNV-xC48,FSM1IS-BW-800LF-930K-1C-UNV-xC48,Batwing Optic,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-930K-1C-UNV-xC96,FSM1IS-BW-800LF-930K-1C-UNV-xC96,Batwing Optic,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-930K-1C-347-xC24,FSM1IS-BW-800LF-930K-1C-347-xC24,Batwing Optic,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-930K-1C-347-xC48,FSM1IS-BW-800LF-930K-1C-347-xC48,Batwing Optic,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-930K-1C-347-xC96,FSM1IS-BW-800LF-930K-1C-347-xC96,Batwing Optic,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-35K-1C-UNV-xC24,FSM1IS-BW-800LF-35K-1C-UNV-xC24,Batwing Optic,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-35K-1C-UNV-xC48,FSM1IS-BW-800LF-35K-1C-UNV-xC48,Batwing Optic,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-35K-1C-UNV-xC96,FSM1IS-BW-800LF-35K-1C-UNV-xC96,Batwing Optic,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-35K-1C-347-xC24,FSM1IS-BW-800LF-35K-1C-347-xC24,Batwing Optic,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-35K-1C-347-xC48,FSM1IS-BW-800LF-35K-1C-347-xC48,Batwing Optic,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-35K-1C-347-xC96,FSM1IS-BW-800LF-35K-1C-347-xC96,Batwing Optic,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-935K-1C-UNV-xC24,FSM1IS-BW-800LF-935K-1C-UNV-xC24,Batwing Optic,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-935K-1C-UNV-xC48,FSM1IS-BW-800LF-935K-1C-UNV-xC48,Batwing Optic,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-935K-1C-UNV-xC96,FSM1IS-BW-800LF-935K-1C-UNV-xC96,Batwing Optic,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-935K-1C-347-xC24,FSM1IS-BW-800LF-935K-1C-347-xC24,Batwing Optic,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-935K-1C-347-xC48,FSM1IS-BW-800LF-935K-1C-347-xC48,Batwing Optic,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-935K-1C-347-xC96,FSM1IS-BW-800LF-935K-1C-347-xC96,Batwing Optic,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-40K-1C-UNV-xC24,FSM1IS-BW-800LF-40K-1C-UNV-xC24,Batwing Optic,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-40K-1C-UNV-xC48,FSM1IS-BW-800LF-40K-1C-UNV-xC48,Batwing Optic,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-40K-1C-UNV-xC96,FSM1IS-BW-800LF-40K-1C-UNV-xC96,Batwing Optic,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-40K-1C-347-xC24,FSM1IS-BW-800LF-40K-1C-347-xC24,Batwing Optic,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-40K-1C-347-xC48,FSM1IS-BW-800LF-40K-1C-347-xC48,Batwing Optic,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-40K-1C-347-xC96,FSM1IS-BW-800LF-40K-1C-347-xC96,Batwing Optic,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-940K-1C-UNV-xC24,FSM1IS-BW-800LF-940K-1C-UNV-xC24,Batwing Optic,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-940K-1C-UNV-xC48,FSM1IS-BW-800LF-940K-1C-UNV-xC48,Batwing Optic,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-940K-1C-UNV-xC96,FSM1IS-BW-800LF-940K-1C-UNV-xC96,Batwing Optic,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-800LF-940K-1C-347-xC24,FSM1IS-BW-800LF-940K-1C-347-xC24,Batwing Optic,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-800LF-940K-1C-347-xC48,FSM1IS-BW-800LF-940K-1C-347-xC48,Batwing Optic,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-800LF-940K-1C-347-xC96,FSM1IS-BW-800LF-940K-1C-347-xC96,Batwing Optic,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,130,800 Lumens per foot,FSM1IS-BW-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-27K-1C-UNV-xC24,FSM1IS-BW-1000LF-27K-1C-UNV-xC24,Batwing Optic,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-27K-1C-UNV-xC48,FSM1IS-BW-1000LF-27K-1C-UNV-xC48,Batwing Optic,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-27K-1C-UNV-xC96,FSM1IS-BW-1000LF-27K-1C-UNV-xC96,Batwing Optic,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-27K-1C-347-xC24,FSM1IS-BW-1000LF-27K-1C-347-xC24,Batwing Optic,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-27K-1C-347-xC48,FSM1IS-BW-1000LF-27K-1C-347-xC48,Batwing Optic,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-27K-1C-347-xC96,FSM1IS-BW-1000LF-27K-1C-347-xC96,Batwing Optic,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-927K-1C-UNV-xC24,FSM1IS-BW-1000LF-927K-1C-UNV-xC24,Batwing Optic,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-927K-1C-UNV-xC48,FSM1IS-BW-1000LF-927K-1C-UNV-xC48,Batwing Optic,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-927K-1C-UNV-xC96,FSM1IS-BW-1000LF-927K-1C-UNV-xC96,Batwing Optic,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-927K-1C-347-xC24,FSM1IS-BW-1000LF-927K-1C-347-xC24,Batwing Optic,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-927K-1C-347-xC48,FSM1IS-BW-1000LF-927K-1C-347-xC48,Batwing Optic,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-927K-1C-347-xC96,FSM1IS-BW-1000LF-927K-1C-347-xC96,Batwing Optic,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-30K-1C-UNV-xC24,FSM1IS-BW-1000LF-30K-1C-UNV-xC24,Batwing Optic,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-30K-1C-UNV-xC48,FSM1IS-BW-1000LF-30K-1C-UNV-xC48,Batwing Optic,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-30K-1C-UNV-xC96,FSM1IS-BW-1000LF-30K-1C-UNV-xC96,Batwing Optic,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-30K-1C-347-xC24,FSM1IS-BW-1000LF-30K-1C-347-xC24,Batwing Optic,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-30K-1C-347-xC48,FSM1IS-BW-1000LF-30K-1C-347-xC48,Batwing Optic,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-30K-1C-347-xC96,FSM1IS-BW-1000LF-30K-1C-347-xC96,Batwing Optic,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-930K-1C-UNV-xC24,FSM1IS-BW-1000LF-930K-1C-UNV-xC24,Batwing Optic,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-930K-1C-UNV-xC48,FSM1IS-BW-1000LF-930K-1C-UNV-xC48,Batwing Optic,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-930K-1C-UNV-xC96,FSM1IS-BW-1000LF-930K-1C-UNV-xC96,Batwing Optic,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-930K-1C-347-xC24,FSM1IS-BW-1000LF-930K-1C-347-xC24,Batwing Optic,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-930K-1C-347-xC48,FSM1IS-BW-1000LF-930K-1C-347-xC48,Batwing Optic,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-930K-1C-347-xC96,FSM1IS-BW-1000LF-930K-1C-347-xC96,Batwing Optic,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-35K-1C-UNV-xC24,FSM1IS-BW-1000LF-35K-1C-UNV-xC24,Batwing Optic,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-35K-1C-UNV-xC48,FSM1IS-BW-1000LF-35K-1C-UNV-xC48,Batwing Optic,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-35K-1C-UNV-xC96,FSM1IS-BW-1000LF-35K-1C-UNV-xC96,Batwing Optic,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-35K-1C-347-xC24,FSM1IS-BW-1000LF-35K-1C-347-xC24,Batwing Optic,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-35K-1C-347-xC48,FSM1IS-BW-1000LF-35K-1C-347-xC48,Batwing Optic,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-35K-1C-347-xC96,FSM1IS-BW-1000LF-35K-1C-347-xC96,Batwing Optic,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-935K-1C-UNV-xC24,FSM1IS-BW-1000LF-935K-1C-UNV-xC24,Batwing Optic,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-935K-1C-UNV-xC48,FSM1IS-BW-1000LF-935K-1C-UNV-xC48,Batwing Optic,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-935K-1C-UNV-xC96,FSM1IS-BW-1000LF-935K-1C-UNV-xC96,Batwing Optic,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-935K-1C-347-xC24,FSM1IS-BW-1000LF-935K-1C-347-xC24,Batwing Optic,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-935K-1C-347-xC48,FSM1IS-BW-1000LF-935K-1C-347-xC48,Batwing Optic,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-935K-1C-347-xC96,FSM1IS-BW-1000LF-935K-1C-347-xC96,Batwing Optic,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-40K-1C-UNV-xC24,FSM1IS-BW-1000LF-40K-1C-UNV-xC24,Batwing Optic,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-40K-1C-UNV-xC48,FSM1IS-BW-1000LF-40K-1C-UNV-xC48,Batwing Optic,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-40K-1C-UNV-xC96,FSM1IS-BW-1000LF-40K-1C-UNV-xC96,Batwing Optic,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-40K-1C-347-xC24,FSM1IS-BW-1000LF-40K-1C-347-xC24,Batwing Optic,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-40K-1C-347-xC48,FSM1IS-BW-1000LF-40K-1C-347-xC48,Batwing Optic,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-40K-1C-347-xC96,FSM1IS-BW-1000LF-40K-1C-347-xC96,Batwing Optic,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-940K-1C-UNV-xC24,FSM1IS-BW-1000LF-940K-1C-UNV-xC24,Batwing Optic,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-940K-1C-UNV-xC48,FSM1IS-BW-1000LF-940K-1C-UNV-xC48,Batwing Optic,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-940K-1C-UNV-xC96,FSM1IS-BW-1000LF-940K-1C-UNV-xC96,Batwing Optic,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1000LF-940K-1C-347-xC24,FSM1IS-BW-1000LF-940K-1C-347-xC24,Batwing Optic,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1000LF-940K-1C-347-xC48,FSM1IS-BW-1000LF-940K-1C-347-xC48,Batwing Optic,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1000LF-940K-1C-347-xC96,FSM1IS-BW-1000LF-940K-1C-347-xC96,Batwing Optic,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,129,1000 Lumens per foot. Not available with DALI.,FSM1IS-BW-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-27K-1C-UNV-xC24,FSM1IS-BW-1250LF-27K-1C-UNV-xC24,Batwing Optic,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-27K-1C-UNV-xC48,FSM1IS-BW-1250LF-27K-1C-UNV-xC48,Batwing Optic,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-27K-1C-UNV-xC96,FSM1IS-BW-1250LF-27K-1C-UNV-xC96,Batwing Optic,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-27K-1C-347-xC24,FSM1IS-BW-1250LF-27K-1C-347-xC24,Batwing Optic,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-27K-1C-347-xC48,FSM1IS-BW-1250LF-27K-1C-347-xC48,Batwing Optic,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-27K-1C-347-xC96,FSM1IS-BW-1250LF-27K-1C-347-xC96,Batwing Optic,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-927K-1C-UNV-xC24,FSM1IS-BW-1250LF-927K-1C-UNV-xC24,Batwing Optic,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-927K-1C-UNV-xC48,FSM1IS-BW-1250LF-927K-1C-UNV-xC48,Batwing Optic,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-927K-1C-UNV-xC96,FSM1IS-BW-1250LF-927K-1C-UNV-xC96,Batwing Optic,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-927K-1C-347-xC24,FSM1IS-BW-1250LF-927K-1C-347-xC24,Batwing Optic,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-927K-1C-347-xC48,FSM1IS-BW-1250LF-927K-1C-347-xC48,Batwing Optic,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-927K-1C-347-xC96,FSM1IS-BW-1250LF-927K-1C-347-xC96,Batwing Optic,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-30K-1C-UNV-xC24,FSM1IS-BW-1250LF-30K-1C-UNV-xC24,Batwing Optic,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-30K-1C-UNV-xC48,FSM1IS-BW-1250LF-30K-1C-UNV-xC48,Batwing Optic,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-30K-1C-UNV-xC96,FSM1IS-BW-1250LF-30K-1C-UNV-xC96,Batwing Optic,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-30K-1C-347-xC24,FSM1IS-BW-1250LF-30K-1C-347-xC24,Batwing Optic,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-30K-1C-347-xC48,FSM1IS-BW-1250LF-30K-1C-347-xC48,Batwing Optic,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-30K-1C-347-xC96,FSM1IS-BW-1250LF-30K-1C-347-xC96,Batwing Optic,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-930K-1C-UNV-xC24,FSM1IS-BW-1250LF-930K-1C-UNV-xC24,Batwing Optic,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-930K-1C-UNV-xC48,FSM1IS-BW-1250LF-930K-1C-UNV-xC48,Batwing Optic,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-930K-1C-UNV-xC96,FSM1IS-BW-1250LF-930K-1C-UNV-xC96,Batwing Optic,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-930K-1C-347-xC24,FSM1IS-BW-1250LF-930K-1C-347-xC24,Batwing Optic,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-930K-1C-347-xC48,FSM1IS-BW-1250LF-930K-1C-347-xC48,Batwing Optic,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-930K-1C-347-xC96,FSM1IS-BW-1250LF-930K-1C-347-xC96,Batwing Optic,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-35K-1C-UNV-xC24,FSM1IS-BW-1250LF-35K-1C-UNV-xC24,Batwing Optic,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-35K-1C-UNV-xC48,FSM1IS-BW-1250LF-35K-1C-UNV-xC48,Batwing Optic,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-35K-1C-UNV-xC96,FSM1IS-BW-1250LF-35K-1C-UNV-xC96,Batwing Optic,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-35K-1C-347-xC24,FSM1IS-BW-1250LF-35K-1C-347-xC24,Batwing Optic,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-35K-1C-347-xC48,FSM1IS-BW-1250LF-35K-1C-347-xC48,Batwing Optic,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-35K-1C-347-xC96,FSM1IS-BW-1250LF-35K-1C-347-xC96,Batwing Optic,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-935K-1C-UNV-xC24,FSM1IS-BW-1250LF-935K-1C-UNV-xC24,Batwing Optic,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-935K-1C-UNV-xC48,FSM1IS-BW-1250LF-935K-1C-UNV-xC48,Batwing Optic,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-935K-1C-UNV-xC96,FSM1IS-BW-1250LF-935K-1C-UNV-xC96,Batwing Optic,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-935K-1C-347-xC24,FSM1IS-BW-1250LF-935K-1C-347-xC24,Batwing Optic,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-935K-1C-347-xC48,FSM1IS-BW-1250LF-935K-1C-347-xC48,Batwing Optic,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-935K-1C-347-xC96,FSM1IS-BW-1250LF-935K-1C-347-xC96,Batwing Optic,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-40K-1C-UNV-xC24,FSM1IS-BW-1250LF-40K-1C-UNV-xC24,Batwing Optic,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-40K-1C-UNV-xC48,FSM1IS-BW-1250LF-40K-1C-UNV-xC48,Batwing Optic,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-40K-1C-UNV-xC96,FSM1IS-BW-1250LF-40K-1C-UNV-xC96,Batwing Optic,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-40K-1C-347-xC24,FSM1IS-BW-1250LF-40K-1C-347-xC24,Batwing Optic,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-40K-1C-347-xC48,FSM1IS-BW-1250LF-40K-1C-347-xC48,Batwing Optic,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-40K-1C-347-xC96,FSM1IS-BW-1250LF-40K-1C-347-xC96,Batwing Optic,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-940K-1C-UNV-xC24,FSM1IS-BW-1250LF-940K-1C-UNV-xC24,Batwing Optic,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-940K-1C-UNV-xC48,FSM1IS-BW-1250LF-940K-1C-UNV-xC48,Batwing Optic,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-940K-1C-UNV-xC96,FSM1IS-BW-1250LF-940K-1C-UNV-xC96,Batwing Optic,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-BW-1250LF-940K-1C-347-xC24,FSM1IS-BW-1250LF-940K-1C-347-xC24,Batwing Optic,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-BW-1250LF-940K-1C-347-xC48,FSM1IS-BW-1250LF-940K-1C-347-xC48,Batwing Optic,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-BW-1250LF-940K-1C-347-xC96,FSM1IS-BW-1250LF-940K-1C-347-xC96,Batwing Optic,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,126,1250 Lumens per foot. Not available with DALI.,FSM1IS-BW-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-27K-1C-UNV-xC24,FSM1IS-AS-250LF-27K-1C-UNV-xC24,Asymmetric Optic,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-27K-1C-UNV-xC48,FSM1IS-AS-250LF-27K-1C-UNV-xC48,Asymmetric Optic,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-27K-1C-UNV-xC96,FSM1IS-AS-250LF-27K-1C-UNV-xC96,Asymmetric Optic,250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-27K-1C-347-xC24,FSM1IS-AS-250LF-27K-1C-347-xC24,Asymmetric Optic,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-27K-1C-347-xC48,FSM1IS-AS-250LF-27K-1C-347-xC48,Asymmetric Optic,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-27K-1C-347-xC96,FSM1IS-AS-250LF-27K-1C-347-xC96,Asymmetric Optic,250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-927K-1C-UNV-xC24,FSM1IS-AS-250LF-927K-1C-UNV-xC24,Asymmetric Optic,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-927K-1C-UNV-xC48,FSM1IS-AS-250LF-927K-1C-UNV-xC48,Asymmetric Optic,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-927K-1C-UNV-xC96,FSM1IS-AS-250LF-927K-1C-UNV-xC96,Asymmetric Optic,250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-927K-1C-347-xC24,FSM1IS-AS-250LF-927K-1C-347-xC24,Asymmetric Optic,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-927K-1C-347-xC48,FSM1IS-AS-250LF-927K-1C-347-xC48,Asymmetric Optic,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-927K-1C-347-xC96,FSM1IS-AS-250LF-927K-1C-347-xC96,Asymmetric Optic,250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-30K-1C-UNV-xC24,FSM1IS-AS-250LF-30K-1C-UNV-xC24,Asymmetric Optic,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-30K-1C-UNV-xC48,FSM1IS-AS-250LF-30K-1C-UNV-xC48,Asymmetric Optic,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-30K-1C-UNV-xC96,FSM1IS-AS-250LF-30K-1C-UNV-xC96,Asymmetric Optic,250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-30K-1C-347-xC24,FSM1IS-AS-250LF-30K-1C-347-xC24,Asymmetric Optic,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-30K-1C-347-xC48,FSM1IS-AS-250LF-30K-1C-347-xC48,Asymmetric Optic,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-30K-1C-347-xC96,FSM1IS-AS-250LF-30K-1C-347-xC96,Asymmetric Optic,250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-930K-1C-UNV-xC24,FSM1IS-AS-250LF-930K-1C-UNV-xC24,Asymmetric Optic,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-930K-1C-UNV-xC48,FSM1IS-AS-250LF-930K-1C-UNV-xC48,Asymmetric Optic,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-930K-1C-UNV-xC96,FSM1IS-AS-250LF-930K-1C-UNV-xC96,Asymmetric Optic,250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-930K-1C-347-xC24,FSM1IS-AS-250LF-930K-1C-347-xC24,Asymmetric Optic,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-930K-1C-347-xC48,FSM1IS-AS-250LF-930K-1C-347-xC48,Asymmetric Optic,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-930K-1C-347-xC96,FSM1IS-AS-250LF-930K-1C-347-xC96,Asymmetric Optic,250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-35K-1C-UNV-xC24,FSM1IS-AS-250LF-35K-1C-UNV-xC24,Asymmetric Optic,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-35K-1C-UNV-xC48,FSM1IS-AS-250LF-35K-1C-UNV-xC48,Asymmetric Optic,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-35K-1C-UNV-xC96,FSM1IS-AS-250LF-35K-1C-UNV-xC96,Asymmetric Optic,250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-35K-1C-347-xC24,FSM1IS-AS-250LF-35K-1C-347-xC24,Asymmetric Optic,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-35K-1C-347-xC48,FSM1IS-AS-250LF-35K-1C-347-xC48,Asymmetric Optic,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-35K-1C-347-xC96,FSM1IS-AS-250LF-35K-1C-347-xC96,Asymmetric Optic,250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-935K-1C-UNV-xC24,FSM1IS-AS-250LF-935K-1C-UNV-xC24,Asymmetric Optic,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-935K-1C-UNV-xC48,FSM1IS-AS-250LF-935K-1C-UNV-xC48,Asymmetric Optic,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-935K-1C-UNV-xC96,FSM1IS-AS-250LF-935K-1C-UNV-xC96,Asymmetric Optic,250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-935K-1C-347-xC24,FSM1IS-AS-250LF-935K-1C-347-xC24,Asymmetric Optic,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-935K-1C-347-xC48,FSM1IS-AS-250LF-935K-1C-347-xC48,Asymmetric Optic,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-935K-1C-347-xC96,FSM1IS-AS-250LF-935K-1C-347-xC96,Asymmetric Optic,250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-40K-1C-UNV-xC24,FSM1IS-AS-250LF-40K-1C-UNV-xC24,Asymmetric Optic,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-40K-1C-UNV-xC48,FSM1IS-AS-250LF-40K-1C-UNV-xC48,Asymmetric Optic,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-40K-1C-UNV-xC96,FSM1IS-AS-250LF-40K-1C-UNV-xC96,Asymmetric Optic,250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-40K-1C-347-xC24,FSM1IS-AS-250LF-40K-1C-347-xC24,Asymmetric Optic,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-40K-1C-347-xC48,FSM1IS-AS-250LF-40K-1C-347-xC48,Asymmetric Optic,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-40K-1C-347-xC96,FSM1IS-AS-250LF-40K-1C-347-xC96,Asymmetric Optic,250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-940K-1C-UNV-xC24,FSM1IS-AS-250LF-940K-1C-UNV-xC24,Asymmetric Optic,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-940K-1C-UNV-xC48,FSM1IS-AS-250LF-940K-1C-UNV-xC48,Asymmetric Optic,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-940K-1C-UNV-xC96,FSM1IS-AS-250LF-940K-1C-UNV-xC96,Asymmetric Optic,250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-250LF-940K-1C-347-xC24,FSM1IS-AS-250LF-940K-1C-347-xC24,Asymmetric Optic,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-250LF-940K-1C-347-xC48,FSM1IS-AS-250LF-940K-1C-347-xC48,Asymmetric Optic,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-250LF-940K-1C-347-xC96,FSM1IS-AS-250LF-940K-1C-347-xC96,Asymmetric Optic,250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,9,9W,118,250 Lumens per foot.,FSM1IS-AS-250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-27K-1C-UNV-xC24,FSM1IS-AS-375LF-27K-1C-UNV-xC24,Asymmetric Optic,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-27K-1C-UNV-xC48,FSM1IS-AS-375LF-27K-1C-UNV-xC48,Asymmetric Optic,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-27K-1C-UNV-xC96,FSM1IS-AS-375LF-27K-1C-UNV-xC96,Asymmetric Optic,375,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-27K-1C-347-xC24,FSM1IS-AS-375LF-27K-1C-347-xC24,Asymmetric Optic,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-27K-1C-347-xC48,FSM1IS-AS-375LF-27K-1C-347-xC48,Asymmetric Optic,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-27K-1C-347-xC96,FSM1IS-AS-375LF-27K-1C-347-xC96,Asymmetric Optic,375,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-927K-1C-UNV-xC24,FSM1IS-AS-375LF-927K-1C-UNV-xC24,Asymmetric Optic,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-927K-1C-UNV-xC48,FSM1IS-AS-375LF-927K-1C-UNV-xC48,Asymmetric Optic,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-927K-1C-UNV-xC96,FSM1IS-AS-375LF-927K-1C-UNV-xC96,Asymmetric Optic,375,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-927K-1C-347-xC24,FSM1IS-AS-375LF-927K-1C-347-xC24,Asymmetric Optic,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-927K-1C-347-xC48,FSM1IS-AS-375LF-927K-1C-347-xC48,Asymmetric Optic,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-927K-1C-347-xC96,FSM1IS-AS-375LF-927K-1C-347-xC96,Asymmetric Optic,375,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-30K-1C-UNV-xC24,FSM1IS-AS-375LF-30K-1C-UNV-xC24,Asymmetric Optic,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-30K-1C-UNV-xC48,FSM1IS-AS-375LF-30K-1C-UNV-xC48,Asymmetric Optic,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-30K-1C-UNV-xC96,FSM1IS-AS-375LF-30K-1C-UNV-xC96,Asymmetric Optic,375,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-30K-1C-347-xC24,FSM1IS-AS-375LF-30K-1C-347-xC24,Asymmetric Optic,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-30K-1C-347-xC48,FSM1IS-AS-375LF-30K-1C-347-xC48,Asymmetric Optic,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-30K-1C-347-xC96,FSM1IS-AS-375LF-30K-1C-347-xC96,Asymmetric Optic,375,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-930K-1C-UNV-xC24,FSM1IS-AS-375LF-930K-1C-UNV-xC24,Asymmetric Optic,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-930K-1C-UNV-xC48,FSM1IS-AS-375LF-930K-1C-UNV-xC48,Asymmetric Optic,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-930K-1C-UNV-xC96,FSM1IS-AS-375LF-930K-1C-UNV-xC96,Asymmetric Optic,375,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-930K-1C-347-xC24,FSM1IS-AS-375LF-930K-1C-347-xC24,Asymmetric Optic,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-930K-1C-347-xC48,FSM1IS-AS-375LF-930K-1C-347-xC48,Asymmetric Optic,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-930K-1C-347-xC96,FSM1IS-AS-375LF-930K-1C-347-xC96,Asymmetric Optic,375,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-35K-1C-UNV-xC24,FSM1IS-AS-375LF-35K-1C-UNV-xC24,Asymmetric Optic,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-35K-1C-UNV-xC48,FSM1IS-AS-375LF-35K-1C-UNV-xC48,Asymmetric Optic,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-35K-1C-UNV-xC96,FSM1IS-AS-375LF-35K-1C-UNV-xC96,Asymmetric Optic,375,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-35K-1C-347-xC24,FSM1IS-AS-375LF-35K-1C-347-xC24,Asymmetric Optic,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-35K-1C-347-xC48,FSM1IS-AS-375LF-35K-1C-347-xC48,Asymmetric Optic,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-35K-1C-347-xC96,FSM1IS-AS-375LF-35K-1C-347-xC96,Asymmetric Optic,375,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-935K-1C-UNV-xC24,FSM1IS-AS-375LF-935K-1C-UNV-xC24,Asymmetric Optic,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-935K-1C-UNV-xC48,FSM1IS-AS-375LF-935K-1C-UNV-xC48,Asymmetric Optic,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-935K-1C-UNV-xC96,FSM1IS-AS-375LF-935K-1C-UNV-xC96,Asymmetric Optic,375,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-935K-1C-347-xC24,FSM1IS-AS-375LF-935K-1C-347-xC24,Asymmetric Optic,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-935K-1C-347-xC48,FSM1IS-AS-375LF-935K-1C-347-xC48,Asymmetric Optic,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-935K-1C-347-xC96,FSM1IS-AS-375LF-935K-1C-347-xC96,Asymmetric Optic,375,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-40K-1C-UNV-xC24,FSM1IS-AS-375LF-40K-1C-UNV-xC24,Asymmetric Optic,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-40K-1C-UNV-xC48,FSM1IS-AS-375LF-40K-1C-UNV-xC48,Asymmetric Optic,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-40K-1C-UNV-xC96,FSM1IS-AS-375LF-40K-1C-UNV-xC96,Asymmetric Optic,375,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-40K-1C-347-xC24,FSM1IS-AS-375LF-40K-1C-347-xC24,Asymmetric Optic,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-40K-1C-347-xC48,FSM1IS-AS-375LF-40K-1C-347-xC48,Asymmetric Optic,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-40K-1C-347-xC96,FSM1IS-AS-375LF-40K-1C-347-xC96,Asymmetric Optic,375,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-940K-1C-UNV-xC24,FSM1IS-AS-375LF-940K-1C-UNV-xC24,Asymmetric Optic,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-940K-1C-UNV-xC48,FSM1IS-AS-375LF-940K-1C-UNV-xC48,Asymmetric Optic,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-940K-1C-UNV-xC96,FSM1IS-AS-375LF-940K-1C-UNV-xC96,Asymmetric Optic,375,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-375LF-940K-1C-347-xC24,FSM1IS-AS-375LF-940K-1C-347-xC24,Asymmetric Optic,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-375LF-940K-1C-347-xC48,FSM1IS-AS-375LF-940K-1C-347-xC48,Asymmetric Optic,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-375LF-940K-1C-347-xC96,FSM1IS-AS-375LF-940K-1C-347-xC96,Asymmetric Optic,375,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,12,12W,126,350 Lumens per foot.,FSM1IS-AS-375UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-27K-1C-UNV-xC24,FSM1IS-AS-500LF-27K-1C-UNV-xC24,Asymmetric Optic,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-27K-1C-UNV-xC48,FSM1IS-AS-500LF-27K-1C-UNV-xC48,Asymmetric Optic,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-27K-1C-UNV-xC96,FSM1IS-AS-500LF-27K-1C-UNV-xC96,Asymmetric Optic,500,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-27K-1C-347-xC24,FSM1IS-AS-500LF-27K-1C-347-xC24,Asymmetric Optic,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-27K-1C-347-xC48,FSM1IS-AS-500LF-27K-1C-347-xC48,Asymmetric Optic,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-27K-1C-347-xC96,FSM1IS-AS-500LF-27K-1C-347-xC96,Asymmetric Optic,500,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-927K-1C-UNV-xC24,FSM1IS-AS-500LF-927K-1C-UNV-xC24,Asymmetric Optic,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-927K-1C-UNV-xC48,FSM1IS-AS-500LF-927K-1C-UNV-xC48,Asymmetric Optic,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-927K-1C-UNV-xC96,FSM1IS-AS-500LF-927K-1C-UNV-xC96,Asymmetric Optic,500,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-927K-1C-347-xC24,FSM1IS-AS-500LF-927K-1C-347-xC24,Asymmetric Optic,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-927K-1C-347-xC48,FSM1IS-AS-500LF-927K-1C-347-xC48,Asymmetric Optic,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-927K-1C-347-xC96,FSM1IS-AS-500LF-927K-1C-347-xC96,Asymmetric Optic,500,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-30K-1C-UNV-xC24,FSM1IS-AS-500LF-30K-1C-UNV-xC24,Asymmetric Optic,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-30K-1C-UNV-xC48,FSM1IS-AS-500LF-30K-1C-UNV-xC48,Asymmetric Optic,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-30K-1C-UNV-xC96,FSM1IS-AS-500LF-30K-1C-UNV-xC96,Asymmetric Optic,500,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-30K-1C-347-xC24,FSM1IS-AS-500LF-30K-1C-347-xC24,Asymmetric Optic,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-30K-1C-347-xC48,FSM1IS-AS-500LF-30K-1C-347-xC48,Asymmetric Optic,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-30K-1C-347-xC96,FSM1IS-AS-500LF-30K-1C-347-xC96,Asymmetric Optic,500,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-930K-1C-UNV-xC24,FSM1IS-AS-500LF-930K-1C-UNV-xC24,Asymmetric Optic,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-930K-1C-UNV-xC48,FSM1IS-AS-500LF-930K-1C-UNV-xC48,Asymmetric Optic,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-930K-1C-UNV-xC96,FSM1IS-AS-500LF-930K-1C-UNV-xC96,Asymmetric Optic,500,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-930K-1C-347-xC24,FSM1IS-AS-500LF-930K-1C-347-xC24,Asymmetric Optic,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-930K-1C-347-xC48,FSM1IS-AS-500LF-930K-1C-347-xC48,Asymmetric Optic,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-930K-1C-347-xC96,FSM1IS-AS-500LF-930K-1C-347-xC96,Asymmetric Optic,500,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-35K-1C-UNV-xC24,FSM1IS-AS-500LF-35K-1C-UNV-xC24,Asymmetric Optic,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-35K-1C-UNV-xC48,FSM1IS-AS-500LF-35K-1C-UNV-xC48,Asymmetric Optic,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-35K-1C-UNV-xC96,FSM1IS-AS-500LF-35K-1C-UNV-xC96,Asymmetric Optic,500,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-35K-1C-347-xC24,FSM1IS-AS-500LF-35K-1C-347-xC24,Asymmetric Optic,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-35K-1C-347-xC48,FSM1IS-AS-500LF-35K-1C-347-xC48,Asymmetric Optic,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-35K-1C-347-xC96,FSM1IS-AS-500LF-35K-1C-347-xC96,Asymmetric Optic,500,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-935K-1C-UNV-xC24,FSM1IS-AS-500LF-935K-1C-UNV-xC24,Asymmetric Optic,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-935K-1C-UNV-xC48,FSM1IS-AS-500LF-935K-1C-UNV-xC48,Asymmetric Optic,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-935K-1C-UNV-xC96,FSM1IS-AS-500LF-935K-1C-UNV-xC96,Asymmetric Optic,500,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-935K-1C-347-xC24,FSM1IS-AS-500LF-935K-1C-347-xC24,Asymmetric Optic,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-935K-1C-347-xC48,FSM1IS-AS-500LF-935K-1C-347-xC48,Asymmetric Optic,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-935K-1C-347-xC96,FSM1IS-AS-500LF-935K-1C-347-xC96,Asymmetric Optic,500,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-40K-1C-UNV-xC24,FSM1IS-AS-500LF-40K-1C-UNV-xC24,Asymmetric Optic,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-40K-1C-UNV-xC48,FSM1IS-AS-500LF-40K-1C-UNV-xC48,Asymmetric Optic,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-40K-1C-UNV-xC96,FSM1IS-AS-500LF-40K-1C-UNV-xC96,Asymmetric Optic,500,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-40K-1C-347-xC24,FSM1IS-AS-500LF-40K-1C-347-xC24,Asymmetric Optic,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-40K-1C-347-xC48,FSM1IS-AS-500LF-40K-1C-347-xC48,Asymmetric Optic,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-40K-1C-347-xC96,FSM1IS-AS-500LF-40K-1C-347-xC96,Asymmetric Optic,500,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-940K-1C-UNV-xC24,FSM1IS-AS-500LF-940K-1C-UNV-xC24,Asymmetric Optic,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-940K-1C-UNV-xC48,FSM1IS-AS-500LF-940K-1C-UNV-xC48,Asymmetric Optic,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-940K-1C-UNV-xC96,FSM1IS-AS-500LF-940K-1C-UNV-xC96,Asymmetric Optic,500,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-500LF-940K-1C-347-xC24,FSM1IS-AS-500LF-940K-1C-347-xC24,Asymmetric Optic,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-500LF-940K-1C-347-xC48,FSM1IS-AS-500LF-940K-1C-347-xC48,Asymmetric Optic,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-500LF-940K-1C-347-xC96,FSM1IS-AS-500LF-940K-1C-347-xC96,Asymmetric Optic,500,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,15,15W,133,500 Lumens per foot.,FSM1IS-AS-500UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-27K-1C-UNV-xC24,FSM1IS-AS-625LF-27K-1C-UNV-xC24,Asymmetric Optic,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-27K-1C-UNV-xC48,FSM1IS-AS-625LF-27K-1C-UNV-xC48,Asymmetric Optic,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-27K-1C-UNV-xC96,FSM1IS-AS-625LF-27K-1C-UNV-xC96,Asymmetric Optic,625,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-27K-1C-347-xC24,FSM1IS-AS-625LF-27K-1C-347-xC24,Asymmetric Optic,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-27K-1C-347-xC48,FSM1IS-AS-625LF-27K-1C-347-xC48,Asymmetric Optic,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-27K-1C-347-xC96,FSM1IS-AS-625LF-27K-1C-347-xC96,Asymmetric Optic,625,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-927K-1C-UNV-xC24,FSM1IS-AS-625LF-927K-1C-UNV-xC24,Asymmetric Optic,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-927K-1C-UNV-xC48,FSM1IS-AS-625LF-927K-1C-UNV-xC48,Asymmetric Optic,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-927K-1C-UNV-xC96,FSM1IS-AS-625LF-927K-1C-UNV-xC96,Asymmetric Optic,625,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-927K-1C-347-xC24,FSM1IS-AS-625LF-927K-1C-347-xC24,Asymmetric Optic,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-927K-1C-347-xC48,FSM1IS-AS-625LF-927K-1C-347-xC48,Asymmetric Optic,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-927K-1C-347-xC96,FSM1IS-AS-625LF-927K-1C-347-xC96,Asymmetric Optic,625,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-30K-1C-UNV-xC24,FSM1IS-AS-625LF-30K-1C-UNV-xC24,Asymmetric Optic,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-30K-1C-UNV-xC48,FSM1IS-AS-625LF-30K-1C-UNV-xC48,Asymmetric Optic,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-30K-1C-UNV-xC96,FSM1IS-AS-625LF-30K-1C-UNV-xC96,Asymmetric Optic,625,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-30K-1C-347-xC24,FSM1IS-AS-625LF-30K-1C-347-xC24,Asymmetric Optic,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-30K-1C-347-xC48,FSM1IS-AS-625LF-30K-1C-347-xC48,Asymmetric Optic,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-30K-1C-347-xC96,FSM1IS-AS-625LF-30K-1C-347-xC96,Asymmetric Optic,625,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-930K-1C-UNV-xC24,FSM1IS-AS-625LF-930K-1C-UNV-xC24,Asymmetric Optic,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-930K-1C-UNV-xC48,FSM1IS-AS-625LF-930K-1C-UNV-xC48,Asymmetric Optic,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-930K-1C-UNV-xC96,FSM1IS-AS-625LF-930K-1C-UNV-xC96,Asymmetric Optic,625,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-930K-1C-347-xC24,FSM1IS-AS-625LF-930K-1C-347-xC24,Asymmetric Optic,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-930K-1C-347-xC48,FSM1IS-AS-625LF-930K-1C-347-xC48,Asymmetric Optic,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-930K-1C-347-xC96,FSM1IS-AS-625LF-930K-1C-347-xC96,Asymmetric Optic,625,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-35K-1C-UNV-xC24,FSM1IS-AS-625LF-35K-1C-UNV-xC24,Asymmetric Optic,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-35K-1C-UNV-xC48,FSM1IS-AS-625LF-35K-1C-UNV-xC48,Asymmetric Optic,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-35K-1C-UNV-xC96,FSM1IS-AS-625LF-35K-1C-UNV-xC96,Asymmetric Optic,625,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-35K-1C-347-xC24,FSM1IS-AS-625LF-35K-1C-347-xC24,Asymmetric Optic,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-35K-1C-347-xC48,FSM1IS-AS-625LF-35K-1C-347-xC48,Asymmetric Optic,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-35K-1C-347-xC96,FSM1IS-AS-625LF-35K-1C-347-xC96,Asymmetric Optic,625,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-935K-1C-UNV-xC24,FSM1IS-AS-625LF-935K-1C-UNV-xC24,Asymmetric Optic,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-935K-1C-UNV-xC48,FSM1IS-AS-625LF-935K-1C-UNV-xC48,Asymmetric Optic,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-935K-1C-UNV-xC96,FSM1IS-AS-625LF-935K-1C-UNV-xC96,Asymmetric Optic,625,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-935K-1C-347-xC24,FSM1IS-AS-625LF-935K-1C-347-xC24,Asymmetric Optic,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-935K-1C-347-xC48,FSM1IS-AS-625LF-935K-1C-347-xC48,Asymmetric Optic,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-935K-1C-347-xC96,FSM1IS-AS-625LF-935K-1C-347-xC96,Asymmetric Optic,625,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-40K-1C-UNV-xC24,FSM1IS-AS-625LF-40K-1C-UNV-xC24,Asymmetric Optic,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-40K-1C-UNV-xC48,FSM1IS-AS-625LF-40K-1C-UNV-xC48,Asymmetric Optic,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-40K-1C-UNV-xC96,FSM1IS-AS-625LF-40K-1C-UNV-xC96,Asymmetric Optic,625,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-40K-1C-347-xC24,FSM1IS-AS-625LF-40K-1C-347-xC24,Asymmetric Optic,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-40K-1C-347-xC48,FSM1IS-AS-625LF-40K-1C-347-xC48,Asymmetric Optic,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-40K-1C-347-xC96,FSM1IS-AS-625LF-40K-1C-347-xC96,Asymmetric Optic,625,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-940K-1C-UNV-xC24,FSM1IS-AS-625LF-940K-1C-UNV-xC24,Asymmetric Optic,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-940K-1C-UNV-xC48,FSM1IS-AS-625LF-940K-1C-UNV-xC48,Asymmetric Optic,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-940K-1C-UNV-xC96,FSM1IS-AS-625LF-940K-1C-UNV-xC96,Asymmetric Optic,625,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-625LF-940K-1C-347-xC24,FSM1IS-AS-625LF-940K-1C-347-xC24,Asymmetric Optic,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-625LF-940K-1C-347-xC48,FSM1IS-AS-625LF-940K-1C-347-xC48,Asymmetric Optic,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-625LF-940K-1C-347-xC96,FSM1IS-AS-625LF-940K-1C-347-xC96,Asymmetric Optic,625,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,19,19W,135,625 Lumens per foot.,FSM1IS-AS-625UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-27K-1C-UNV-xC24,FSM1IS-AS-800LF-27K-1C-UNV-xC24,Asymmetric Optic,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-27K-1C-UNV-xC48,FSM1IS-AS-800LF-27K-1C-UNV-xC48,Asymmetric Optic,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-27K-1C-UNV-xC96,FSM1IS-AS-800LF-27K-1C-UNV-xC96,Asymmetric Optic,800,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-27K-1C-347-xC24,FSM1IS-AS-800LF-27K-1C-347-xC24,Asymmetric Optic,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-27K-1C-347-xC48,FSM1IS-AS-800LF-27K-1C-347-xC48,Asymmetric Optic,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-27K-1C-347-xC96,FSM1IS-AS-800LF-27K-1C-347-xC96,Asymmetric Optic,800,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-927K-1C-UNV-xC24,FSM1IS-AS-800LF-927K-1C-UNV-xC24,Asymmetric Optic,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-927K-1C-UNV-xC48,FSM1IS-AS-800LF-927K-1C-UNV-xC48,Asymmetric Optic,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-927K-1C-UNV-xC96,FSM1IS-AS-800LF-927K-1C-UNV-xC96,Asymmetric Optic,800,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-927K-1C-347-xC24,FSM1IS-AS-800LF-927K-1C-347-xC24,Asymmetric Optic,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-927K-1C-347-xC48,FSM1IS-AS-800LF-927K-1C-347-xC48,Asymmetric Optic,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-927K-1C-347-xC96,FSM1IS-AS-800LF-927K-1C-347-xC96,Asymmetric Optic,800,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-30K-1C-UNV-xC24,FSM1IS-AS-800LF-30K-1C-UNV-xC24,Asymmetric Optic,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-30K-1C-UNV-xC48,FSM1IS-AS-800LF-30K-1C-UNV-xC48,Asymmetric Optic,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-30K-1C-UNV-xC96,FSM1IS-AS-800LF-30K-1C-UNV-xC96,Asymmetric Optic,800,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-30K-1C-347-xC24,FSM1IS-AS-800LF-30K-1C-347-xC24,Asymmetric Optic,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-30K-1C-347-xC48,FSM1IS-AS-800LF-30K-1C-347-xC48,Asymmetric Optic,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-30K-1C-347-xC96,FSM1IS-AS-800LF-30K-1C-347-xC96,Asymmetric Optic,800,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-930K-1C-UNV-xC24,FSM1IS-AS-800LF-930K-1C-UNV-xC24,Asymmetric Optic,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-930K-1C-UNV-xC48,FSM1IS-AS-800LF-930K-1C-UNV-xC48,Asymmetric Optic,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-930K-1C-UNV-xC96,FSM1IS-AS-800LF-930K-1C-UNV-xC96,Asymmetric Optic,800,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-930K-1C-347-xC24,FSM1IS-AS-800LF-930K-1C-347-xC24,Asymmetric Optic,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-930K-1C-347-xC48,FSM1IS-AS-800LF-930K-1C-347-xC48,Asymmetric Optic,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-930K-1C-347-xC96,FSM1IS-AS-800LF-930K-1C-347-xC96,Asymmetric Optic,800,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-35K-1C-UNV-xC24,FSM1IS-AS-800LF-35K-1C-UNV-xC24,Asymmetric Optic,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-35K-1C-UNV-xC48,FSM1IS-AS-800LF-35K-1C-UNV-xC48,Asymmetric Optic,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-35K-1C-UNV-xC96,FSM1IS-AS-800LF-35K-1C-UNV-xC96,Asymmetric Optic,800,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-35K-1C-347-xC24,FSM1IS-AS-800LF-35K-1C-347-xC24,Asymmetric Optic,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-35K-1C-347-xC48,FSM1IS-AS-800LF-35K-1C-347-xC48,Asymmetric Optic,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-35K-1C-347-xC96,FSM1IS-AS-800LF-35K-1C-347-xC96,Asymmetric Optic,800,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-935K-1C-UNV-xC24,FSM1IS-AS-800LF-935K-1C-UNV-xC24,Asymmetric Optic,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-935K-1C-UNV-xC48,FSM1IS-AS-800LF-935K-1C-UNV-xC48,Asymmetric Optic,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-935K-1C-UNV-xC96,FSM1IS-AS-800LF-935K-1C-UNV-xC96,Asymmetric Optic,800,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-935K-1C-347-xC24,FSM1IS-AS-800LF-935K-1C-347-xC24,Asymmetric Optic,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-935K-1C-347-xC48,FSM1IS-AS-800LF-935K-1C-347-xC48,Asymmetric Optic,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-935K-1C-347-xC96,FSM1IS-AS-800LF-935K-1C-347-xC96,Asymmetric Optic,800,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-40K-1C-UNV-xC24,FSM1IS-AS-800LF-40K-1C-UNV-xC24,Asymmetric Optic,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-40K-1C-UNV-xC48,FSM1IS-AS-800LF-40K-1C-UNV-xC48,Asymmetric Optic,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-40K-1C-UNV-xC96,FSM1IS-AS-800LF-40K-1C-UNV-xC96,Asymmetric Optic,800,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-40K-1C-347-xC24,FSM1IS-AS-800LF-40K-1C-347-xC24,Asymmetric Optic,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-40K-1C-347-xC48,FSM1IS-AS-800LF-40K-1C-347-xC48,Asymmetric Optic,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-40K-1C-347-xC96,FSM1IS-AS-800LF-40K-1C-347-xC96,Asymmetric Optic,800,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-940K-1C-UNV-xC24,FSM1IS-AS-800LF-940K-1C-UNV-xC24,Asymmetric Optic,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-940K-1C-UNV-xC48,FSM1IS-AS-800LF-940K-1C-UNV-xC48,Asymmetric Optic,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-940K-1C-UNV-xC96,FSM1IS-AS-800LF-940K-1C-UNV-xC96,Asymmetric Optic,800,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-800LF-940K-1C-347-xC24,FSM1IS-AS-800LF-940K-1C-347-xC24,Asymmetric Optic,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-800LF-940K-1C-347-xC48,FSM1IS-AS-800LF-940K-1C-347-xC48,Asymmetric Optic,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-800LF-940K-1C-347-xC96,FSM1IS-AS-800LF-940K-1C-347-xC96,Asymmetric Optic,800,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,25,25W,132,800 Lumens per foot,FSM1IS-AS-800UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-27K-1C-UNV-xC24,FSM1IS-AS-1000LF-27K-1C-UNV-xC24,Asymmetric Optic,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-27K-1C-UNV-xC48,FSM1IS-AS-1000LF-27K-1C-UNV-xC48,Asymmetric Optic,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-27K-1C-UNV-xC96,FSM1IS-AS-1000LF-27K-1C-UNV-xC96,Asymmetric Optic,1000,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-27K-1C-347-xC24,FSM1IS-AS-1000LF-27K-1C-347-xC24,Asymmetric Optic,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-27K-1C-347-xC48,FSM1IS-AS-1000LF-27K-1C-347-xC48,Asymmetric Optic,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-27K-1C-347-xC96,FSM1IS-AS-1000LF-27K-1C-347-xC96,Asymmetric Optic,1000,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-927K-1C-UNV-xC24,FSM1IS-AS-1000LF-927K-1C-UNV-xC24,Asymmetric Optic,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-927K-1C-UNV-xC48,FSM1IS-AS-1000LF-927K-1C-UNV-xC48,Asymmetric Optic,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-927K-1C-UNV-xC96,FSM1IS-AS-1000LF-927K-1C-UNV-xC96,Asymmetric Optic,1000,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-927K-1C-347-xC24,FSM1IS-AS-1000LF-927K-1C-347-xC24,Asymmetric Optic,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-927K-1C-347-xC48,FSM1IS-AS-1000LF-927K-1C-347-xC48,Asymmetric Optic,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-927K-1C-347-xC96,FSM1IS-AS-1000LF-927K-1C-347-xC96,Asymmetric Optic,1000,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-30K-1C-UNV-xC24,FSM1IS-AS-1000LF-30K-1C-UNV-xC24,Asymmetric Optic,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-30K-1C-UNV-xC48,FSM1IS-AS-1000LF-30K-1C-UNV-xC48,Asymmetric Optic,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-30K-1C-UNV-xC96,FSM1IS-AS-1000LF-30K-1C-UNV-xC96,Asymmetric Optic,1000,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-30K-1C-347-xC24,FSM1IS-AS-1000LF-30K-1C-347-xC24,Asymmetric Optic,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-30K-1C-347-xC48,FSM1IS-AS-1000LF-30K-1C-347-xC48,Asymmetric Optic,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-30K-1C-347-xC96,FSM1IS-AS-1000LF-30K-1C-347-xC96,Asymmetric Optic,1000,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-930K-1C-UNV-xC24,FSM1IS-AS-1000LF-930K-1C-UNV-xC24,Asymmetric Optic,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-930K-1C-UNV-xC48,FSM1IS-AS-1000LF-930K-1C-UNV-xC48,Asymmetric Optic,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-930K-1C-UNV-xC96,FSM1IS-AS-1000LF-930K-1C-UNV-xC96,Asymmetric Optic,1000,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-930K-1C-347-xC24,FSM1IS-AS-1000LF-930K-1C-347-xC24,Asymmetric Optic,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-930K-1C-347-xC48,FSM1IS-AS-1000LF-930K-1C-347-xC48,Asymmetric Optic,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-930K-1C-347-xC96,FSM1IS-AS-1000LF-930K-1C-347-xC96,Asymmetric Optic,1000,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-35K-1C-UNV-xC24,FSM1IS-AS-1000LF-35K-1C-UNV-xC24,Asymmetric Optic,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-35K-1C-UNV-xC48,FSM1IS-AS-1000LF-35K-1C-UNV-xC48,Asymmetric Optic,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-35K-1C-UNV-xC96,FSM1IS-AS-1000LF-35K-1C-UNV-xC96,Asymmetric Optic,1000,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-35K-1C-347-xC24,FSM1IS-AS-1000LF-35K-1C-347-xC24,Asymmetric Optic,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-35K-1C-347-xC48,FSM1IS-AS-1000LF-35K-1C-347-xC48,Asymmetric Optic,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-35K-1C-347-xC96,FSM1IS-AS-1000LF-35K-1C-347-xC96,Asymmetric Optic,1000,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-935K-1C-UNV-xC24,FSM1IS-AS-1000LF-935K-1C-UNV-xC24,Asymmetric Optic,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-935K-1C-UNV-xC48,FSM1IS-AS-1000LF-935K-1C-UNV-xC48,Asymmetric Optic,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-935K-1C-UNV-xC96,FSM1IS-AS-1000LF-935K-1C-UNV-xC96,Asymmetric Optic,1000,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-935K-1C-347-xC24,FSM1IS-AS-1000LF-935K-1C-347-xC24,Asymmetric Optic,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-935K-1C-347-xC48,FSM1IS-AS-1000LF-935K-1C-347-xC48,Asymmetric Optic,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-935K-1C-347-xC96,FSM1IS-AS-1000LF-935K-1C-347-xC96,Asymmetric Optic,1000,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-40K-1C-UNV-xC24,FSM1IS-AS-1000LF-40K-1C-UNV-xC24,Asymmetric Optic,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-40K-1C-UNV-xC48,FSM1IS-AS-1000LF-40K-1C-UNV-xC48,Asymmetric Optic,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-40K-1C-UNV-xC96,FSM1IS-AS-1000LF-40K-1C-UNV-xC96,Asymmetric Optic,1000,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-40K-1C-347-xC24,FSM1IS-AS-1000LF-40K-1C-347-xC24,Asymmetric Optic,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-40K-1C-347-xC48,FSM1IS-AS-1000LF-40K-1C-347-xC48,Asymmetric Optic,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-40K-1C-347-xC96,FSM1IS-AS-1000LF-40K-1C-347-xC96,Asymmetric Optic,1000,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-940K-1C-UNV-xC24,FSM1IS-AS-1000LF-940K-1C-UNV-xC24,Asymmetric Optic,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-940K-1C-UNV-xC48,FSM1IS-AS-1000LF-940K-1C-UNV-xC48,Asymmetric Optic,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-940K-1C-UNV-xC96,FSM1IS-AS-1000LF-940K-1C-UNV-xC96,Asymmetric Optic,1000,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1000LF-940K-1C-347-xC24,FSM1IS-AS-1000LF-940K-1C-347-xC24,Asymmetric Optic,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1000LF-940K-1C-347-xC48,FSM1IS-AS-1000LF-940K-1C-347-xC48,Asymmetric Optic,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1000LF-940K-1C-347-xC96,FSM1IS-AS-1000LF-940K-1C-347-xC96,Asymmetric Optic,1000,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,31,31W,131,1000 Lumens per foot. Not available with DALI.,FSM1IS-AS-1000UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-27K-1C-UNV-xC24,FSM1IS-AS-1250LF-27K-1C-UNV-xC24,Asymmetric Optic,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-27K-1C-UNV-xC48,FSM1IS-AS-1250LF-27K-1C-UNV-xC48,Asymmetric Optic,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-27K-1C-UNV-xC96,FSM1IS-AS-1250LF-27K-1C-UNV-xC96,Asymmetric Optic,1250,2700,"2700K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-27K-1C-347-xC24,FSM1IS-AS-1250LF-27K-1C-347-xC24,Asymmetric Optic,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-27K-1C-347-xC48,FSM1IS-AS-1250LF-27K-1C-347-xC48,Asymmetric Optic,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-27K-1C-347-xC96,FSM1IS-AS-1250LF-27K-1C-347-xC96,Asymmetric Optic,1250,2700,"2700K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-927K-1C-UNV-xC24,FSM1IS-AS-1250LF-927K-1C-UNV-xC24,Asymmetric Optic,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-927K-1C-UNV-xC48,FSM1IS-AS-1250LF-927K-1C-UNV-xC48,Asymmetric Optic,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-927K-1C-UNV-xC96,FSM1IS-AS-1250LF-927K-1C-UNV-xC96,Asymmetric Optic,1250,2700,"2700K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-927K-1C-347-xC24,FSM1IS-AS-1250LF-927K-1C-347-xC24,Asymmetric Optic,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-927K-1C-347-xC48,FSM1IS-AS-1250LF-927K-1C-347-xC48,Asymmetric Optic,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-927K-1C-347-xC96,FSM1IS-AS-1250LF-927K-1C-347-xC96,Asymmetric Optic,1250,2700,"2700K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-30K-1C-UNV-xC24,FSM1IS-AS-1250LF-30K-1C-UNV-xC24,Asymmetric Optic,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-30K-1C-UNV-xC48,FSM1IS-AS-1250LF-30K-1C-UNV-xC48,Asymmetric Optic,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-30K-1C-UNV-xC96,FSM1IS-AS-1250LF-30K-1C-UNV-xC96,Asymmetric Optic,1250,3000,"3000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-30K-1C-347-xC24,FSM1IS-AS-1250LF-30K-1C-347-xC24,Asymmetric Optic,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-30K-1C-347-xC48,FSM1IS-AS-1250LF-30K-1C-347-xC48,Asymmetric Optic,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-30K-1C-347-xC96,FSM1IS-AS-1250LF-30K-1C-347-xC96,Asymmetric Optic,1250,3000,"3000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-930K-1C-UNV-xC24,FSM1IS-AS-1250LF-930K-1C-UNV-xC24,Asymmetric Optic,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-930K-1C-UNV-xC48,FSM1IS-AS-1250LF-930K-1C-UNV-xC48,Asymmetric Optic,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-930K-1C-UNV-xC96,FSM1IS-AS-1250LF-930K-1C-UNV-xC96,Asymmetric Optic,1250,3000,"3000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-930K-1C-347-xC24,FSM1IS-AS-1250LF-930K-1C-347-xC24,Asymmetric Optic,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-930K-1C-347-xC48,FSM1IS-AS-1250LF-930K-1C-347-xC48,Asymmetric Optic,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-930K-1C-347-xC96,FSM1IS-AS-1250LF-930K-1C-347-xC96,Asymmetric Optic,1250,3000,"3000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-35K-1C-UNV-xC24,FSM1IS-AS-1250LF-35K-1C-UNV-xC24,Asymmetric Optic,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-35K-1C-UNV-xC48,FSM1IS-AS-1250LF-35K-1C-UNV-xC48,Asymmetric Optic,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-35K-1C-UNV-xC96,FSM1IS-AS-1250LF-35K-1C-UNV-xC96,Asymmetric Optic,1250,3500,"3500K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-35K-1C-347-xC24,FSM1IS-AS-1250LF-35K-1C-347-xC24,Asymmetric Optic,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-35K-1C-347-xC48,FSM1IS-AS-1250LF-35K-1C-347-xC48,Asymmetric Optic,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-35K-1C-347-xC96,FSM1IS-AS-1250LF-35K-1C-347-xC96,Asymmetric Optic,1250,3500,"3500K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-935K-1C-UNV-xC24,FSM1IS-AS-1250LF-935K-1C-UNV-xC24,Asymmetric Optic,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-935K-1C-UNV-xC48,FSM1IS-AS-1250LF-935K-1C-UNV-xC48,Asymmetric Optic,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-935K-1C-UNV-xC96,FSM1IS-AS-1250LF-935K-1C-UNV-xC96,Asymmetric Optic,1250,3500,"3500K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-935K-1C-347-xC24,FSM1IS-AS-1250LF-935K-1C-347-xC24,Asymmetric Optic,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-935K-1C-347-xC48,FSM1IS-AS-1250LF-935K-1C-347-xC48,Asymmetric Optic,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-935K-1C-347-xC96,FSM1IS-AS-1250LF-935K-1C-347-xC96,Asymmetric Optic,1250,3500,"3500K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-40K-1C-UNV-xC24,FSM1IS-AS-1250LF-40K-1C-UNV-xC24,Asymmetric Optic,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-40K-1C-UNV-xC48,FSM1IS-AS-1250LF-40K-1C-UNV-xC48,Asymmetric Optic,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-40K-1C-UNV-xC96,FSM1IS-AS-1250LF-40K-1C-UNV-xC96,Asymmetric Optic,1250,4000,"4000K, 80+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-40K-1C-347-xC24,FSM1IS-AS-1250LF-40K-1C-347-xC24,Asymmetric Optic,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-40K-1C-347-xC48,FSM1IS-AS-1250LF-40K-1C-347-xC48,Asymmetric Optic,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-40K-1C-347-xC96,FSM1IS-AS-1250LF-40K-1C-347-xC96,Asymmetric Optic,1250,4000,"4000K, 80+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-940K-1C-UNV-xC24,FSM1IS-AS-1250LF-940K-1C-UNV-xC24,Asymmetric Optic,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-940K-1C-UNV-xC48,FSM1IS-AS-1250LF-940K-1C-UNV-xC48,Asymmetric Optic,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-940K-1C-UNV-xC96,FSM1IS-AS-1250LF-940K-1C-UNV-xC96,Asymmetric Optic,1250,4000,"4000K, 90+ CRI",120,120/277 UNV Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
FSM1IS-AS-1250LF-940K-1C-347-xC24,FSM1IS-AS-1250LF-940K-1C-347-xC24,Asymmetric Optic,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,24,"24"" Cable Suspension"
FSM1IS-AS-1250LF-940K-1C-347-xC48,FSM1IS-AS-1250LF-940K-1C-347-xC48,Asymmetric Optic,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,48,"48"" Cable Suspension"
FSM1IS-AS-1250LF-940K-1C-347-xC96,FSM1IS-AS-1250LF-940K-1C-347-xC96,Asymmetric Optic,1250,4000,"4000K, 90+ CRI",347,347 Volt,N/A,Please Contact Manufacturer for Driver Information,Single Circuit,40,40W,128,1250 Lumens per foot. Not available with DALI.,FSM1IS-AS-1250UP-35K-4FT.ies,96,"96"" Cable Suspension"
