,Model##OTHER##,Shielding Type##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Color Temperature Note##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Driver##Other##,Circuit##OTHER##,Mounting##Other##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Photometric Web File##OTHER##,Driver Comment##OTHER##,Voltage Comment##OTHER##,Lumen Output Comment##OTHER##,Pop Down Lens##OTHER##
FSM1WAS125LF30K1CUNVxWM,FSM1WAS125LF30K1CUNVxWM,Asymmetric Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF30K1C347xWM,FSM1WAS125LF30K1C347xWM,Asymmetric Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF30K1CLVxWM,FSM1WAS125LF30K1CLVxWM,Asymmetric Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS250LF30K1CUNVxWM,FSM1WAS250LF30K1CUNVxWM,Asymmetric Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF30K1C347xWM,FSM1WAS250LF30K1C347xWM,Asymmetric Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF30K1CLVxWM,FSM1WAS250LF30K1CLVxWM,Asymmetric Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS375LF30K1CUNVxWM,FSM1WAS375LF30K1CUNVxWM,Asymmetric Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF30K1C347xWM,FSM1WAS375LF30K1C347xWM,Asymmetric Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF30K1CLVxWM,FSM1WAS375LF30K1CLVxWM,Asymmetric Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS500LF30K1CUNVxWM,FSM1WAS500LF30K1CUNVxWM,Asymmetric Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF30K1C347xWM,FSM1WAS500LF30K1C347xWM,Asymmetric Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF30K1CLVxWM,FSM1WAS500LF30K1CLVxWM,Asymmetric Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS625LF30K1CUNVxWM,FSM1WAS625LF30K1CUNVxWM,Asymmetric Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF30K1C347xWM,FSM1WAS625LF30K1C347xWM,Asymmetric Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF30K1CLVxWM,FSM1WAS625LF30K1CLVxWM,Asymmetric Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL125LF30K1CUNVxWM,FSM1WFL125LF30K1CUNVxWM,Flush Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF30K1C347xWM,FSM1WFL125LF30K1C347xWM,Flush Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF30K1CLVxWM,FSM1WFL125LF30K1CLVxWM,Flush Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL250LF30K1CUNVxWM,FSM1WFL250LF30K1CUNVxWM,Flush Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF30K1C347xWM,FSM1WFL250LF30K1C347xWM,Flush Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF30K1CLVxWM,FSM1WFL250LF30K1CLVxWM,Flush Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL375LF30K1CUNVxWM,FSM1WFL375LF30K1CUNVxWM,Flush Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF30K1C347xWM,FSM1WFL375LF30K1C347xWM,Flush Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF30K1CLVxWM,FSM1WFL375LF30K1CLVxWM,Flush Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL500LF30K1CUNVxWM,FSM1WFL500LF30K1CUNVxWM,Flush Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF30K1C347xWM,FSM1WFL500LF30K1C347xWM,Flush Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF30K1CLVxWM,FSM1WFL500LF30K1CLVxWM,Flush Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL625LF30K1CUNVxWM,FSM1WFL625LF30K1CUNVxWM,Flush Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF30K1C347xWM,FSM1WFL625LF30K1C347xWM,Flush Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF30K1CLVxWM,FSM1WFL625LF30K1CLVxWM,Flush Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WPD05125LF30K1CUNVxWM,FSM1WPD05125LF30K1CUNVxWM,Pop-Down Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF30K1C347xWM,FSM1WPD05125LF30K1C347xWM,Pop-Down Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF30K1CLVxWM,FSM1WPD05125LF30K1CLVxWM,Pop-Down Lens,125,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05250LF30K1CUNVxWM,FSM1WPD05250LF30K1CUNVxWM,Pop-Down Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF30K1C347xWM,FSM1WPD05250LF30K1C347xWM,Pop-Down Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF30K1CLVxWM,FSM1WPD05250LF30K1CLVxWM,Pop-Down Lens,250,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05375LF30K1CUNVxWM,FSM1WPD05375LF30K1CUNVxWM,Pop-Down Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF30K1C347xWM,FSM1WPD05375LF30K1C347xWM,Pop-Down Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF30K1CLVxWM,FSM1WPD05375LF30K1CLVxWM,Pop-Down Lens,375,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05500LF30K1CUNVxWM,FSM1WPD05500LF30K1CUNVxWM,Pop-Down Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF30K1C347xWM,FSM1WPD05500LF30K1C347xWM,Pop-Down Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF30K1CLVxWM,FSM1WPD05500LF30K1CLVxWM,Pop-Down Lens,500,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05625LF30K1CUNVxWM,FSM1WPD05625LF30K1CUNVxWM,Pop-Down Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF30K1C347xWM,FSM1WPD05625LF30K1C347xWM,Pop-Down Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF30K1CLVxWM,FSM1WPD05625LF30K1CLVxWM,Pop-Down Lens,625,3000,"3000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,1
FSM1WAS125LF930K1CUNVxWM,FSM1WAS125LF930K1CUNVxWM,Asymmetric Lens,125,3000,"3000K, 90+ CRI",347,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF930K1C347xWM,FSM1WAS125LF930K1C347xWM,Asymmetric Lens,125,3000,"3000K, 90+ CRI",347,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF930K1CLVxWM,FSM1WAS125LF930K1CLVxWM,Asymmetric Lens,125,3000,"3000K, 90+ CRI",347,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS250LF930K1CUNVxWM,FSM1WAS250LF930K1CUNVxWM,Asymmetric Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF930K1C347xWM,FSM1WAS250LF930K1C347xWM,Asymmetric Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF930K1CLVxWM,FSM1WAS250LF930K1CLVxWM,Asymmetric Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS375LF930K1CUNVxWM,FSM1WAS375LF930K1CUNVxWM,Asymmetric Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF930K1C347xWM,FSM1WAS375LF930K1C347xWM,Asymmetric Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF930K1CLVxWM,FSM1WAS375LF930K1CLVxWM,Asymmetric Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS500LF930K1CUNVxWM,FSM1WAS500LF930K1CUNVxWM,Asymmetric Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF930K1C347xWM,FSM1WAS500LF930K1C347xWM,Asymmetric Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF930K1CLVxWM,FSM1WAS500LF930K1CLVxWM,Asymmetric Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS625LF930K1CUNVxWM,FSM1WAS625LF930K1CUNVxWM,Asymmetric Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF930K1C347xWM,FSM1WAS625LF930K1C347xWM,Asymmetric Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF930K1CLVxWM,FSM1WAS625LF930K1CLVxWM,Asymmetric Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL125LF930K1CUNVxWM,FSM1WFL125LF930K1CUNVxWM,Flush Lens,125,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF930K1C347xWM,FSM1WFL125LF930K1C347xWM,Flush Lens,125,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF930K1CLVxWM,FSM1WFL125LF930K1CLVxWM,Flush Lens,125,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL250LF930K1CUNVxWM,FSM1WFL250LF930K1CUNVxWM,Flush Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF930K1C347xWM,FSM1WFL250LF930K1C347xWM,Flush Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF930K1CLVxWM,FSM1WFL250LF930K1CLVxWM,Flush Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL375LF930K1CUNVxWM,FSM1WFL375LF930K1CUNVxWM,Flush Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF930K1C347xWM,FSM1WFL375LF930K1C347xWM,Flush Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF930K1CLVxWM,FSM1WFL375LF930K1CLVxWM,Flush Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL500LF930K1CUNVxWM,FSM1WFL500LF930K1CUNVxWM,Flush Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF930K1C347xWM,FSM1WFL500LF930K1C347xWM,Flush Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF930K1CLVxWM,FSM1WFL500LF930K1CLVxWM,Flush Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL625LF930K1CUNVxWM,FSM1WFL625LF930K1CUNVxWM,Flush Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF930K1C347xWM,FSM1WFL625LF930K1C347xWM,Flush Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF930K1CLVxWM,FSM1WFL625LF930K1CLVxWM,Flush Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WPD05125LF930K1CUNVxWM,FSM1WPD05125LF930K1CUNVxWM,Pop-Down Lens,125,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF930K1C347xWM,FSM1WPD05125LF930K1C347xWM,Pop-Down Lens,125,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF930K1CLVxWM,FSM1WPD05125LF930K1CLVxWM,Pop-Down Lens,125,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05250LF930K1CUNVxWM,FSM1WPD05250LF930K1CUNVxWM,Pop-Down Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF930K1C347xWM,FSM1WPD05250LF930K1C347xWM,Pop-Down Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF930K1CLVxWM,FSM1WPD05250LF930K1CLVxWM,Pop-Down Lens,250,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05375LF930K1CUNVxWM,FSM1WPD05375LF930K1CUNVxWM,Pop-Down Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF930K1C347xWM,FSM1WPD05375LF930K1C347xWM,Pop-Down Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF930K1CLVxWM,FSM1WPD05375LF930K1CLVxWM,Pop-Down Lens,375,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05500LF930K1CUNVxWM,FSM1WPD05500LF930K1CUNVxWM,Pop-Down Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF930K1C347xWM,FSM1WPD05500LF930K1C347xWM,Pop-Down Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF930K1CLVxWM,FSM1WPD05500LF930K1CLVxWM,Pop-Down Lens,500,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05625LF930K1CUNVxWM,FSM1WPD05625LF930K1CUNVxWM,Pop-Down Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF930K1C347xWM,FSM1WPD05625LF930K1C347xWM,Pop-Down Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF930K1CLVxWM,FSM1WPD05625LF930K1CLVxWM,Pop-Down Lens,625,3000,"3000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,1
FSM1WAS125LF35K1CUNVxWM,FSM1WAS125LF35K1CUNVxWM,Asymmetric Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF35K1C347xWM,FSM1WAS125LF35K1C347xWM,Asymmetric Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF35K1CLVxWM,FSM1WAS125LF35K1CLVxWM,Asymmetric Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS250LF35K1CUNVxWM,FSM1WAS250LF35K1CUNVxWM,Asymmetric Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF35K1C347xWM,FSM1WAS250LF35K1C347xWM,Asymmetric Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF35K1CLVxWM,FSM1WAS250LF35K1CLVxWM,Asymmetric Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS375LF35K1CUNVxWM,FSM1WAS375LF35K1CUNVxWM,Asymmetric Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF35K1C347xWM,FSM1WAS375LF35K1C347xWM,Asymmetric Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF35K1CLVxWM,FSM1WAS375LF35K1CLVxWM,Asymmetric Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS500LF35K1CUNVxWM,FSM1WAS500LF35K1CUNVxWM,Asymmetric Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF35K1C347xWM,FSM1WAS500LF35K1C347xWM,Asymmetric Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF35K1CLVxWM,FSM1WAS500LF35K1CLVxWM,Asymmetric Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS625LF35K1CUNVxWM,FSM1WAS625LF35K1CUNVxWM,Asymmetric Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF35K1C347xWM,FSM1WAS625LF35K1C347xWM,Asymmetric Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF35K1CLVxWM,FSM1WAS625LF35K1CLVxWM,Asymmetric Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL125LF35K1CUNVxWM,FSM1WFL125LF35K1CUNVxWM,Flush Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF35K1C347xWM,FSM1WFL125LF35K1C347xWM,Flush Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF35K1CLVxWM,FSM1WFL125LF35K1CLVxWM,Flush Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL250LF35K1CUNVxWM,FSM1WFL250LF35K1CUNVxWM,Flush Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF35K1C347xWM,FSM1WFL250LF35K1C347xWM,Flush Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF35K1CLVxWM,FSM1WFL250LF35K1CLVxWM,Flush Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL375LF35K1CUNVxWM,FSM1WFL375LF35K1CUNVxWM,Flush Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF35K1C347xWM,FSM1WFL375LF35K1C347xWM,Flush Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF35K1CLVxWM,FSM1WFL375LF35K1CLVxWM,Flush Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL500LF35K1CUNVxWM,FSM1WFL500LF35K1CUNVxWM,Flush Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF35K1C347xWM,FSM1WFL500LF35K1C347xWM,Flush Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF35K1CLVxWM,FSM1WFL500LF35K1CLVxWM,Flush Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL625LF35K1CUNVxWM,FSM1WFL625LF35K1CUNVxWM,Flush Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF35K1C347xWM,FSM1WFL625LF35K1C347xWM,Flush Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF35K1CLVxWM,FSM1WFL625LF35K1CLVxWM,Flush Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WPD05125LF35K1CUNVxWM,FSM1WPD05125LF35K1CUNVxWM,Pop-Down Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF35K1C347xWM,FSM1WPD05125LF35K1C347xWM,Pop-Down Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF35K1CLVxWM,FSM1WPD05125LF35K1CLVxWM,Pop-Down Lens,125,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05250LF35K1CUNVxWM,FSM1WPD05250LF35K1CUNVxWM,Pop-Down Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF35K1C347xWM,FSM1WPD05250LF35K1C347xWM,Pop-Down Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF35K1CLVxWM,FSM1WPD05250LF35K1CLVxWM,Pop-Down Lens,250,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05375LF35K1CUNVxWM,FSM1WPD05375LF35K1CUNVxWM,Pop-Down Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF35K1C347xWM,FSM1WPD05375LF35K1C347xWM,Pop-Down Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF35K1CLVxWM,FSM1WPD05375LF35K1CLVxWM,Pop-Down Lens,375,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05500LF35K1CUNVxWM,FSM1WPD05500LF35K1CUNVxWM,Pop-Down Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF35K1C347xWM,FSM1WPD05500LF35K1C347xWM,Pop-Down Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF35K1CLVxWM,FSM1WPD05500LF35K1CLVxWM,Pop-Down Lens,500,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05625LF35K1CUNVxWM,FSM1WPD05625LF35K1CUNVxWM,Pop-Down Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF35K1C347xWM,FSM1WPD05625LF35K1C347xWM,Pop-Down Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF35K1CLVxWM,FSM1WPD05625LF35K1CLVxWM,Pop-Down Lens,625,3500,"3500K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,1
FSM1WAS125LF935K1CUNVxWM,FSM1WAS125LF935K1CUNVxWM,Asymmetric Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF935K1C347xWM,FSM1WAS125LF935K1C347xWM,Asymmetric Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF935K1CLVxWM,FSM1WAS125LF935K1CLVxWM,Asymmetric Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS250LF935K1CUNVxWM,FSM1WAS250LF935K1CUNVxWM,Asymmetric Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF935K1C347xWM,FSM1WAS250LF935K1C347xWM,Asymmetric Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF935K1CLVxWM,FSM1WAS250LF935K1CLVxWM,Asymmetric Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS375LF935K1CUNVxWM,FSM1WAS375LF935K1CUNVxWM,Asymmetric Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF935K1C347xWM,FSM1WAS375LF935K1C347xWM,Asymmetric Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF935K1CLVxWM,FSM1WAS375LF935K1CLVxWM,Asymmetric Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS500LF935K1CUNVxWM,FSM1WAS500LF935K1CUNVxWM,Asymmetric Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF935K1C347xWM,FSM1WAS500LF935K1C347xWM,Asymmetric Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF935K1CLVxWM,FSM1WAS500LF935K1CLVxWM,Asymmetric Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS625LF935K1CUNVxWM,FSM1WAS625LF935K1CUNVxWM,Asymmetric Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF935K1C347xWM,FSM1WAS625LF935K1C347xWM,Asymmetric Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF935K1CLVxWM,FSM1WAS625LF935K1CLVxWM,Asymmetric Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL125LF935K1CUNVxWM,FSM1WFL125LF935K1CUNVxWM,Flush Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF935K1C347xWM,FSM1WFL125LF935K1C347xWM,Flush Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF935K1CLVxWM,FSM1WFL125LF935K1CLVxWM,Flush Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL250LF935K1CUNVxWM,FSM1WFL250LF935K1CUNVxWM,Flush Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF935K1C347xWM,FSM1WFL250LF935K1C347xWM,Flush Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF935K1CLVxWM,FSM1WFL250LF935K1CLVxWM,Flush Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL375LF935K1CUNVxWM,FSM1WFL375LF935K1CUNVxWM,Flush Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF935K1C347xWM,FSM1WFL375LF935K1C347xWM,Flush Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF935K1CLVxWM,FSM1WFL375LF935K1CLVxWM,Flush Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL500LF935K1CUNVxWM,FSM1WFL500LF935K1CUNVxWM,Flush Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF935K1C347xWM,FSM1WFL500LF935K1C347xWM,Flush Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF935K1CLVxWM,FSM1WFL500LF935K1CLVxWM,Flush Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL625LF935K1CUNVxWM,FSM1WFL625LF935K1CUNVxWM,Flush Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF935K1C347xWM,FSM1WFL625LF935K1C347xWM,Flush Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF935K1CLVxWM,FSM1WFL625LF935K1CLVxWM,Flush Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WPD05125LF935K1CUNVxWM,FSM1WPD05125LF935K1CUNVxWM,Pop-Down Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF935K1C347xWM,FSM1WPD05125LF935K1C347xWM,Pop-Down Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF935K1CLVxWM,FSM1WPD05125LF935K1CLVxWM,Pop-Down Lens,125,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05250LF935K1CUNVxWM,FSM1WPD05250LF935K1CUNVxWM,Pop-Down Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF935K1C347xWM,FSM1WPD05250LF935K1C347xWM,Pop-Down Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF935K1CLVxWM,FSM1WPD05250LF935K1CLVxWM,Pop-Down Lens,250,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05375LF935K1CUNVxWM,FSM1WPD05375LF935K1CUNVxWM,Pop-Down Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF935K1C347xWM,FSM1WPD05375LF935K1C347xWM,Pop-Down Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF935K1CLVxWM,FSM1WPD05375LF935K1CLVxWM,Pop-Down Lens,375,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05500LF935K1CUNVxWM,FSM1WPD05500LF935K1CUNVxWM,Pop-Down Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF935K1C347xWM,FSM1WPD05500LF935K1C347xWM,Pop-Down Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF935K1CLVxWM,FSM1WPD05500LF935K1CLVxWM,Pop-Down Lens,500,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05625LF935K1CUNVxWM,FSM1WPD05625LF935K1CUNVxWM,Pop-Down Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF935K1C347xWM,FSM1WPD05625LF935K1C347xWM,Pop-Down Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF935K1CLVxWM,FSM1WPD05625LF935K1CLVxWM,Pop-Down Lens,625,3500,"3500K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,1
FSM1WAS125LF40K1CUNVxWM,FSM1WAS125LF40K1CUNVxWM,Asymmetric Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF40K1C347xWM,FSM1WAS125LF40K1C347xWM,Asymmetric Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF40K1CLVxWM,FSM1WAS125LF40K1CLVxWM,Asymmetric Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS250LF40K1CUNVxWM,FSM1WAS250LF40K1CUNVxWM,Asymmetric Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF40K1C347xWM,FSM1WAS250LF40K1C347xWM,Asymmetric Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF40K1CLVxWM,FSM1WAS250LF40K1CLVxWM,Asymmetric Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS375LF40K1CUNVxWM,FSM1WAS375LF40K1CUNVxWM,Asymmetric Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF40K1C347xWM,FSM1WAS375LF40K1C347xWM,Asymmetric Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF40K1CLVxWM,FSM1WAS375LF40K1CLVxWM,Asymmetric Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS500LF40K1CUNVxWM,FSM1WAS500LF40K1CUNVxWM,Asymmetric Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF40K1C347xWM,FSM1WAS500LF40K1C347xWM,Asymmetric Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF40K1CLVxWM,FSM1WAS500LF40K1CLVxWM,Asymmetric Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS625LF40K1CUNVxWM,FSM1WAS625LF40K1CUNVxWM,Asymmetric Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF40K1C347xWM,FSM1WAS625LF40K1C347xWM,Asymmetric Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF40K1CLVxWM,FSM1WAS625LF40K1CLVxWM,Asymmetric Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL125LF40K1CUNVxWM,FSM1WFL125LF40K1CUNVxWM,Flush Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF40K1C347xWM,FSM1WFL125LF40K1C347xWM,Flush Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF40K1CLVxWM,FSM1WFL125LF40K1CLVxWM,Flush Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL250LF40K1CUNVxWM,FSM1WFL250LF40K1CUNVxWM,Flush Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF40K1C347xWM,FSM1WFL250LF40K1C347xWM,Flush Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF40K1CLVxWM,FSM1WFL250LF40K1CLVxWM,Flush Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL375LF40K1CUNVxWM,FSM1WFL375LF40K1CUNVxWM,Flush Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF40K1C347xWM,FSM1WFL375LF40K1C347xWM,Flush Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF40K1CLVxWM,FSM1WFL375LF40K1CLVxWM,Flush Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL500LF40K1CUNVxWM,FSM1WFL500LF40K1CUNVxWM,Flush Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF40K1C347xWM,FSM1WFL500LF40K1C347xWM,Flush Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF40K1CLVxWM,FSM1WFL500LF40K1CLVxWM,Flush Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL625LF40K1CUNVxWM,FSM1WFL625LF40K1CUNVxWM,Flush Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF40K1C347xWM,FSM1WFL625LF40K1C347xWM,Flush Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF40K1CLVxWM,FSM1WFL625LF40K1CLVxWM,Flush Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WPD05125LF40K1CUNVxWM,FSM1WPD05125LF40K1CUNVxWM,Pop-Down Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF40K1C347xWM,FSM1WPD05125LF40K1C347xWM,Pop-Down Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF40K1CLVxWM,FSM1WPD05125LF40K1CLVxWM,Pop-Down Lens,125,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05250LF40K1CUNVxWM,FSM1WPD05250LF40K1CUNVxWM,Pop-Down Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF40K1C347xWM,FSM1WPD05250LF40K1C347xWM,Pop-Down Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF40K1CLVxWM,FSM1WPD05250LF40K1CLVxWM,Pop-Down Lens,250,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05375LF40K1CUNVxWM,FSM1WPD05375LF40K1CUNVxWM,Pop-Down Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF40K1C347xWM,FSM1WPD05375LF40K1C347xWM,Pop-Down Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF40K1CLVxWM,FSM1WPD05375LF40K1CLVxWM,Pop-Down Lens,375,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05500LF40K1CUNVxWM,FSM1WPD05500LF40K1CUNVxWM,Pop-Down Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF40K1C347xWM,FSM1WPD05500LF40K1C347xWM,Pop-Down Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF40K1CLVxWM,FSM1WPD05500LF40K1CLVxWM,Pop-Down Lens,500,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05625LF40K1CUNVxWM,FSM1WPD05625LF40K1CUNVxWM,Pop-Down Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF40K1C347xWM,FSM1WPD05625LF40K1C347xWM,Pop-Down Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF40K1CLVxWM,FSM1WPD05625LF40K1CLVxWM,Pop-Down Lens,625,4000,"4000K, 80+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,1
FSM1WAS125LF940K1CUNVxWM,FSM1WAS125LF940K1CUNVxWM,Asymmetric Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF940K1C347xWM,FSM1WAS125LF940K1C347xWM,Asymmetric Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS125LF940K1CLVxWM,FSM1WAS125LF940K1CLVxWM,Asymmetric Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-AS-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WAS250LF940K1CUNVxWM,FSM1WAS250LF940K1CUNVxWM,Asymmetric Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF940K1C347xWM,FSM1WAS250LF940K1C347xWM,Asymmetric Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS250LF940K1CLVxWM,FSM1WAS250LF940K1CLVxWM,Asymmetric Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-AS-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WAS375LF940K1CUNVxWM,FSM1WAS375LF940K1CUNVxWM,Asymmetric Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF940K1C347xWM,FSM1WAS375LF940K1C347xWM,Asymmetric Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS375LF940K1CLVxWM,FSM1WAS375LF940K1CLVxWM,Asymmetric Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-AS-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WAS500LF940K1CUNVxWM,FSM1WAS500LF940K1CUNVxWM,Asymmetric Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF940K1C347xWM,FSM1WAS500LF940K1C347xWM,Asymmetric Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS500LF940K1CLVxWM,FSM1WAS500LF940K1CLVxWM,Asymmetric Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-AS-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WAS625LF940K1CUNVxWM,FSM1WAS625LF940K1CUNVxWM,Asymmetric Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF940K1C347xWM,FSM1WAS625LF940K1C347xWM,Asymmetric Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WAS625LF940K1CLVxWM,FSM1WAS625LF940K1CLVxWM,Asymmetric Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-AS-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL125LF940K1CUNVxWM,FSM1WFL125LF940K1CUNVxWM,Flush Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF940K1C347xWM,FSM1WFL125LF940K1C347xWM,Flush Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL125LF940K1CLVxWM,FSM1WFL125LF940K1CLVxWM,Flush Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-FL-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,0
FSM1WFL250LF940K1CUNVxWM,FSM1WFL250LF940K1CUNVxWM,Flush Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF940K1C347xWM,FSM1WFL250LF940K1C347xWM,Flush Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL250LF940K1CLVxWM,FSM1WFL250LF940K1CLVxWM,Flush Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-FL-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,0
FSM1WFL375LF940K1CUNVxWM,FSM1WFL375LF940K1CUNVxWM,Flush Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF940K1C347xWM,FSM1WFL375LF940K1C347xWM,Flush Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL375LF940K1CLVxWM,FSM1WFL375LF940K1CLVxWM,Flush Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-FL-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,0
FSM1WFL500LF940K1CUNVxWM,FSM1WFL500LF940K1CUNVxWM,Flush Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF940K1C347xWM,FSM1WFL500LF940K1C347xWM,Flush Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL500LF940K1CLVxWM,FSM1WFL500LF940K1CLVxWM,Flush Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-FL-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,0
FSM1WFL625LF940K1CUNVxWM,FSM1WFL625LF940K1CUNVxWM,Flush Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF940K1C347xWM,FSM1WFL625LF940K1C347xWM,Flush Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,0
FSM1WFL625LF940K1CLVxWM,FSM1WFL625LF940K1CLVxWM,Flush Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-FL-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,0
FSM1WPD05125LF940K1CUNVxWM,FSM1WPD05125LF940K1CUNVxWM,Pop-Down Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF940K1C347xWM,FSM1WPD05125LF940K1C347xWM,Pop-Down Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05125LF940K1CLVxWM,FSM1WPD05125LF940K1CLVxWM,Pop-Down Lens,125,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,6,6W,FSM1W-PD05-125LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 125 Lumens per foot.,1
FSM1WPD05250LF940K1CUNVxWM,FSM1WPD05250LF940K1CUNVxWM,Pop-Down Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF940K1C347xWM,FSM1WPD05250LF940K1C347xWM,Pop-Down Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05250LF940K1CLVxWM,FSM1WPD05250LF940K1CLVxWM,Pop-Down Lens,250,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,10,10W,FSM1W-PD05-250LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 250 Lumens per foot.,1
FSM1WPD05375LF940K1CUNVxWM,FSM1WPD05375LF940K1CUNVxWM,Pop-Down Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF940K1C347xWM,FSM1WPD05375LF940K1C347xWM,Pop-Down Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05375LF940K1CLVxWM,FSM1WPD05375LF940K1CLVxWM,Pop-Down Lens,375,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,15,15W,FSM1W-PD05-375LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 375 Lumens per foot.,1
FSM1WPD05500LF940K1CUNVxWM,FSM1WPD05500LF940K1CUNVxWM,Pop-Down Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF940K1C347xWM,FSM1WPD05500LF940K1C347xWM,Pop-Down Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05500LF940K1CLVxWM,FSM1WPD05500LF940K1CLVxWM,Pop-Down Lens,500,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,19,19W,FSM1W-PD05-500LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 500 Lumens per foot.,1
FSM1WPD05625LF940K1CUNVxWM,FSM1WPD05625LF940K1CUNVxWM,Pop-Down Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,120/277 UNV Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF940K1C347xWM,FSM1WPD05625LF940K1C347xWM,Pop-Down Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,347 Volt,Direct Distribution - 625 Lumens per foot.,1
FSM1WPD05625LF940K1CLVxWM,FSM1WPD05625LF940K1CLVxWM,Pop-Down Lens,625,4000,"4000K, 90+ CRI",120,N/A,Single Circuit,Wall Mount,24,24W,FSM1W-PD05-625LF-35K-UNV-WH-4.ies,Please Contact Manufacturer for Driver Information,Low Voltage,Direct Distribution - 625 Lumens per foot.,1
