,Model##OTHER##,Shielding Type##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Lumen Output##OTHER##,Color Temperature Note##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Driver##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Photometric Web File##OTHER##,Mounting##OTHER##,TF Mount##OTHER##,FixtureOffset##Length##INCHES
TRSM4PR-FXH-SW-AF0-275LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-275LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-375LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-375LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-625LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-625LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-750LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-750LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-875LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-875LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1000LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1000LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1125LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1125LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-27K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-30K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-35K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-40K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-927K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-930K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-935K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-1250LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-AF0-1250LF-940K-1C-UNV-LD1-TF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-275LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-275LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-375LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-375LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-625LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-625LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-750LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-750LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-875LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-875LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1000LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1000LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1125LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1125LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-27K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-30K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-35K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-40K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-927K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-930K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-935K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-FL0-1250LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-FL0-1250LF-940K-1C-UNV-LD1-TF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-275LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-275LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-375LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-375LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-625LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-625LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-750LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-750LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-875LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-875LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1000LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1000LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1125LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1125LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-27K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-27K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-30K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-30K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-35K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-35K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-40K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-40K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-927K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-927K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-930K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-930K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-935K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-935K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-GR0-1250LF-940K-1C-UNV-LD1-TF-WH,TRSM4PR-FXH-SW-GR0-1250LF-940K-1C-UNV-LD1-TF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,
TRSM4PR-FXH-SW-AF0-275LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-275LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-275LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-275LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-275LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-275LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-275LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-275LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-275LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.7,9.7  Watts per foot,114,TRSM4PR-AF0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-375LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-375LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.7,12.7  Watts per foot,118,TRSM4PR-AF0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-625LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-625LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.6,20.6  Watts per foot,122,TRSM4PR-AF0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-750LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-750LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25.6,25.6  Watts per foot,117,TRSM4PR-AF0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-875LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-875LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,30.1,30.1  Watts per foot,116,TRSM4PR-AF0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1000LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1000LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,34.7,34.7  Watts per foot,115,TRSM4PR-AF0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1125LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1125LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4PR-AF0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-27K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-30K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-35K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-40K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-927K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-930K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-935K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-AF0-1250LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-AF0-1250LF-940K-1C-UNV-LD1-XF-WH,Flush Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4PR-AF0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-275LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-275LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,10.14,10.14  Watts per foot,108,TRSM4PR-FL0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-375LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-375LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,13.33,13.33  Watts per foot,113,TRSM4PR-FL0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-625LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-625LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,22.48,22.48  Watts per foot,111,TRSM4PR-FL0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-750LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-750LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,27.1,27.1  Watts per foot,111,TRSM4PR-FL0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-875LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-875LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,31.88,31.88  Watts per foot,110,TRSM4PR-FL0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1000LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1000LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,36.88,36.88  Watts per foot,108,TRSM4PR-FL0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1125LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1125LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4PR-FL0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-27K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-30K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-35K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-40K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-927K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-930K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-935K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-FL0-1250LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-FL0-1250LF-940K-1C-UNV-LD1-XF-WH,Flush Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4PR-FL0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-275LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-275LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.9,9.9  Watts per foot,111,TRSM4PR-GR0-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-375LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-375LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.4,12.4  Watts per foot,121,TRSM4PR-GR0-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-625LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-625LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.1,20.1  Watts per foot,124,TRSM4PR-GR0-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-750LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-750LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25,25  Watts per foot,120,TRSM4PR-GR0-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-875LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-875LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,29.4,29.4  Watts per foot,119,TRSM4PR-GR0-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1000LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1000LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,33.8,33.8  Watts per foot,118,TRSM4PR-GR0-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1125LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1125LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,38.5,38.5 Watts per foot,117,TRSM4PR-GR0-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-27K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-27K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-30K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-30K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-35K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-35K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-40K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-40K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-927K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-927K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-930K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-930K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-935K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-935K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
TRSM4PR-FXH-SW-GR0-1250LF-940K-1C-UNV-LD1-XF-WH,TRSM4PR-FXH-SW-GR0-1250LF-940K-1C-UNV-LD1-XF-WH,Flush Grazer,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,42.8,42.8 Watts per foot,117,TRSM4PR-GR0-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,
