,Model##OTHER##,Shielding Type##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Lumen Output##OTHER##,Color Temperature Note##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Driver##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Photometric Web File##OTHER##,Mounting##OTHER##,TF Mount##OTHER##,FixtureOffset##Length##INCHES
TRSM4L-SW-AS-275LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-275LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-275LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-275LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-275LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-275LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-275LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-275LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-375LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-375LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-375LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-375LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-375LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-375LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-375LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-375LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-625LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-625LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-625LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-625LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-625LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-625LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-625LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-625LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-750LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-750LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-750LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-750LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-750LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-750LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-750LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-750LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-875LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-875LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-875LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-875LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-875LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-875LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-875LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-875LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1000LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1000LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1000LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1000LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1000LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1000LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1000LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1000LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1125LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1125LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1125LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1125LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1125LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1125LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1125LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1125LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-1250LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AS-1250LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-27K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-30K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-35K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-40K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-927K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-930K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-935K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AF-1250LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-AF-1250LF-940K-1C-UNV-LD1-TF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-27K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-30K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-35K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-40K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-927K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-930K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-935K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-BW-1250LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-BW-1250LF-940K-1C-UNV-LD1-TF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-27K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-27K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-30K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-30K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-35K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-35K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-40K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-40K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-927K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-927K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-930K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-930K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-935K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-935K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-FL-1250LF-940K-1C-UNV-LD1-TF-WH,TRSM4L-SW-FL-1250LF-940K-1C-UNV-LD1-TF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Trim Flange Drywall,1,0.0166
TRSM4L-SW-AS-275LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-275LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-275LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-275LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-275LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-275LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-275LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-275LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-275LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,10,10 Watts per foot,110,TRSM4L-AS-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-275LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-275LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.7,9.7 Watts per foot,114,TRSM4L-AF-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-275LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-275LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,9.9,9.9 Watts per foot,112,TRSM4L-BW-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-275LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-275LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,275,Lumen Output - 275 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,10.14,10.14 Watts per foot,108,TRSM4L-FL-275LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-375LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-375LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.5,12.5 Watts per foot,120,TRSM4L-AS-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-375LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-375LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.7,12.7 Watts per foot,118,TRSM4L-AF-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-375LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-375LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,12.9,12.9 Watts per foot,116,TRSM4L-BW-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-375LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-375LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,375,Lumen Output - 375 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,13.33,13.33 Watts per foot,113,TRSM4L-FL-375LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-625LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-625LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.3,20.3 Watts per foot,123,TRSM4L-AS-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-625LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-625LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,20.6,20.6 Watts per foot,122,TRSM4L-AF-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-625LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-625LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,21.1,21.1 Watts per foot,119,TRSM4L-BW-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-625LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-625LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,625,Lumen Output - 625 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,22.48,22.48 Watts per foot,111,TRSM4L-FL-625LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-750LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-750LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25.3,25.3 Watts per foot,119,TRSM4L-AS-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-750LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-750LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,25.6,25.6 Watts per foot,117,TRSM4L-AF-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-750LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-750LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,26.2,26.2 Watts per foot,114,TRSM4L-BW-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-750LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-750LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,750,Lumen Output - 750 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,27.1,27.1 Watts per foot,111,TRSM4L-FL-750LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-875LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-875LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,29.7,29.7 Watts per foot,118,TRSM4L-AS-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-875LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-875LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,30.1,30.1 Watts per foot,116,TRSM4L-AF-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-875LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-875LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,30.9,30.9 Watts per foot,113,TRSM4L-BW-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-875LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-875LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,875,Lumen Output - 875 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,31.88,31.88 Watts per foot,110,TRSM4L-FL-875LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1000LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1000LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,34.3,34.3 Watts per foot,117,TRSM4L-AS-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1000LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1000LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,34.7,34.7 Watts per foot,115,TRSM4L-AF-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1000LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1000LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,35.6,35.6 Watts per foot,112,TRSM4L-BW-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1000LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1000LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1000,Lumen Output - 1000 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,36.88,36.88 Watts per foot,108,TRSM4L-FL-1000LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1125LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1125LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,38.9,38.9 Watts per foot,116,TRSM4L-AS-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1125LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1125LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,39.5,39.5 Watts per foot,114,TRSM4L-AF-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1125LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1125LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,40.6,40.6 Watts per foot,111,TRSM4L-BW-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1125LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1125LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1125,Lumen Output - 1125 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,41.97,41.97 Watts per foot,107,TRSM4L-FL-1125LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AS-1250LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AS-1250LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,43.2,43.2 Watts per foot,116,TRSM4L-AS-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-27K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-30K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-35K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-40K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-927K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-930K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-935K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-AF-1250LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-AF-1250LF-940K-1C-UNV-LD1-XF-WH,Asymmetric Room Fill Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,43.9,43.9 Watts per foot,114,TRSM4L-AF-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-27K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-30K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-35K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-40K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-927K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-930K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-935K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-BW-1250LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-BW-1250LF-940K-1C-UNV-LD1-XF-WH,Batwing Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,45.1,45.1 Watts per foot,111,TRSM4L-BW-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-27K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-27K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 80+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-30K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-30K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 80+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-35K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-35K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 80+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-40K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-40K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 80+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-927K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-927K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"2700K, 90+ CRI",2700,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-930K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-930K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3000K, 90+ CRI",3000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-935K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-935K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"3500K, 90+ CRI",3500,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
TRSM4L-SW-FL-1250LF-940K-1C-UNV-LD1-XF-WH,TRSM4L-SW-FL-1250LF-940K-1C-UNV-LD1-XF-WH,Flush Satin Lens,1250,Lumen Output - 1250 Lumens per foot,"4000K, 90+ CRI",4000,0-10V - 10% Dimming,46.75,46.75 Watts per foot,107,TRSM4L-FL-1250LF-35K-1C-UNV-WH-4FT.ies,Mud-in Trimless,0,0.137
